<table style="border-collapse: collapse; border: none;">
  <tr style="border-collapse: collapse; border: none;">
    <td style="border-collapse: collapse; border: none;">
      <a href="http://www.openairinterface.org/">
         <img src="../../../doc/images/oai_final_logo.png" alt="" border=3 height=50 width=150>
         </img>
      </a>
    </td>
    <td style="border-collapse: collapse; border: none; vertical-align: center;">
      <b><font size = "5">OAI Full Stack 5G-NR RF simulation with containers</font></b>
    </td>
  </tr>
</table>

This page is only valid for an `Ubuntu 22` host.

**NOTE: this version (2023-01-27) has been updated  for the `v1.5.0` version of the `OAI 5G CN`.**

**Table of Contents**

[[_TOC_]]

# 1. Retrieving the images on Docker-Hub #

Currently the images are hosted under the team account `oaisoftwarealliance`. They were previously hosted under the user account `rdefosseoai`.

Once again you may need to log on [docker-hub](https://hub.docker.com/) if your organization has reached pulling limit as `anonymous`.

```bash
$ docker login
Login with your Docker ID to push and pull images from Docker Hub. If you don't have a Docker ID, head over to https://hub.docker.com to create one.
Username:
Password:
```

Now pull images.

```bash
$ docker pull mysql:8.0
$ docker pull oaisoftwarealliance/oai-amf:v2.0.0
$ docker pull oaisoftwarealliance/oai-smf:v2.0.0
$ docker pull oaisoftwarealliance/oai-upf:v2.0.0
$ docker pull oaisoftwarealliance/trf-gen-cn5g:focal

$ docker pull oaisoftwarealliance/oai-gnb:develop
$ docker pull oaisoftwarealliance/oai-nr-ue:develop
```

```bash
$ docker logout
```

**CAUTION: 2023/01/27 with the release `v1.5.0` of the `CN5G`, the previous version was not compatible any-more.**

**This new version is working only with the `v2.0.0` of the `CN5G`.**

# 2. Deploy containers #

![Deployment](./oai-end-to-end.jpg)

**CAUTION: this SHALL be done in multiple steps.**

**Just `docker-compose up -d` WILL NOT WORK!**

All the following commands **SHALL** be run from the `ci-scripts/yaml_files/5g_rfsimulator` folder for a deployment with monolithic gNB.

For a deployment with the gNB split in CU and DU components, please refer to the `../5g_f1_rfsimulator` folder.
For a deployment with the gNB split in CU-CP, CU-UP, and DU components, please refer to the `../5g_rfsimulator_e1` folder.

## 2.1. Deploy OAI 5G Core Network ##

```bash
$ cd ci-scripts/yaml_files/5g_rfsimulator
$ docker-compose up -d mysql oai-amf oai-smf oai-upf oai-ext-dn
Creating network "rfsim5g-oai-public-net" with driver "bridge"
Creating network "rfsim5g-oai-traffic_net-net" with driver "bridge"
Creating rfsim5g-mysql      ... done
Creating rfsim5g-oai-upf   ... done
Creating rfsim5g-oai-amf   ... done
Creating rfsim5g-oai-smf   ... done
Creating rfsim5g-oai-ext-dn ... done
```

Wait for a bit.

```bash
$ docker-compose ps -a
       Name                     Command                  State                  Ports
-------------------------------------------------------------------------------------------------
rfsim5g-mysql        docker-entrypoint.sh mysqld      Up (healthy)   3306/tcp, 33060/tcp
rfsim5g-oai-amf      /bin/bash /openair-amf/bin ...   Up (healthy)   38412/sctp, 80/tcp, 9090/tcp
rfsim5g-oai-ext-dn   /bin/bash -c  apt update;  ...   Up (healthy)
rfsim5g-oai-smf      /bin/bash -c /openair-smf/ ...   Up (healthy)   80/tcp, 8805/udp, 9090/tcp
rfsim5g-oai-upf      /bin/bash -c /openair-upf/ ...   Up (healthy)   2152/udp, 8805/udp
```

At this point, you can prepare a capture on the newly-created public docker bridges:

```bash
$ ifconfig
...
rfsim5g-public: flags=4163<UP,BROADCAST,RUNNING,MULTICAST>  mtu 1500
        inet 192.168.71.129  netmask 255.255.255.192  broadcast 192.168.71.191
        inet6 fe80::42:c4ff:fe2b:3d38  prefixlen 64  scopeid 0x20<link>
        ether 02:42:c4:2b:3d:38  txqueuelen 0  (Ethernet)
        RX packets 4  bytes 112 (112.0 B)
        RX errors 0  dropped 0  overruns 0  frame 0
        TX packets 7  bytes 626 (626.0 B)
        TX errors 0  dropped 0 overruns 0  carrier 0  collisions 0

rfsim5g-traffic: flags=4163<UP,BROADCAST,RUNNING,MULTICAST>  mtu 1500
        inet 192.168.72.129  netmask 255.255.255.192  broadcast 192.168.72.191
        inet6 fe80::42:b5ff:fed3:e732  prefixlen 64  scopeid 0x20<link>
        ether 02:42:b5:d3:e7:32  txqueuelen 0  (Ethernet)
        RX packets 2652  bytes 142335 (142.3 KB)
        RX errors 0  dropped 0  overruns 0  frame 0
        TX packets 3999  bytes 23367972 (23.3 MB)
        TX errors 0  dropped 0 overruns 0  carrier 0  collisions 0
...
```

## 2.2. Deploy OAI gNB in RF simulator mode and in Standalone Mode ##

**CAUTION: To execute this 2nd step, the whole `CN5G` SHALL be in `healthy` state (especially the `mysql` container).**

The gNB can be deployed either in monolithic mode, or in CU/DU split mode.
- For a deployment with a monolithic gNB:

```bash
$ docker-compose up -d oai-gnb
rfsim5g-oai-upf is up-to-date
rfsim5g-oai-ext-dn is up-to-date
Creating rfsim5g-oai-gnb ... done
```
- For a deployment with the gNB split in CU and DU components:
```bash
#Deployment of the CU
$ docker-compose up -d oai-cu
```

```bash
#Deployment of the DU
$ docker-compose up -d oai-du
```
Wait for a bit.

```bash
$ docker-compose ps -a
       Name                     Command                  State                  Ports
-------------------------------------------------------------------------------------------------
rfsim5g-mysql        docker-entrypoint.sh mysqld      Up (healthy)   3306/tcp, 33060/tcp
rfsim5g-oai-amf      /bin/bash /openair-amf/bin ...   Up (healthy)   38412/sctp, 80/tcp, 9090/tcp
rfsim5g-oai-ext-dn   /bin/bash -c  apt update;  ...   Up (healthy)
rfsim5g-oai-gnb      /opt/oai-gnb/bin/entrypoin ...   Up (healthy)
rfsim5g-oai-smf      /bin/bash -c /openair-smf/ ...   Up (healthy)   80/tcp, 8805/udp, 9090/tcp
rfsim5g-oai-upf      /bin/bash -c /openair-upf/ ...   Up (healthy)   2152/udp, 8805/udp
```

You can verify that the `gNB` is connected with the `AMF`:

```bagh
$ docker logs rfsim5g-oai-amf
...
[AMF] [amf_app] [info ] |----------------------------------------------------gNBs' information-------------------------------------------|
[AMF] [amf_app] [info ] |    Index    |      Status      |       Global ID       |       gNB Name       |               PLMN             |
[AMF] [amf_app] [info ] |      1      |    Connected     |         0x0       |         gnb-rfsim        |            208, 99             |
[AMF] [amf_app] [info ] |----------------------------------------------------------------------------------------------------------------|
...
```

## 2.3. Deploy OAI NR-UE in RF simulator mode and in Standalone Mode ##

```bash
$ docker-compose up -d oai-nr-ue
rfsim5g-mysql is up-to-date
rfsim5g-oai-amf is up-to-date
rfsim5g-oai-smf is up-to-date
rfsim5g-oai-upf is up-to-date
rfsim5g-oai-ext-dn is up-to-date
rfsim5g-oai-gnb is up-to-date
Creating rfsim5g-oai-nr-ue ... done
```

Wait for a bit.

```bash
$ docker-compose ps -a
       Name                     Command                  State                  Ports
-------------------------------------------------------------------------------------------------
rfsim5g-mysql        docker-entrypoint.sh mysqld      Up (healthy)   3306/tcp, 33060/tcp
rfsim5g-oai-amf      /bin/bash /openair-amf/bin ...   Up (healthy)   38412/sctp, 80/tcp, 9090/tcp
rfsim5g-oai-ext-dn   /bin/bash -c  apt update;  ...   Up (healthy)
rfsim5g-oai-gnb      /opt/oai-gnb/bin/entrypoin ...   Up (healthy)
rfsim5g-oai-nr-ue    /opt/oai-nr-ue/bin/entrypo ...   Up (healthy)
rfsim5g-oai-smf      /bin/bash -c /openair-smf/ ...   Up (healthy)   80/tcp, 8805/udp, 9090/tcp
rfsim5g-oai-upf      /bin/bash -c /openair-upf/ ...   Up (healthy)   2152/udp, 8805/udp
```

Making sure the OAI UE is connected:

```bash
$ docker exec -it rfsim5g-oai-nr-ue /bin/bash
root@bb4d400a832d:/opt/oai-nr-ue# ifconfig
eth0: flags=4163<UP,BROADCAST,RUNNING,MULTICAST>  mtu 1500
        inet 192.168.71.150  netmask 255.255.255.192  broadcast 192.168.71.191
        ether 02:42:c0:a8:47:89  txqueuelen 0  (Ethernet)
        RX packets 224259  bytes 5821372018 (5.8 GB)
        RX errors 0  dropped 0  overruns 0  frame 0
        TX packets 235916  bytes 7848786376 (7.8 GB)
        TX errors 0  dropped 0 overruns 0  carrier 0  collisions 0

lo: flags=73<UP,LOOPBACK,RUNNING>  mtu 65536
        inet 127.0.0.1  netmask 255.0.0.0
        loop  txqueuelen 1000  (Local Loopback)
        RX packets 0  bytes 0 (0.0 B)
        RX errors 0  dropped 0  overruns 0  frame 0
        TX packets 0  bytes 0 (0.0 B)
        TX errors 0  dropped 0 overruns 0  carrier 0  collisions 0

oaitun_ue1: flags=4305<UP,POINTOPOINT,RUNNING,NOARP,MULTICAST>  mtu 1500
        inet 12.1.1.2  netmask 255.255.255.0  destination 12.1.1.2
        unspec 00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00  txqueuelen 500  (UNSPEC)
        RX packets 0  bytes 0 (0.0 B)
        RX errors 0  dropped 0  overruns 0  frame 0
        TX packets 0  bytes 0 (0.0 B)
        TX errors 0  dropped 0 overruns 0  carrier 0  collisions 0
```

## 2.4. Deploy Second OAI NR-UE in RF simulator mode and in Standalone Mode ##

Create a entry for new IMSI (208990100001101) in oai_db.sql file.
For this, refer to section [Making the NR-UE connect to the core
network](#51-making-the-nr-ue-connect-to-the-core-network)

Create the entry for the second UE in `docker-compose.yaml` file as follows:

```yaml
    oai-nr-ue2:
        image: oai-nr-ue:develop
        container_name: rfsim5g-oai-nr-ue2
        cap_drop:
            - ALL
        cap_add:
            - NET_ADMIN  # for interface bringup
            - NET_RAW    # for ping
        environment:
            USE_ADDITIONAL_OPTIONS: -E --rfsim -r 106 --numerology 1 -C 3619200000 --rfsimulator.serveraddr 192.168.71.140 --log_config.global_log_options level,nocolor,time
        depends_on:
            - oai-gnb
        devices:
             - /dev/net/tun:/dev/net/tun
        volumes:
            - ../../conf_files/nrue.uicc.conf:/opt/oai-nr-ue/etc/nr-ue.conf
        networks:
            public_net:
                ipv4_address: 192.168.71.151
        healthcheck:
            test: /bin/bash -c "pgrep nr-uesoftmodem"
            interval: 10s
            timeout: 5s
            retries: 5
```


```bash
$ docker-compose up -d oai-nr-ue2
rfsim5g-mysql is up-to-date
rfsim5g-oai-amf is up-to-date
rfsim5g-oai-smf is up-to-date
rfsim5g-oai-upf is up-to-date
rfsim5g-oai-ext-dn is up-to-date
rfsim5g-oai-gnb is up-to-date
Creating rfsim5g-oai-nr-ue2 ... done
```

Wait for a bit.

```bash
$ docker-compose ps -a
       Name                     Command                  State                  Ports
-------------------------------------------------------------------------------------------------
rfsim5g-mysql        docker-entrypoint.sh mysqld      Up (healthy)   3306/tcp, 33060/tcp
rfsim5g-oai-amf      /bin/bash /openair-amf/bin ...   Up (healthy)   38412/sctp, 80/tcp, 9090/tcp
rfsim5g-oai-ext-dn   /bin/bash -c  apt update;  ...   Up (healthy)
rfsim5g-oai-gnb      /opt/oai-gnb/bin/entrypoin ...   Up (healthy)
rfsim5g-oai-nr-ue    /opt/oai-nr-ue/bin/entrypo ...   Up (healthy)
rfsim5g-oai-nr-ue2   /opt/oai-nr-ue/bin/entrypo ...   Up (healthy)
rfsim5g-oai-smf      /bin/bash /openair-smf/bin ...   Up (healthy)   80/tcp, 8805/udp, 9090/tcp
rfsim5g-oai-upf      /bin/bash /openair-upf/bin ...   Up (healthy)   2152/udp, 8805/udp
```

Making sure the Second OAI UE is connected:

```bash
$ docker exec -it rfsim5g-oai-nr-ue2 /bin/bash
root@bb4d400a832d:/opt/oai-nr-ue# ifconfig
eth0: flags=4163<UP,BROADCAST,RUNNING,MULTICAST>  mtu 1500
        inet 192.168.71.151  netmask 255.255.255.192  broadcast 192.168.71.191
        ether 02:42:c0:a8:47:8a  txqueuelen 0  (Ethernet)
        RX packets 3192021  bytes 67784900946 (67.7 GB)
        RX errors 0  dropped 0  overruns 0  frame 0
        TX packets 3397743  bytes 91320004542 (91.3 GB)
        TX errors 0  dropped 0 overruns 0  carrier 0  collisions 0

lo: flags=73<UP,LOOPBACK,RUNNING>  mtu 65536
        inet 127.0.0.1  netmask 255.0.0.0
        loop  txqueuelen 1000  (Local Loopback)
        RX packets 0  bytes 0 (0.0 B)
        RX errors 0  dropped 0  overruns 0  frame 0
        TX packets 0  bytes 0 (0.0 B)
        TX errors 0  dropped 0 overruns 0  carrier 0  collisions 0

oaitun_ue1: flags=4305<UP,POINTOPOINT,RUNNING,NOARP,MULTICAST>  mtu 1500
        inet 12.1.1.3  netmask 255.255.255.0  destination 12.1.1.3
        unspec 00-00-00-00-00-00-00-00-00-00-00-00-00-00-00-00  txqueuelen 500  (UNSPEC)
        RX packets 0  bytes 0 (0.0 B)
        RX errors 0  dropped 0  overruns 0  frame 0
        TX packets 0  bytes 0 (0.0 B)
        TX errors 0  dropped 0 overruns 0  carrier 0  collisions 0
```

# 3. Check traffic #

## 3.1. Check your Internet connectivity ##

```bash
$ docker exec -it rfsim5g-oai-nr-ue /bin/bash
root@bb4d400a832d:/opt/oai-nr-ue# ping -I oaitun_ue1 -c 10 www.lemonde.fr
PING s2.shared.global.fastly.net (151.101.122.217) from 12.1.1.2 oaitun_ue1: 56(84) bytes of data.
64 bytes from 151.101.122.217 (151.101.122.217): icmp_seq=1 ttl=53 time=64.5 ms
64 bytes from 151.101.122.217 (151.101.122.217): icmp_seq=2 ttl=53 time=37.0 ms
64 bytes from 151.101.122.217 (151.101.122.217): icmp_seq=3 ttl=53 time=43.2 ms
64 bytes from 151.101.122.217 (151.101.122.217): icmp_seq=4 ttl=53 time=43.2 ms
64 bytes from 151.101.122.217 (151.101.122.217): icmp_seq=5 ttl=53 time=54.3 ms
64 bytes from 151.101.122.217 (151.101.122.217): icmp_seq=6 ttl=53 time=24.0 ms
64 bytes from 151.101.122.217 (151.101.122.217): icmp_seq=7 ttl=53 time=32.5 ms
64 bytes from 151.101.122.217 (151.101.122.217): icmp_seq=8 ttl=53 time=37.0 ms
64 bytes from 151.101.122.217 (151.101.122.217): icmp_seq=9 ttl=53 time=41.2 ms
64 bytes from 151.101.122.217 (151.101.122.217): icmp_seq=10 ttl=53 time=50.3 ms

--- s2.shared.global.fastly.net ping statistics ---
10 packets transmitted, 10 received, 0% packet loss, time 9011ms
rtt min/avg/max/mdev = 24.035/42.765/64.557/10.904 ms
```

If it does not work, certainly you need to modify the DNS values in the docker-compose.

But you can also check with the `ext-dn` container (IP address is `192.168.72.135` in docker-compose)

```bash
$ docker exec -it rfsim5g-oai-nr-ue /bin/bash
root@bb4d400a832d# ping -I oaitun_ue1 -c 2 192.168.72.135
PING 192.168.72.135 (192.168.72.135) from 12.1.1.2 oaitun_ue1: 56(84) bytes of data.
64 bytes from 192.168.72.135: icmp_seq=1 ttl=63 time=10.9 ms
64 bytes from 192.168.72.135: icmp_seq=2 ttl=63 time=16.5 ms

--- 192.168.72.135 ping statistics ---
2 packets transmitted, 2 received, 0% packet loss, time 1001ms
rtt min/avg/max/mdev = 10.939/13.747/16.556/2.810 ms
```

Let now try to check UDP traffic in Downlink.

You will need 2 terminals: one in the NR-UE container, one in the ext-dn container.

Note:
Similarly, Second OAI UE Internet connectivity can be checked.

## 3.2. Start the `iperf` server inside the NR-UE container ##

```bash
$ docker exec -it rfsim5g-oai-nr-ue /bin/bash
root@bb4d400a832d:/opt/oai-nr-ue# iperf -B 12.1.1.2 -u -i 1 -s
------------------------------------------------------------
Server listening on UDP port 5001
Binding to local address 12.1.1.2
Receiving 1470 byte datagrams
UDP buffer size:  208 KByte (default)
------------------------------------------------------------
```

## 3.3. Start the `iperf` client inside the ext-dn container ##

```bash
$ docker exec -it rfsim5g-oai-ext-dn /bin/bash
root@f239e31a0bd0:/# iperf -c 12.1.1.2 -u -i 1 -t 20 -b 500K
------------------------------------------------------------
Client connecting to 12.1.1.2, UDP port 5001
Sending 1470 byte datagrams, IPG target: 22968.75 us (kalman adjust)
UDP buffer size:  208 KByte (default)
------------------------------------------------------------
[  3] local 192.168.72.135 port 58800 connected with 12.1.1.2 port 5001
[ ID] Interval       Transfer     Bandwidth
[  3]  0.0- 1.0 sec  64.6 KBytes   529 Kbits/sec
[  3]  1.0- 2.0 sec  63.2 KBytes   517 Kbits/sec
[  3]  2.0- 3.0 sec  61.7 KBytes   506 Kbits/sec
[  3]  3.0- 4.0 sec  63.2 KBytes   517 Kbits/sec
[  3]  4.0- 5.0 sec  61.7 KBytes   506 Kbits/sec
[  3]  5.0- 6.0 sec  63.2 KBytes   517 Kbits/sec
[  3]  6.0- 7.0 sec  61.7 KBytes   506 Kbits/sec
[  3]  7.0- 8.0 sec  63.2 KBytes   517 Kbits/sec
[  3]  8.0- 9.0 sec  61.7 KBytes   506 Kbits/sec
[  3]  9.0-10.0 sec  63.2 KBytes   517 Kbits/sec
[  3] 10.0-11.0 sec  61.7 KBytes   506 Kbits/sec
[  3] 11.0-12.0 sec  63.2 KBytes   517 Kbits/sec
[  3] 12.0-13.0 sec  61.7 KBytes   506 Kbits/sec
[  3] 13.0-14.0 sec  63.2 KBytes   517 Kbits/sec
[  3] 14.0-15.0 sec  63.2 KBytes   517 Kbits/sec
[  3] 15.0-16.0 sec  61.7 KBytes   506 Kbits/sec
[  3] 16.0-17.0 sec  63.2 KBytes   517 Kbits/sec
[  3] 17.0-18.0 sec  61.7 KBytes   506 Kbits/sec
[  3] 18.0-19.0 sec  63.2 KBytes   517 Kbits/sec
[  3] 19.0-20.0 sec  61.7 KBytes   506 Kbits/sec
[  3]  0.0-20.0 sec  1.22 MBytes   512 Kbits/sec
[  3] Sent 872 datagrams
[  3] Server Report:
[  3]  0.0-20.0 sec  1.22 MBytes   510 Kbits/sec   0.000 ms    3/  872 (0%)
```

Back on your NR-UE terminal you shall see:

```bash
[  3] local 12.1.1.2 port 5001 connected with 192.168.72.135 port 58800
[ ID] Interval       Transfer     Bandwidth        Jitter   Lost/Total Datagrams
[  3]  0.0- 1.0 sec  63.2 KBytes   517 Kbits/sec   1.113 ms    0/   44 (0%)
[  3]  1.0- 2.0 sec  61.7 KBytes   506 Kbits/sec   1.466 ms    0/   43 (0%)
[  3]  2.0- 3.0 sec  63.2 KBytes   517 Kbits/sec   1.770 ms    0/   44 (0%)
[  3]  3.0- 4.0 sec  61.7 KBytes   506 Kbits/sec   1.378 ms    0/   43 (0%)
[  3]  4.0- 5.0 sec  63.2 KBytes   517 Kbits/sec   1.614 ms    0/   44 (0%)
[  3]  5.0- 6.0 sec  63.2 KBytes   517 Kbits/sec   1.427 ms    0/   44 (0%)
[  3]  6.0- 7.0 sec  60.3 KBytes   494 Kbits/sec   1.507 ms    1/   43 (2.3%)
[  3]  7.0- 8.0 sec  63.2 KBytes   517 Kbits/sec   1.409 ms    0/   44 (0%)
[  3]  8.0- 9.0 sec  61.7 KBytes   506 Kbits/sec   1.525 ms    0/   43 (0%)
[  3]  9.0-10.0 sec  63.2 KBytes   517 Kbits/sec   1.393 ms    0/   44 (0%)
[  3] 10.0-11.0 sec  61.7 KBytes   506 Kbits/sec   1.377 ms    0/   43 (0%)
[  3] 11.0-12.0 sec  63.2 KBytes   517 Kbits/sec   1.501 ms    0/   44 (0%)
[  3] 12.0-13.0 sec  61.7 KBytes   506 Kbits/sec   1.788 ms    0/   43 (0%)
[  3] 13.0-14.0 sec  63.2 KBytes   517 Kbits/sec   1.466 ms    0/   44 (0%)
[  3] 14.0-15.0 sec  61.7 KBytes   506 Kbits/sec   1.381 ms    0/   43 (0%)
[  3] 15.0-16.0 sec  61.7 KBytes   506 Kbits/sec   1.417 ms    1/   44 (2.3%)
[  3] 16.0-17.0 sec  61.7 KBytes   506 Kbits/sec   1.569 ms    0/   43 (0%)
[  3] 17.0-18.0 sec  63.2 KBytes   517 Kbits/sec   1.492 ms    1/   45 (2.2%)
[  3] 18.0-19.0 sec  61.7 KBytes   506 Kbits/sec   1.376 ms    0/   43 (0%)
[  3] 19.0-20.0 sec  61.7 KBytes   506 Kbits/sec   1.589 ms    0/   43 (0%)
[  3]  0.0-20.0 sec  1.22 MBytes   510 Kbits/sec   1.551 ms    3/  872 (0.34%)
```

The `500 Kbits/sec` value may change depending on your CPU power!

# 4. Un-deployment #

```bash
$ docker-compose down
Stopping rfsim5g-oai-nr-ue2 ... done
Stopping rfsim5g-oai-nr-ue  ... done
Stopping rfsim5g-oai-gnb    ... done
Stopping rfsim5g-oai-ext-dn ... done
Stopping rfsim5g-oai-upf    ... done
Stopping rfsim5g-oai-smf    ... done
Stopping rfsim5g-oai-amf    ... done
Stopping rfsim5g-mysql      ... done
Removing rfsim5g-oai-nr-ue2 ... done
Removing rfsim5g-oai-nr-ue  ... done
Removing rfsim5g-oai-gnb    ... done
Removing rfsim5g-oai-ext-dn ... done
Removing rfsim5g-oai-upf    ... done
Removing rfsim5g-oai-smf    ... done
Removing rfsim5g-oai-amf    ... done
Removing rfsim5g-mysql      ... done
Removing network rfsim5g-oai-public-net
Removing network rfsim5g-oai-traffic-net
```

# 5. Explanations on the configuration in the `docker-compose.yaml` #

## 5.1. Making the NR-UE connect to the core network ##

The NR-UE **SHALL** be provisioned in the core network, especially in the `SQL` database and in the `AMF`.

* in AMF section of `docker-compose.yaml` --> `OPERATOR_KEY=c42449363bbad02b66d16bc975d77cc1`
* in NR-UE section                        --> `OPC: 'C42449363BBAD02B66D16BC975D77CC1'

Both values shall match!

This value is also present in the `oai_db.sql` file:

```bash
INSERT INTO `users` VALUES ('208990100001100','1','55000000000000',NULL,'PURGED',50,40000000,100000000,47,0000000000,1,0xfec86ba6eb707ed08905757b1bb44b8f,0,0,0x40,'ebd07771ace8677a',0xc42449363bbad02b66d16bc975d77cc1);
INSERT INTO `users` VALUES ('208990100001101','1','55000000000000',NULL,'PURGED',50,40000000,100000000,47,0000000000,1,0xfec86ba6eb707ed08905757b1bb44b8f,0,0,0x40,'ebd07771ace8677a',0xc42449363bbad02b66d16bc975d77cc1);
```

As you can see, 2 other values shall match in the NR-UE section of `docker-compose.yaml`:

All the values such as IMSI and KEY are taken from the configuration file mounted into the container. For the first UE, provision as usual through the config file

```yaml
 oai-nr-ue:
        [...]
        volumes:
            - ../../conf_files/nrue.uicc.conf:/opt/oai-nr-ue/etc/nr-ue.conf
```

with the config having:
```libconfig
uicc0 = {
  imsi = "208990100001100";
  key = "fec86ba6eb707ed08905757b1bb44b8f";
  opc= "C42449363BBAD02B66D16BC975D77CC1";
  dnn= "oai";
  nssai_sst=1;
}
```

The second UE's IMSI might be changed by either having the second UEs
docker-compose entry mount another config, or add `--uicc0.imsi
208990100001101` in `USE_ADDITIONAL_OPTIONS` entry. Note that the latter is a
feature of the configuration module to overwrite any configuration option in
the config file on the command line.

## 5.2. Making the gNB connect to the core network ##

Mainly you need to match the PLMN in `gNB`, `AMF` and `UPF` parameters in the `mini_nonrf_config.yaml`:

```yaml
  plmn_support_list:
    - mcc: 208
      mnc: 99
      tac: 0x0001
      nssai:
        - *embb_slice1
...
snssais:
  - &embb_slice1
    sst: 1
```

The `ST` and `SD` values shall also match.


# 6. Running with local changes

You can run the testcase with local changes by substituting the binaries in
execution images. `local-override.yaml` file provides a way to substitute the
gNB and nrUE executables as well as librfsimulator.so. Refer to the `-volumes`
section in the file for details. This includes an image build service as well as
code compilation service. This is necessary as the executable has to be linked
against the same libraries that are present in the executing image. This might
take a while the first time but other that that is very fast. Here is a list of
commands (wait between each command). Tested with `docker compose` v2.27.0


This command deploys OAI 5G Core Network
```bash
docker compose -f docker-compose.yaml -f local-override.yaml up -d mysql oai-amf oai-smf oai-upf oai-ext-dn
```
This command builds base images locally, builds local gNB & nrUE executable and
runs the gnb service with modified gNB executable.
```bash
docker compose -f docker-compose.yaml -f local-override.yaml up -d oai-gnb
```
This command rebuilds both the gNB & nrUE and runs the oai-nr-ue container with 
modified nrUE executable.
```bash
docker compose -f docker-compose.yaml -f local-override.yaml up -d oai-nr-ue
```

## 6.1 Running nrUE in gdb
`local-override-ue-gdb.yaml` is an additional override file which can be used
to run the UE executable in gdb. Replace the last command above with the
following:

```bash
docker compose -f docker-compose.yaml -f local-override.yaml -f local-override-ue-gdb.yaml run oai-nr-ue
```
