EUTRA-UE-Variables DEFINITIONS AUTOMATIC TAGS ::=
 
BEGIN


VarConnEstFailReport-r11 ::=		SEQUENCE {
	connEstFailReport-r11				ConnEstFailReport-r11,
	plmn-Identity-r11					PLMN-Identity
}


VarLogMeasConfig-r10 ::=				SEQUENCE {
	areaConfiguration-r10			AreaConfiguration-r10		OPTIONAL,
	loggingDuration-r10				LoggingDuration-r10,
	loggingInterval-r10				LoggingInterval-r10
}

VarLogMeasConfig-r11 ::=		SEQUENCE {
	areaConfiguration-r10			AreaConfiguration-r10		OPTIONAL,
	areaConfiguration-v1130			AreaConfiguration-v1130		OPTIONAL,
	loggingDuration-r10				LoggingDuration-r10,
	loggingInterval-r10				LoggingInterval-r10
}

VarLogMeasConfig-r12 ::=		SEQUENCE {
	areaConfiguration-r10			AreaConfiguration-r10		OPTIONAL,
	areaConfiguration-v1130			AreaConfiguration-v1130		OPTIONAL,
	loggingDuration-r10				LoggingDuration-r10,
	loggingInterval-r10				LoggingInterval-r10,
	targetMBSFN-AreaList-r12		TargetMBSFN-AreaList-r12	OPTIONAL
}


VarLogMeasReport-r10 ::=				SEQUENCE {
	traceReference-r10					TraceReference-r10,
	traceRecordingSessionRef-r10			OCTET STRING (SIZE (2)),
	tce-Id-r10							OCTET STRING (SIZE (1)),
	plmn-Identity-r10					PLMN-Identity,
	absoluteTimeInfo-r10				AbsoluteTimeInfo-r10,
	logMeasInfoList-r10					LogMeasInfoList2-r10
}

VarLogMeasReport-r11 ::=			SEQUENCE {
	traceReference-r10					TraceReference-r10,
	traceRecordingSessionRef-r10		OCTET STRING (SIZE (2)),
	tce-Id-r10							OCTET STRING (SIZE (1)),
	plmn-IdentityList-r11				PLMN-IdentityList3-r11,
	absoluteTimeInfo-r10				AbsoluteTimeInfo-r10,
	logMeasInfoList-r10					LogMeasInfoList2-r10
}

LogMeasInfoList2-r10 ::=				SEQUENCE (SIZE (1..maxLogMeas-r10)) OF LogMeasInfo-r10


VarMeasConfig ::=					SEQUENCE {
	-- Measurement identities
	measIdList							MeasIdToAddModList					OPTIONAL,
	measIdListExt-r12					MeasIdToAddModListExt-r12			OPTIONAL,
	-- Measurement objects
	measObjectList						MeasObjectToAddModList				OPTIONAL,
	measObjectList-v9i0					MeasObjectToAddModList-v9e0			OPTIONAL,
	-- Reporting configurations
	reportConfigList					ReportConfigToAddModList			OPTIONAL,
	-- Other parameters
	quantityConfig						QuantityConfig						OPTIONAL,
	measScaleFactor-r12					MeasScaleFactor-r12					OPTIONAL, 
	s-Measure							INTEGER (-140..-44)					OPTIONAL,
	speedStatePars						CHOICE {
		release								NULL,
		setup								SEQUENCE {
			mobilityStateParameters				MobilityStateParameters,
			timeToTrigger-SF					SpeedStateScaleFactors
		}
	}																		OPTIONAL,
	allowInterruptions-r11			BOOLEAN								OPTIONAL
}


VarMeasReportList ::=				SEQUENCE (SIZE (1..maxMeasId)) OF VarMeasReport
VarMeasReportList-r12 ::=			SEQUENCE (SIZE (1..maxMeasId-r12)) OF VarMeasReport

VarMeasReport ::=					SEQUENCE {
	-- List of measurement that have been triggered
	measId								MeasId,
	measId-v1250						MeasId-v1250					OPTIONAL,
	cellsTriggeredList					CellsTriggeredList				OPTIONAL,
	csi-RS-TriggeredList-r12			CSI-RS-TriggeredList-r12		OPTIONAL,
	numberOfReportsSent					INTEGER
}

CellsTriggeredList ::=				SEQUENCE (SIZE (1..maxCellMeas)) OF CHOICE {
	physCellIdEUTRA							PhysCellId,
	physCellIdUTRA							CHOICE {
		fdd										PhysCellIdUTRA-FDD,
		tdd										PhysCellIdUTRA-TDD
	},
	physCellIdGERAN							SEQUENCE {
		carrierFreq								CarrierFreqGERAN,
		physCellId								PhysCellIdGERAN
	},
	physCellIdCDMA2000						PhysCellIdCDMA2000
}

CSI-RS-TriggeredList-r12 ::=		SEQUENCE (SIZE (1..maxCSI-RS-Meas-r12)) OF MeasCSI-RS-Id-r12

VarMobilityHistoryReport-r12 ::=	VisitedCellInfoList-r12


VarRLF-Report-r10 ::=				SEQUENCE {
	rlf-Report-r10							RLF-Report-r9,
	plmn-Identity-r10						PLMN-Identity
}

VarRLF-Report-r11 ::=				SEQUENCE {
	rlf-Report-r10						RLF-Report-r9,
	plmn-IdentityList-r11				PLMN-IdentityList3-r11
}


VarShortMAC-Input ::=					SEQUENCE {
	cellIdentity							CellIdentity,
	physCellId								PhysCellId,
	c-RNTI									C-RNTI
}

maxLogMeas-r10				INTEGER ::= 4060-- Maximum number of logged measurement entries
											--  that can be stored by the UE


END

