EUTRA-UE-Variables DEFINITIONS AUTOMATIC TAGS ::=
 
BEGIN


VarLogMeasConfig-r10 ::=				SEQUENCE {
	areaConfiguration-r10			AreaConfiguration-r10		OPTIONAL,
	loggingDuration-r10				LoggingDuration-r10,
	loggingInterval-r10				LoggingInterval-r10
}


VarLogMeasReport-r10 ::=				SEQUENCE {
	traceReference-r10					TraceReference-r10,
	traceRecordingSessionRef-r10			OCTET STRING (SIZE (2)),
	tce-Id-r10							OCTET STRING (SIZE (1)),
	plmn-Identity-r10					PLMN-Identity,
	absoluteTimeInfo-r10				AbsoluteTimeInfo-r10,
	logMeasInfoList-r10					LogMeasInfoList2-r10
}

LogMeasInfoList2-r10 ::=				SEQUENCE (SIZE (1..maxLogMeas-r10)) OF LogMeasInfo-r10


VarMeasConfig ::=					SEQUENCE {
	-- Measurement identities
	measIdList							MeasIdToAddModList					OPTIONAL,
	-- Measurement objects
	measObjectList						MeasObjectToAddModList				OPTIONAL,
	measObjectList-v9i0					MeasObjectToAddModList-v9e0			OPTIONAL,
	-- Reporting configurations
	reportConfigList					ReportConfigToAddModList			OPTIONAL,
	-- Other parameters
	quantityConfig						QuantityConfig						OPTIONAL,
	s-Measure							INTEGER (-140..-44)					OPTIONAL,
	speedStatePars						CHOICE {
		release								NULL,
		setup								SEQUENCE {
			mobilityStateParameters				MobilityStateParameters,
			timeToTrigger-SF					SpeedStateScaleFactors
		}
	}																		OPTIONAL
}


VarMeasReportList ::=				SEQUENCE (SIZE (1..maxMeasId)) OF VarMeasReport

VarMeasReport ::=					SEQUENCE {
	-- List of measurement that have been triggered
	measId								MeasId,
	cellsTriggeredList					CellsTriggeredList				OPTIONAL,
	numberOfReportsSent					INTEGER
}

CellsTriggeredList ::=				SEQUENCE (SIZE (1..maxCellMeas)) OF CHOICE {
	physCellIdEUTRA							PhysCellId,
	physCellIdUTRA							CHOICE {
		fdd										PhysCellIdUTRA-FDD,
		tdd										PhysCellIdUTRA-TDD
	},
	physCellIdGERAN							SEQUENCE {
		carrierFreq								CarrierFreqGERAN,
		physCellId								PhysCellIdGERAN
	},
	physCellIdCDMA2000						PhysCellIdCDMA2000
}

VarRLF-Report-r10 ::=				SEQUENCE {
	rlf-Report-r10							RLF-Report-r9,
	plmn-Identity-r10						PLMN-Identity
}


VarShortMAC-Input ::=					SEQUENCE {
	cellIdentity							CellIdentity,
	physCellId								PhysCellId,
	c-RNTI									C-RNTI
}

maxLogMeas-r10				INTEGER ::= 4060-- Maximum number of logged measurement entries
											--  that can be stored by the UE


END

