[CONFIG] get parameters from libconfig ../../../targets/PROJECTS/GENERIC-LTE-EPC/CONF/enb.minimassive.master.conf , debug flags: 0x00000000
[CONFIG] function config_libconfig_init returned 0
[CONFIG] config module libconfig loaded
[LIBCONFIG] config: 1/1 parameters successfully set, (1 to default value)
# /dev/cpu_dma_latency set to 0us
[LIBCONFIG] log_config: 3/3 parameters successfully set, (1 to default value)
[LIBCONFIG] log_config: 52/52 parameters successfully set, (46 to default value)
[LIBCONFIG] log_config: 52/52 parameters successfully set, (52 to default value)
[LIBCONFIG] log_config: 15/15 parameters successfully set, (15 to default value)
[LIBCONFIG] log_config: 15/15 parameters successfully set, (15 to default value)
log init done
Reading in command-line options
[LIBCONFIG] (root): 23/23 parameters successfully set, (19 to default value)
[LIBCONFIG] (root): 5/5 parameters successfully set, (4 to default value)
Getting ENBSParams
[LIBCONFIG] (root): 3/3 parameters successfully set, (1 to default value)
[LIBCONFIG] THREAD_STRUCT.[0]: 2/2 parameters successfully set, (0 to default value)
[0m[1;31m[ENB_APP]   Impossible value: PARALLEL_RU_L1_TRX_SPLITaaaaaa
[0m[CONFIG] parallel_conf is set to 0
[LIBCONFIG] THREAD_STRUCT.[0]: 2/2 parameters successfully set, (0 to default value)
[0m[1;31m[ENB_APP]   Impossible value: ENABLE
[0m[CONFIG] worker_conf is set to 0
Configuration: nb_rrc_inst 1, nb_L1_inst 1, nb_ru 1
[LIBCONFIG] loader: 2/2 parameters successfully set, (2 to default value)
[LIBCONFIG] loader.NB_IoT: 2/2 parameters successfully set, (1 to default value)
               nb_nbiot_rrc_inst 0, nb_nbiot_L1_inst 0, nb_nbiot_macrlc_inst 0
[LIBCONFIG] TTracer: 4/4 parameters successfully set, (4 to default value)
configuring for RAU/RRU
CPU Freq is 2.992899 
ITTI init, useMME: 1
[0m[TMR]   Starting itti queue: TASK_UNKNOWN as task 0
[0m[0m[TMR]   Starting itti queue: TASK_TIMER as task 1
[0m[0m[TMR]   Starting itti queue: TASK_L2L1 as task 2
[0m[0m[TMR]   Starting itti queue: TASK_BM as task 3
[0m[0m[TMR]   Starting itti queue: TASK_PHY_ENB as task 4
[0m[0m[TMR]   Starting itti queue: TASK_MAC_ENB as task 5
[0m[0m[TMR]   Starting itti queue: TASK_RLC_ENB as task 6
[0m[0m[TMR]   Starting itti queue: TASK_RRC_ENB_NB_IoT as task 7
[0m[0m[TMR]   Starting itti queue: TASK_PDCP_ENB as task 8
[0m[0m[TMR]   Starting itti queue: TASK_DATA_FORWARDING as task 9
[0m[0m[TMR]   Starting itti queue: TASK_END_MARKER as task 10
[0m[0m[TMR]   Starting itti queue: TASK_RRC_ENB as task 11
[0m[0m[TMR]   Starting itti queue: TASK_RRC_GNB as task 12
[0m[0m[TMR]   Starting itti queue: TASK_RAL_ENB as task 13
[0m[0m[TMR]   Starting itti queue: TASK_S1AP as task 14
[0m[0m[TMR]   Starting itti queue: TASK_X2AP as task 15
[0m[0m[TMR]   Starting itti queue: TASK_M2AP_ENB as task 16
[0m[0m[TMR]   Starting itti queue: TASK_M2AP_MCE as task 17
[0m[0m[TMR]   Starting itti queue: TASK_M3AP as task 18
[0m[0m[TMR]   Starting itti queue: TASK_M3AP_MME as task 19
[0m[0m[TMR]   Starting itti queue: TASK_M3AP_MCE as task 20
[0m[0m[TMR]   Starting itti queue: TASK_SCTP as task 21
[0m[0m[TMR]   Starting itti queue: TASK_ENB_APP as task 22
[0m[0m[TMR]   Starting itti queue: TASK_GNB_APP as task 23
[0m[0m[TMR]   Starting itti queue: TASK_MCE_APP as task 24
[0m[0m[TMR]   Starting itti queue: TASK_MME_APP as task 25
[0m[0m[TMR]   Starting itti queue: TASK_FLEXRAN_AGENT as task 26
[0m[0m[TMR]   Starting itti queue: TASK_PHY_UE as task 27
[0m[0m[TMR]   Starting itti queue: TASK_MAC_UE as task 28
[0m[0m[TMR]   Starting itti queue: TASK_RLC_UE as task 29
[0m[0m[TMR]   Starting itti queue: TASK_PDCP_UE as task 30
[0m[0m[TMR]   Starting itti queue: TASK_RRC_UE as task 31
[0m[0m[TMR]   Starting itti queue: TASK_NAS_UE as task 32
[0m[0m[TMR]   Starting itti queue: TASK_RAL_UE as task 33
[0m[0m[TMR]   Starting itti queue: TASK_MSC as task 34
[0m[0m[TMR]   Starting itti queue: TASK_GTPV1_U as task 35
[0m[0m[TMR]   Starting itti queue: TASK_UDP as task 36
[0m[0m[TMR]   Starting itti queue: TASK_CU_F1 as task 37
[0m[0m[TMR]   Starting itti queue: TASK_DU_F1 as task 38
[0m[LIBCONFIG] opt: 3/3 parameters successfully set, (3 to default value)
[0m[OPT]   OPT disabled
[0mreported resolution = 1 ns
[0m[HW]   Version: Branch: NR_RRC_harq_hacks Abrev. Hash: 94fa9c5 Date: Fri Jun 19 18:16:53 2020 +0200
[0mRuntime table
[0m[PHY]   RC.eNB = 0x2b10b70
[0m[LIBCONFIG] L1s.[0]: 24/24 parameters successfully set, (22 to default value)
[0m[PHY]   RC.eNB[0] = 0x2b10c20
[0m[0m[PHY]   RC.eNB[0][0] = 0x7f9fab347010
[0m[0m[ENB_APP]   Initializing northbound interface for L1
[0m[0m[PHY]   l1_north_init_eNB() RC.nb_L1_inst:1
[0m[0m[PHY]   l1_north_init_eNB() RC.nb_L1_CC[0]:1
[0m[0m[PHY]   l1_north_init_eNB() RC.eNB[0][0] installing callbacks
[0m[0m[PHY]   read_config_and_init() RC.nb_L1_inst: 1
[0m[LIBCONFIG] MACRLCs.[0]: 20/20 parameters successfully set, (15 to default value)
[LIBCONFIG] MACRLCs.[0]: 20/20 parameters successfully set, (15 to default value)
[0m[MAC]   [MAIN] Init function start:nb_macrlc_inst=1
[0m[0m[PDCP]   PDCP layer has been initialized
[0mConfiguring local RRC for MACRLC
[0m[ENB_APP]   sched mode = default 0 [default]
[0m[0m[MAC]   read_config_and_init() RC.nb_macrlc_inst: 1
[0m[0m[PHY]   l1_north_init_eNB() RC.nb_L1_inst:1
[0m[0m[PHY]   l1_north_init_eNB() RC.nb_L1_CC[0]:1
[0m[0m[PHY]   l1_north_init_eNB() RC.eNB[0][0] installing callbacks
[0m[LIBCONFIG] (root): 3/3 parameters successfully set, (1 to default value)
[LIBCONFIG] eNBs.[0]: 20/20 parameters successfully set, (11 to default value)
[0m[RRC]   Instance 0: Southbound Transport local_mac
[0m[0m[RRC]   Setting node_type to ngran_eNB
[0m[LIBCONFIG] eNBs.[0].plmn_list.[0]: 3/3 parameters successfully set, (0 to default value)
[0m[RRC]   num component carriers 1 
[0m[0m[RRC]   enb_config::RCconfig_RRC() parameter number: 0, total number of parameters: 78, ccspath: eNBs.[0].component_carriers.[0] 
 
[0m[LIBCONFIG] eNBs.[0].component_carriers.[0]: 78/78 parameters successfully set, (17 to default value)
phich.resource 0 (ONESIXTH), phich.duration 0 (NORMAL)
No eMBMS configuration, skipping it
[LIBCONFIG] eNBs.[0].component_carriers.[0].emtc_parameters: 88/88 parameters successfully set, (88 to default value)
No eMTC configuration, skipping it
[LIBCONFIG] eNBs.[0].component_carriers.[0].SLparameters: 39/39 parameters successfully set, (39 to default value)
No SL configuration skipping it
[LIBCONFIG] eNBs.[0].srb1_parameters: 6/6 parameters successfully set, (0 to default value)
[0m[RRC]   Node type 0 
 [0m[LIBCONFIG] (root): 3/3 parameters successfully set, (1 to default value)
[LIBCONFIG] NETWORK_CONTROLLER: 6/6 parameters successfully set, (6 to default value)
[LIBCONFIG] RUs.[0]: 27/27 parameters successfully set, (18 to default value)
Creating RC.ru[0]:0x2b41780
Setting function for RU 0 to eNodeB_3GPP
[0m[PHY]   number of L1 instances 1, number of RU 1, number of CPU cores 4
[0m[0m[FLEXRAN_AGENT]   FlexRAN Agent for eNB 0 is DISABLED
[0m[0m[PDCP]   PDCP layer has been initialized
[0m[0m[PDCP]   pdcp init,usegtp 
[0m[0m[93m[PDCP]   ENB pdcp will use tun interface for MBMS
[0m[NETLINK]Opened socket oaitun_enm1 with fd 84
returnValue 0
returnValue 0
returnValue 0
[0m[OIP]   Interface oaitun_enm1 successfully configured, ip address 10.0.2.1, mask 255.255.255.0 broadcast address 10.0.2.255
[0m[0m[ENB_APP]   Creating ENB_APP eNB Task
[0m[0m[TMR]   Created Posix thread TASK_ENB_APP
[0m[0m[RRC]   Creating RRC eNB Task
[0m[LIBCONFIG] (root): 3/3 parameters successfully set, (1 to default value)
[0m[TMR]   Created Posix thread TASK_RRC_ENB
[0m[LIBCONFIG] eNBs.[0]: 20/20 parameters successfully set, (11 to default value)
[0m[TMR]   Created Posix thread TASK_SCTP
[0m[0m[RRC]   Entering main loop of RRC message task
[0m[LIBCONFIG] eNBs.[0].plmn_list.[0]: 3/3 parameters successfully set, (0 to default value)
[0m[TMR]   Created Posix thread TASK_S1AP
[0m[0m[TMR]   Created Posix thread TASK_UDP
[0m[0m[SCTP]   Starting SCTP layer
[0m[0m[S1AP]   Starting S1AP layer
[0m[0m[UDP]   Initializing UDP task interface
[0m[0m[UDP]   Initializing UDP task interface: DONE
[0m[LIBCONFIG] eNBs.[0].component_carriers.[0]: 78/78 parameters successfully set, (17 to default value)
[LIBCONFIG] eNBs.[0].mme_ip_address.[0]: 5/5 parameters successfully set, (0 to default value)
[LIBCONFIG] eNBs.[0].SCTP: 2/2 parameters successfully set, (0 to default value)
[LIBCONFIG] eNBs.[0].NETWORK_INTERFACES: 11/11 parameters successfully set, (2 to default value)
[0m[TMR]   Created Posix thread TASK_GTPV1_U
[0m[0m[GTPV1U]   Configuring GTPu
[0m[LIBCONFIG] (root): 3/3 parameters successfully set, (1 to default value)
[LIBCONFIG] eNBs.[0]: 1/1 parameters successfully set, (0 to default value)
[LIBCONFIG] gNBs.[0]: 1/1 parameters successfully set, (1 to default value)
[LIBCONFIG] eNBs.[0].NETWORK_INTERFACES: 3/3 parameters successfully set, (0 to default value)
[0m[GTPV1U]   Configuring GTPu address : 192.168.18.199 -> c712a8c0
[0m[0m[ENB_APP]   default drx 2
[0m[0m[ENB_APP]   [eNB 0] eNB_app_register via S1AP for instance 0
[0m[LIBCONFIG] (root): 3/3 parameters successfully set, (1 to default value)
[0m[GTPV1U]   Initializing GTPU stack 0x16968b0
[0m[LIBCONFIG] eNBs.[0]: 20/20 parameters successfully set, (11 to default value)
[LIBCONFIG] eNBs.[0].plmn_list.[0]: 3/3 parameters successfully set, (0 to default value)
[0m[S1AP]   Registered new eNB[0] and macro eNB id 3585
[0m[0m[S1AP]   [eNB 0] check the mme registration state
[0m[0m[GTPV1U]   Tx UDP_INIT IP addr 192.168.18.199 (868)
[0m[0m[UDP]   Initializing UDP for local address 192.168.18.199 with port 2152
[0m[0m[TMR]   Created Posix thread TASK_X2AP
[0m[0m[MAC]   Creating MAC eNB Task
[0m[LIBCONFIG] eNBs.[0].component_carriers.[0]: 78/78 parameters successfully set, (17 to default value)
[LIBCONFIG] list eNBs.[0].target_enb_x2_ip_address not found in config file ../../../targets/PROJECTS/GENERIC-LTE-EPC/CONF/enb.minimassive.master.conf 
[LIBCONFIG] eNBs.[0]: 2/2 parameters successfully set, (0 to default value)
[LIBCONFIG] eNBs.[0].SCTP: 2/2 parameters successfully set, (0 to default value)
[0m[UDP]   Inserting new descriptor for task 35, sd 85
[0m[LIBCONFIG] eNBs.[0].NETWORK_INTERFACES: 11/11 parameters successfully set, (2 to default value)
[0m[UDP]   Initializing UDP for local address 192.168.18.199 with port 2152: DONE
[0m[0m[MAC]   Starting main loop of MAC message task
[0m[LIBCONFIG] eNBs.[0]: 1/1 parameters successfully set, (1 to default value)
[0m[SCTP]   sctp_bindx SCTP_BINDX_ADD_ADDR socket bound to : 192.168.18.199
[0m[0m[X2AP]   Registered new eNB[0] and macro eNB id 3585
[0m[0m[X2AP]   eNB[0] eNB id 3585 acting as a listner (server)
[0m[0m[TMR]   Created Posix thread TASK_MAC_ENB
[0m[0m[SCTP]   Converted ipv4 address 192.168.18.99 to network type
[0m[0m[RRC]   [eNB 0] Received RRC_CONFIGURATION_REQ : 0x2b4a80c
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 0] Init...
[0m[0m[SCTP]   connectx assoc_id  903 in progress..., used 1 addresses
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 0] Checking release 
[0m[0m[SCTP]   Inserted new descriptor for sd 86 in list, nb elements 1, assoc_id 903
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 0] Rel14 RRC detected, MBMS flag 0
[0m[0m[SCTP]   Received SCTP_INIT_MSG_MULTI_REQ
[0m[0m[RRC]   [eNB 0] Node type 0 
 [0m[0m[SCTP]   Creating new listen socket on port 36422 with
[0m[0m[SCTP]   ipv4 addresses:
[0m[0m[SCTP]   	- 192.168.18.199
[0m[0m[RRC]   configuration->schedulingInfoSIB1_BR_r13[CC_id] 0
[0m[0m[RRC]   Configuring MIB (N_RB_DL 25,phich_Resource 0,phich_Duration 0)
[0m[0m[RRC]   [MIB] systemBandwidth 2, phich_duration 0, phich_resource 0, sfn 0
[0m[0m[RRC]   [MIB] schedulingInfoSIB1 0
[0m[0m[RRC]   [eNB 0] Configuration SIB2/3, eMBMS = 0
[0m[0m[RRC]   do_SIB23, size 38 
 [0m[0m[MAC]   Configuring MIB for instance 0, CCid 0 : (band 7,N_RB_DL 25,Nid_cell 0,p 1,DL freq 2680000000,phich_config.resource 0, phich_config.duration 0)
[0m[0m[MAC]   config_mib() NFAPI_CONFIG_REQUEST(num_tlv:16) DL_BW:25 UL_BW:25 Ncp 0,p_eNB 1,earfcn 3350,band 7,phich_resource 0 phich_duration 0 phich_power_offset 6000 PSS 6000 SSS 6000 PCI 0 PBCH repetition 0
[0m[0m[MAC]   [CONFIG]SIB2/3 Contents (partial)
[0m[0m[MAC]   [CONFIG]pusch_config_common.n_SB = 1
[0m[0m[MAC]   [CONFIG]pusch_config_common.hoppingMode = 0
[0m[0m[MAC]   [CONFIG]pusch_config_common.pusch_HoppingOffset = 0
[0m[0m[MAC]   [CONFIG]pusch_config_common.enable64QAM = 0
[0m[0m[MAC]   [CONFIG]pusch_config_common.groupHoppingEnabled = 1
[0m[0m[MAC]   [CONFIG]pusch_config_common.groupAssignmentPUSCH = 0
[0m[0m[MAC]   [CONFIG]pusch_config_common.sequenceHoppingEnabled = 0
[0m[0m[MAC]   [CONFIG]pusch_config_common.cyclicShift  = 1
[0m[0m[PHY]   Configuring MIB for instance 0, CCid 0 : (band 7,N_RB_DL 25, N_RB_UL 25, Nid_cell 0,eNB_tx_antenna_ports 1,Ncp 0,DL freq 3350,phich_config.resource 0, phich_config.duration 0)
[0m[0m[PHY]   Initializing frame parms for N_RB_DL 25, Ncp 0, osf 1
[0m[0m[PHY]   lte_parms.c: Setting N_RB_DL to 25, ofdm_symbol_size 512
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   Received notification for sd 86, type 32769
[0m[0m[SCTP]   Client association changed: 0
[0m[0m[SCTP]   ----------------------
[0m[0m[SCTP]   Peer addresses:
[0m[0m[SCTP]       - [192.168.18.99]
[0m[0m[SCTP]   ----------------------
[0m[0m[SCTP]   ----------------------
[0m[0m[SCTP]   SCTP Status:
[0m[0m[SCTP]   assoc id .....: 903
[0m[0m[SCTP]   state ........: 4
[0m[0m[SCTP]   instrms ......: 2
[0m[0m[SCTP]   outstrms .....: 2
[0m[0m[SCTP]   fragmentation : 1452
[0m[0m[SCTP]   pending data .: 0
[0m[0m[SCTP]   unack data ...: 0
[0m[0m[SCTP]   rwnd .........: 106496
[0m[0m[SCTP]   peer info     :
[0m[0m[SCTP]       state ....: 2
[0m[0m[SCTP]       cwnd .....: 4380
[0m[0m[SCTP]       srtt .....: 0
[0m[0m[SCTP]       rto ......: 3000
[0m[0m[SCTP]       mtu ......: 1500
[0m[0m[SCTP]   ----------------------
[0m[0m[SCTP]   Comm up notified for sd 86, assigned assoc_id 903
[0m[0m[S1AP]   3585 -> 00e010
[0m<S1AP-PDU>
    <initiatingMessage>
        <procedureCode>17</procedureCode>
        <criticality><reject/></criticality>
        <value>
            <S1SetupRequest>
                <protocolIEs>
                    <S1SetupRequestIEs>
                        <id>59</id>
                        <criticality><reject/></criticality>
                        <value>
                            <Global-ENB-ID>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <eNB-ID>
                                    <macroENB-ID>
                                        00000000111000000001
                                    </macroENB-ID>
                                </eNB-ID>
                            </Global-ENB-ID>
                        </value>
                    </S1SetupRequestIEs>
                    <S1SetupRequestIEs>
                        <id>60</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <ENBname>eNB-Eurecom-LTEBox</ENBname>
                        </value>
                    </S1SetupRequestIEs>
                    <S1SetupRequestIEs>
                        <id>64</id>
                        <criticality><reject/></criticality>
                        <value>
                            <SupportedTAs>
                                <SupportedTAs-Item>
                                    <tAC>00 01</tAC>
                                    <broadcastPLMNs>
                                        <PLMNidentity>22 F2 10</PLMNidentity>
                                    </broadcastPLMNs>
                                </SupportedTAs-Item>
                            </SupportedTAs>
                        </value>
                    </S1SetupRequestIEs>
                    <S1SetupRequestIEs>
                        <id>137</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <PagingDRX><v128/></PagingDRX>
                        </value>
                    </S1SetupRequestIEs>
                </protocolIEs>
            </S1SetupRequest>
        </value>
    </initiatingMessage>
</S1AP-PDU>
[0m[SCTP]   Successfully sent 59 bytes on stream 0 for assoc_id 903
[0m[LIBCONFIG] loader.coding: 2/2 parameters successfully set, (1 to default value)
[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   Received notification for sd 86, type 32777
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   [903][86] Msg of length 58 received from port 36412, on stream 0, PPID 18
[0m[0m[S1AP]   servedGUMMEIs.list.count 3
[0m[0m[S1AP]   servedPLMNs.list.count 1
[0m[0m[S1AP]   servedPLMNs.list.count 1
[0m[0m[S1AP]   servedPLMNs.list.count 1
[0m[0m[ENB_APP]   [eNB 0] Received S1AP_REGISTER_ENB_CNF: associated MME 1
[0m[LOADER] library libcoding.so successfully loaded
[0m[PHY]   prach_config_common.rootSequenceIndex = 0
[0m[0m[PHY]   prach_config_common.prach_ConfigInfo.prach_ConfigIndex = 0
[0m[0m[PHY]   prach_config_common.prach_ConfigInfo.highSpeedFlag = 0
[0m[0m[PHY]   prach_config_common.prach_ConfigInfo.zeroCorrelationZoneConfig = 1
[0m[0m[PHY]   prach_config_common.prach_ConfigInfo.prach_FreqOffset = 2
[0m[0m[PHY]   pusch_config_common.n_SB = 1
[0m[0m[PHY]   pusch_config_common.hoppingMode = 0
[0m[0m[PHY]   pusch_config_common.pusch_HoppingOffset = 0
[0m[0m[PHY]   pusch_config_common.enable64QAM = 0
[0m[0m[PHY]   pusch_config_common.ul_ReferenceSignalsPUSCH.groupHoppingEnabled = 1
[0m[0m[PHY]   pusch_config_common.ul_ReferenceSignalsPUSCH.groupAssignmentPUSCH = 0
[0m[0m[PHY]   pusch_config_common.ul_ReferenceSignalsPUSCH.sequenceHoppingEnabled = 0
[0m[0m[PHY]   pusch_config_common.ul_ReferenceSignalsPUSCH.cyclicShift = 2
[0m[0m[PHY]   eNB 0/0 configured
[0m[0m[RRC]   [eNB] handover active state is 0 
[0m[0m[RRC]   [eNB] eMBMS active state is 0 
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 0] ENB:OPENAIR RRC IN....
[0m[0m[ENB_APP]   START MAIN THREADS
[0mRC.nb_L1_inst:1
Initializing eNB threads single_thread_flag:0 wait_for_sync:0
[0m[PHY]   [lte-softmodem.c] eNB structure about to allocated RC.nb_L1_inst:1 RC.nb_L1_CC[0]:1
[0m[0m[PHY]   [lte-softmodem.c] eNB structure RC.eNB allocated
[0m[0m[PHY]   Initializing eNB 0 CC_id 0 single_thread_flag:0
[0m[0m[PHY]   Initializing eNB 0 CC_id 0
[0m[0m[PHY]   Registering with MAC interface module
[0m[0m[PHY]   Setting indication lists
[0m[0m[PHY]   [lte-softmodem.c] eNB structure allocated
[0mwait_eNBs()
Waiting for eNB L1 instances to all get configured ... sleeping 50ms (nb_L1_inst 1)
RC.nb_L1_CC[0]:1
eNB L1 are configured
About to Init RU threads RC.nb_RU:1
Initializing RU threads
[0m[1;31m[PHY]   DJP - delete code above this /home/eurecom/panos/NR_RRC_harq_hacks/openairinterface5g/targets/RT/USER/lte-ru.c:2739
[0m[0m[PHY]   Copying frame parms from eNB 0 to ru 0
[0m[0m[PHY]   Initializing RRU descriptor 0 : (local RF,synch_to_ext_device,0)
[0mconfiguring ru_id 0 (start_rf 0x5b1a00)
[0m[PHY]   Starting ru_thread 0, is_slave 0, send_dmrs 0
[0m[0m[PHY]   Initializing RU proc 0 (eNodeB_3GPP,synch_to_ext_device),
[0m[0m[PHY]   init_RU_proc() DJP - added creation of pthread_prach
[0m[0m[93m[HW]   thread_top_init() called with affinity>0, but overruled by #ifndef CPU_AFFINITY.
[0m[0m[HW]   [SCHED][eNB] ru_thread started on CPU 1, sched_policy = SCHED_FIFO , priority = 99, CPU Affinity= CPU_0 CPU_1 CPU_2 CPU_3 
[0m[0m[PHY]   thread ru created id=7295
[0m[0m[PHY]   Starting RU 0 (eNodeB_3GPP,synch_to_ext_device),
[0mwaiting for sync (ru_thread,-1/0xff4968,0x17af520,0x16952a0)
channel 0, Setting tx_gain offset 0.000000, rx_gain offset 118.000000, tx_freq 2680000000.000000, rx_freq 2560000000.000000
[0m[93m[HW]   thread_top_init() called with affinity>0, but overruled by #ifndef CPU_AFFINITY.
[0m[0m[PHY]   Initializing frame parms for N_RB_DL 25, Ncp 0, osf 1
[0m[0m[PHY]   lte_parms.c: Setting N_RB_DL to 25, ofdm_symbol_size 512
[0m[0m[PHY]   Initializing RU signal buffers (if_south local RF) nb_tx 1
[0m[0m[HW]   [SCHED][eNB] ru_thread_prach started on CPU 2, sched_policy = SCHED_FIFO , priority = 99, CPU Affinity= CPU_0 CPU_1 CPU_2 CPU_3 
[0m[0m[PHY]   [INIT] common.txdata[0] = 0x7f9fafc66010 (307200 bytes)
[0m[0m[PHY]   ru_thread_prach() RU configured - RACH processing thread running
[0m[LIBCONFIG] loader.dfts: 2/2 parameters successfully set, (1 to default value)
[LOADER] library libdfts.so successfully loaded
[0m[PHY]   nb_tx 1
[0m[0m[PHY]   rxdata_7_5kHz[0] 0x2b9c1c0 for RU 0
[0m[0m[PHY]   [INIT] common.txdata_BF= 0x2b4ae80 (8 bytes)
[0m[0m[PHY]   txdataF_BF[0] 0x2bba1e0 for RU 0
[0m[0m[PHY]   rxdataF[0] 0x2bc1200 for RU 0
[0m[LIBCONFIG] device.recplay: 7/7 parameters successfully set, (7 to default value)
[LIBCONFIG] device: 1/1 parameters successfully set, (1 to default value)
[LIBCONFIG] loader.oai_device: 2/2 parameters successfully set, (1 to default value)
[LOADER] library liboai_device.so successfully loaded
[0m[HW]   UHD version 3.13.0.HEAD-0-g0ddc19e5 (3.13.0)
[0m[0m[HW]   Found USRP b200
[0mFound USRP b200
[0m[93m[HW]   Clock source set neither in usrp_args nor on command line, using default!
[0m[0m[93m[HW]   Time source set neither in usrp_args nor on command line, using default!
[0m[0m[SCTP]   Found data for descriptor 87
[0m[0m[SCTP]   Received notification for sd 87, type 32769
[0m[0m[SCTP]   Client association changed: 0
[0m[0m[SCTP]   Comm up notified for sd 87, assigned assoc_id 904
[0m[0m[SCTP]   ----------------------
[0m[0m[SCTP]   SCTP Status:
[0m[0m[SCTP]   assoc id .....: 904
[0m[0m[SCTP]   state ........: 4
[0m[0m[SCTP]   instrms ......: 32
[0m[0m[SCTP]   outstrms .....: 32
[0m[0m[SCTP]   fragmentation : 1452
[0m[0m[SCTP]   pending data .: 0
[0m[0m[SCTP]   unack data ...: 0
[0m[0m[SCTP]   rwnd .........: 106496
[0m[0m[SCTP]   peer info     :
[0m[0m[SCTP]       state ....: 2
[0m[0m[SCTP]       cwnd .....: 4380
[0m[0m[SCTP]       srtt .....: 0
[0m[0m[SCTP]       rto ......: 3000
[0m[0m[SCTP]       mtu ......: 1500
[0m[0m[SCTP]   ----------------------
[0mx2ap_eNB_handle_sctp_association_ind at 1 (called for instance 0)
here comes the tree (instance 0):
---------------------------------------------
---------------------------------------------
x2ap_eNB_handle_sctp_association_ind at 2
here comes the tree (instance 0):
---------------------------------------------
-----------------------
eNB id 0 (null)
state 2
nextstream 0
in_streams 0 out_streams 0
cnx_id 1 assoc_id 0
---------------------------------------------
x2ap_eNB_handle_sctp_association_ind at 3
here comes the tree (instance 0):
---------------------------------------------
-----------------------
eNB id 0 (null)
state 2
nextstream 0
in_streams 32 out_streams 32
cnx_id 1 assoc_id 904
---------------------------------------------
[0m[SCTP]   Found data for descriptor 95
[0m[0m[SCTP]   [904][95] Msg of length 66 received from port 36422, on stream 0, PPID 27
[0m<X2AP-PDU>
    <initiatingMessage>
        <procedureCode>36</procedureCode>
        <criticality><reject/></criticality>
        <value>
            <ENDCX2SetupRequest>
                <protocolIEs>
                    <ENDCX2SetupRequest-IEs>
                        <id>244</id>
                        <criticality><reject/></criticality>
                        <value>
                            <InitiatingNodeType-EndcX2Setup>
                                <init-en-gNB>
                                    <En-gNB-ENDCX2SetupReqIEs>
                                        <id>252</id>
                                        <criticality><reject/></criticality>
                                        <value>
                                            <GlobalGNB-ID>
                                                <pLMN-Identity>22 F2 10</pLMN-Identity>
                                                <gNB-ID>
                                                    <gNB-ID>
                                                        00000000000000000000111000000000
                                                    </gNB-ID>
                                                </gNB-ID>
                                            </GlobalGNB-ID>
                                        </value>
                                    </En-gNB-ENDCX2SetupReqIEs>
                                    <En-gNB-ENDCX2SetupReqIEs>
                                        <id>253</id>
                                        <criticality><reject/></criticality>
                                        <value>
                                            <ServedNRcellsENDCX2ManagementList>
                                                <SEQUENCE>
                                                    <servedNRCellInfo>
                                                        <nrpCI>0</nrpCI>
                                                        <nrCellID>
                                                            <pLMN-Identity>22 F2 10</pLMN-Identity>
                                                            <nRcellIdentifier>
                                                                000000000000000000000000111000000000
                                                            </nRcellIdentifier>
                                                        </nrCellID>
                                                        <fiveGS-TAC>00 64 90</fiveGS-TAC>
                                                        <broadcastPLMNs>
                                                            <PLMN-Identity>22 F2 10</PLMN-Identity>
                                                        </broadcastPLMNs>
                                                        <nrModeInfo>
                                                            <tdd>
                                                                <nRFreqInfo>
                                                                    <nRARFCN>0</nRARFCN>
                                                                    <freqBandListNr>
                                                                        <FreqBandNrItem>
                                                                            <freqBandIndicatorNr>1</freqBandIndicatorNr>
                                                                            <supportedSULBandList>
                                                                                <SupportedSULFreqBandItem>
                                                                                    <freqBandIndicatorNr>80</freqBandIndicatorNr>
                                                                                </SupportedSULFreqBandItem>
                                                                            </supportedSULBandList>
                                                                        </FreqBandNrItem>
                                                                    </freqBandListNr>
                                                                </nRFreqInfo>
                                                                <nR-TxBW>
                                                                    <nRSCS><scs15/></nRSCS>
                                                                    <nRNRB><nrb106/></nRNRB>
                                                                </nR-TxBW>
                                                            </tdd>
                                                        </nrModeInfo>
                                                        <measurementTimingConfiguration>00</measurementTimingConfiguration>
                                                    </servedNRCellInfo>
                                                </SEQUENCE>
                                            </ServedNRcellsENDCX2ManagementList>
                                        </value>
                                    </En-gNB-ENDCX2SetupReqIEs>
                                </init-en-gNB>
                            </InitiatingNodeType-EndcX2Setup>
                        </value>
                    </ENDCX2SetupRequest-IEs>
                </protocolIEs>
            </ENDCX2SetupRequest>
        </value>
    </initiatingMessage>
</X2AP-PDU>
[0m[X2AP]   X2AP_ProcedureCode_id_endcX2Setup message!
[0m[0m[X2AP]   TAC: 006490
[0m[0m[X2AP]   PLMN: 22f210
[0m<X2AP-PDU>
    <successfulOutcome>
        <procedureCode>36</procedureCode>
        <criticality><reject/></criticality>
        <value>
            <ENDCX2SetupResponse>
                <protocolIEs>
                    <ENDCX2SetupResponse-IEs>
                        <id>246</id>
                        <criticality><reject/></criticality>
                        <value>
                            <RespondingNodeType-EndcX2Setup>
                                <respond-eNB>
                                    <ENB-ENDCX2SetupReqAckIEs>
                                        <id>21</id>
                                        <criticality><reject/></criticality>
                                        <value>
                                            <GlobalENB-ID>
                                                <pLMN-Identity>22 F2 10</pLMN-Identity>
                                                <eNB-ID>
                                                    <macro-eNB-ID>
                                                        00000000111000000001
                                                    </macro-eNB-ID>
                                                </eNB-ID>
                                            </GlobalENB-ID>
                                        </value>
                                    </ENB-ENDCX2SetupReqAckIEs>
                                    <ENB-ENDCX2SetupReqAckIEs>
                                        <id>250</id>
                                        <criticality><reject/></criticality>
                                        <value>
                                            <ServedEUTRAcellsENDCX2ManagementList>
                                                <SEQUENCE>
                                                    <servedEUTRACellInfo>
                                                        <pCI>0</pCI>
                                                        <cellId>
                                                            <pLMN-Identity>22 F2 10</pLMN-Identity>
                                                            <eUTRANcellIdentifier>
                                                                0000000011100000000100000000
                                                            </eUTRANcellIdentifier>
                                                        </cellId>
                                                        <tAC>00 01</tAC>
                                                        <broadcastPLMNs>
                                                            <PLMN-Identity>22 F2 10</PLMN-Identity>
                                                        </broadcastPLMNs>
                                                        <eUTRA-Mode-Info>
                                                            <fDD>
                                                                <uL-EARFCN>21350</uL-EARFCN>
                                                                <dL-EARFCN>3350</dL-EARFCN>
                                                                <uL-Transmission-Bandwidth><bw25/></uL-Transmission-Bandwidth>
                                                                <dL-Transmission-Bandwidth><bw25/></dL-Transmission-Bandwidth>
                                                            </fDD>
                                                        </eUTRA-Mode-Info>
                                                    </servedEUTRACellInfo>
                                                </SEQUENCE>
                                            </ServedEUTRAcellsENDCX2ManagementList>
                                        </value>
                                    </ENB-ENDCX2SetupReqAckIEs>
                                </respond-eNB>
                            </RespondingNodeType-EndcX2Setup>
                        </value>
                    </ENDCX2SetupResponse-IEs>
                </protocolIEs>
            </ENDCX2SetupResponse>
        </value>
    </successfulOutcome>
</X2AP-PDU>
[0m[SCTP]   Successfully sent 53 bytes on stream 0 for assoc_id 904
[0m[0m[SCTP]   Found data for descriptor 95
[0m[0m[SCTP]   Received notification for sd 95, type 32777
[0m[0m[HW]   cal 0: freq 3500000000.000000, offset 44.000000, diff 940000000.000000
[0m[0m[HW]   cal 1: freq 2660000000.000000, offset 49.800000, diff 100000000.000000
[0m[0m[HW]   cal 2: freq 2300000000.000000, offset 51.000000, diff 260000000.000000
[0m[0m[HW]   cal 3: freq 1880000000.000000, offset 53.000000, diff 680000000.000000
[0m[0m[HW]   cal 4: freq 816000000.000000, offset 57.000000, diff 1744000000.000000
[0m[0m[HW]   RX Gain 0 118.000000 (55.800000) => 62.200000 (max 76.000000)
[0m[0m[HW]   USRP TX_GAIN:89.75 gain_range:89.75 tx_gain:0.00
[0m[0m[HW]   Actual master clock: 30.720000MHz...
[0m[0m[HW]   Actual clock source internal...
[0m[0m[HW]   Actual time source internal...
[0m[0m[HW]   RF board max packet size 1916, size for 100µs jitter 768 
[0m[0m[HW]   rx_max_num_samps 768
[0m[0m[HW]   RX Channel 0
[0m[0m[HW]     Actual RX sample rate: 7.680000MSps...
[0m[0m[HW]     Actual RX frequency: 2.560000GHz...
[0m[0m[HW]     Actual RX gain: 62.000000...
[0m[0m[HW]     Actual RX bandwidth: 20.000000M...
[0m[0m[HW]     Actual RX antenna: RX2...
[0m[0m[HW]   TX Channel 0
[0m[0m[HW]     Actual TX sample rate: 7.680000MSps...
[0m[0m[HW]     Actual TX frequency: 2.680000GHz...
[0m[0m[HW]     Actual TX gain: 89.750000...
[0m[0m[HW]     Actual TX bandwidth: 20.000000M...
[0m[0m[HW]     Actual TX antenna: TX/RX...
[0m[0m[HW]     Actual TX packet size: 1916
[0m[0m[HW]   Device timestamp: 1.703971...
[0m[0m[HW]   [RAU] has loaded USRP B200 device.
[0msetup_RU_buffers: frame_parms = 0x7f9fab347e68
[0m[PHY]   Signaling main thread that RU 0 (is_slave 0,send_dmrs 0) is ready in state RU_RUN
[0mwait RUs
[0m[ENB_APP]   Waiting for RUs to be configured ... RC.ru_mask:00
[0m[0m[PHY]   RUs configured
[0m[0m[ENB_APP]   RC.nb_RU:1
[0mALL RUs ready - init eNBs
[0m[ENB_APP]   Not NFAPI mode - call init_eNB_afterRU()
[0m[0m[PHY]   init_eNB_afterRU() RC.nb_inst:1
[0m[0m[PHY]   RC.nb_CC[inst]:1
[0m[0m[PHY]   RC.nb_CC[inst:0][CC_id:0]:0x7f9fab347010
[0m[0m[PHY]   [eNB 0] phy_init_lte_eNB() About to wait for eNB to be configured[0m[0m[PHY]   [eNB 0] Initializing DL_FRAME_PARMS : N_RB_DL 25, PHICH Resource 1, PHICH Duration 0 nb_antennas_tx:0 nb_antennas_rx:1 nb_antenna_ports_eNB:1 PRACH[rootSequenceIndex:0 prach_Config_enabled:1 configIndex:0 highSpeed:0 zeroCorrelationZoneConfig:1 freqOffset:2]
[0m[0m[PHY]   [eNB 0] Initializing DL_FRAME_PARMS : N_RB_DL 25, PHICH Resource 1, PHICH Duration 0
[0mpcfich_reg : 0,12,25,37
[0m[PHY]   [INIT] NB_ANTENNA_PORTS_ENB:6 fp->nb_antenna_ports_eNB:1
[0m[0m[PHY]   [INIT] common_vars->txdataF[0] = 0x7f9fafb87010 (286720 bytes)
[0m[0m[PHY]   [INIT] common_vars->txdataF[5] = 0x7f9fa80ff010 (286720 bytes)
[0m[0m[PHY]   Mapping RX ports from 1 RUs to eNB 0
[0m[0m[PHY]   Overwriting eNB->prach_vars.rxsigF[0]:0x330a6c0
[0m[0m[PHY]   Overwriting eNB->prach_vars_br.rxsigF.rxsigF[0]:(nil)
[0m[0m[PHY]   Overwriting eNB->prach_vars_br.rxsigF.rxsigF[0]:(nil)
[0m[0m[PHY]   Overwriting eNB->prach_vars_br.rxsigF.rxsigF[0]:(nil)
[0m[0m[PHY]   Overwriting eNB->prach_vars_br.rxsigF.rxsigF[0]:(nil)
[0m[0m[PHY]   eNB->num_RU:1
[0m[0m[PHY]   Attaching RU 0 antenna 0 to eNB antenna 0
[0m[0m[PHY]   init_eNB_afterRU() ************* DJP ***** eNB->frame_parms.nb_antennas_tx:0 - GOING TO HARD CODE TO 1[0m[0m[PHY]   inst 0, CC_id 0 : nb_antennas_rx 1
[0m[0m[PHY]   Initialise transport
[0m[0m[PHY]   init_eNB_proc(inst:0) RC.nb_CC[inst]:1 
[0m[0m[PHY]   Initializing eNB processes instance:0 CC_id 0 
[0m[0m[PHY]   eNB->single_thread_flag:0
[0m[0m[93m[HW]   thread_top_init() called with affinity>0, but overruled by #ifndef CPU_AFFINITY.
[0m[0m[HW]   [SCHED][eNB] eNB_thread_prach started on CPU 0, sched_policy = SCHED_FIFO , priority = 99, CPU Affinity= CPU_0 CPU_1 CPU_2 CPU_3 
[0m[0m[ENB_APP]   ALL RUs ready - ALL eNBs ready
[0m[0m[93m[HW]   thread_top_init() called with affinity>0, but overruled by #ifndef CPU_AFFINITY.
[0m[0m[HW]   [SCHED][eNB] eNB_thread_prach_br started on CPU 0, sched_policy = SCHED_FIFO , priority = 99, CPU Affinity= CPU_0 CPU_1 CPU_2 CPU_3 
[0m[0m[ENB_APP]   Sending sync to all threads
[0m[0m[MME_APP]   Creating MME_APP eNB Task
[0mgot sync (ru_thread)
[0m[TMR]   Created Posix thread TASK_MME_APP
[0m[0m[HW]   Time in secs now: 22168192 
[0m[LIBCONFIG] MMEs.[0]: 1/1 parameters successfully set, (1 to default value)
[0m[MCE_APP]   Creating MCE_APP eNB Task
[0m[0m[HW]   Time in secs last pps: 21747824 
[0m[0m[PHY]   RU 0 rf device ready
[0m[0m[TMR]   Created Posix thread TASK_MCE_APP
[0m[LIBCONFIG] MCEs.[0]: 1/1 parameters successfully set, (1 to default value)
[LIBCONFIG] MCEs.[0]: 1/1 parameters successfully set, (1 to default value)
[0m[ENB_APP]   TYPE <CTRL-C> TO TERMINATE
[0m[0m[ENB_APP]   [MCE 0] MCE_app_register via M3AP for instance 0
[0m[0m[1;31m[HW]   [recv] received 0 samples out of 7680
[0m[0m[1;31m[HW]   ERROR_CODE_OVERFLOW (Out of sequence error)

[0m[0m[1;31m[PHY]   rx_rf: Asked for 7680 samples, got 0 from SDR
[0m[0m[1;31m[PHY]   problem receiving samples[0m[0m[1;31m[MAC]   SCHED_MODE = 0
[0m[0m[PHY]   rx_rf: rfdevice timing drift of 22200737 samples (ts_off 0)
[0m[0m[PHY]   prach_I0 = 0.0 dB
[0m[0m[PHY]   max_I0 18, min_I0 0
[0m[0m[1;31m[PHY]   fill_ulsch UE_id 0 nb_rb = 0
[0m[0m[RRC]   [FRAME 00738][eNB][MOD 00][RNTI 43eb] Decoding UL CCCH 59.e8.a9.2.18.72 (0x3a52693)
[0m[0m[RRC]   [FRAME 00738][eNB][MOD 00][RNTI 43eb] Accept new connection from UE random UE identity (0x8721908a9e000000) MME code 0 TMSI 0 cause 1
[0m[0m[MAC]   UE 0 RNTI 43eb adding LC 1 idx 0 to scheduling control (total 1)
[0m[0m[MAC]   UE 0 RNTI 43eb adding LC 2 idx 1 to scheduling control (total 2)
[0m[0m[MAC]   Added physicalConfigDedicated 0x7f9f600085d0 for 0.0
[0m[0m[RRC]   [FRAME 00738][eNB][MOD 00][RNTI 43eb]CALLING RLC CONFIG SRB1 (rbid 1)
[0madd new uid is 0 43eb

[0m[PDCP]   [FRAME 00738][eNB][MOD 00][RNTI 43eb][SRB 01]  Action ADD  LCID 1 (SRB id 1) configured with SN size 5 bits and RLC AM
[0m[0m[MAC]   generate_Msg4 ra->Msg4_frame SFN/SF: 739.2,  frameP SFN/SF: 739.2 FOR eNB_Mod: 0 
[0m[0m[MAC]   [eNB 0][RAPROC] CC_id 0 Frame 739, subframeP 2: Generating Msg4 with RRC Piggyback (RNTI 43eb)
[0m[0m[1;31m[PHY]   fill_ulsch UE_id 0 nb_rb = 0
[0m[0m[93m[MAC]   [eNB 0][PUSCH 6] CC_id 0 740.6 ULSCH in error in round 0, ul_cqi 132, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 6] CC_id 0 741.4 ULSCH in error in round 1, ul_cqi 138, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 6] CC_id 0 742.2 ULSCH in error in round 2, ul_cqi 134, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 6] CC_id 0 743.0 ULSCH in error in round 3, ul_cqi 132, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 6] CC_id 0 743.8 ULSCH in error in round 0, ul_cqi 140, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 6] CC_id 0 744.6 ULSCH in error in round 1, ul_cqi 140, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 6] CC_id 0 745.4 ULSCH in error in round 2, ul_cqi 142, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 6] CC_id 0 746.2 ULSCH in error in round 3, ul_cqi 143, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 6] CC_id 0 747.0 ULSCH in error in round 0, ul_cqi 143, UE_id 0, RNTI 43eb (len 63)
[0m[0m[1;31m[PHY]   fill_ulsch UE_id 0 nb_rb = 0
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 748.8 ULSCH in error in round 0, ul_cqi 146, UE_id 0, RNTI 43eb (len 63)
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 43eb] [RAPROC] Logical Channel UL-DCCH, processing LTE_RRCConnectionSetupComplete from UE (SRB1 Active)
[0m[0m[NAS]    AttachRequest.c:40  EMM  - attach_request len = 97
[0m[0m[NAS]    UeNetworkCapability.c:46  decode_ue_network_capability len = 7
[0m[0m[NAS]    UeNetworkCapability.c:63  uenetworkcapability decoded UMTS

[0m[0m[NAS]    UeNetworkCapability.c:74  uenetworkcapability decoded GPRS

[0m[0m[NAS]    UeNetworkCapability.c:82  uenetworkcapability decoded=6

[0m[0m[NAS]    UeNetworkCapability.c:86  uenetworkcapability then decoded=8

[0m[0m[NAS]    AttachRequest.c:285  EMM: Can't decode the message with iei 111

[0m[0m[S1AP]   [eNB 0] Build S1AP_NAS_FIRST_REQ adding in s_TMSI: GUMMEI mme_code 1 mme_group_id 32768 ue 43eb
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 43eb] UE State = RRC_CONNECTED 
[0m[0m[S1AP]   [eNB 0] Chose MME 'MME 1' (assoc_id 903) through GUMMEI MCC 222 MNC 1 MMEGI 32768 MMEC 1
[0m[0m[S1AP]   Found usable eNB_ue_s1ap_id: 0x06692d 420141(10)
[0m[0m[S1AP]   GUMMEI_ID_PRESENT
[0m<S1AP-PDU>
    <initiatingMessage>
        <procedureCode>12</procedureCode>
        <criticality><ignore/></criticality>
        <value>
            <InitialUEMessage>
                <protocolIEs>
                    <InitialUEMessage-IEs>
                        <id>8</id>
                        <criticality><reject/></criticality>
                        <value>
                            <ENB-UE-S1AP-ID>420141</ENB-UE-S1AP-ID>
                        </value>
                    </InitialUEMessage-IEs>
                    <InitialUEMessage-IEs>
                        <id>26</id>
                        <criticality><reject/></criticality>
                        <value>
                            <NAS-PDU>
                                17 A0 9C 9B 3F 04 07 41 02 0B F6 22 F2 10 80 00 
                                01 00 00 00 37 07 F0 70 C0 40 10 00 10 00 2A 02 
                                1F D0 11 D1 27 23 80 80 21 10 01 00 00 10 81 06 
                                00 00 00 00 83 06 00 00 00 00 00 0D 00 00 0A 00 
                                00 05 00 00 10 00 00 11 00 52 22 F2 10 00 01 5C 
                                0A 00 31 04 E5 E0 34 01 90 11 03 57 58 A6 5D 01 
                                00 E0 C1 6F 04 F0 00 70 00
                            </NAS-PDU>
                        </value>
                    </InitialUEMessage-IEs>
                    <InitialUEMessage-IEs>
                        <id>67</id>
                        <criticality><reject/></criticality>
                        <value>
                            <TAI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <tAC>00 01</tAC>
                            </TAI>
                        </value>
                    </InitialUEMessage-IEs>
                    <InitialUEMessage-IEs>
                        <id>100</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <EUTRAN-CGI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <cell-ID>
                                    0000000011100000000100000000
                                </cell-ID>
                            </EUTRAN-CGI>
                        </value>
                    </InitialUEMessage-IEs>
                    <InitialUEMessage-IEs>
                        <id>134</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <RRC-Establishment-Cause><highPriorityAccess/></RRC-Establishment-Cause>
                        </value>
                    </InitialUEMessage-IEs>
                    <InitialUEMessage-IEs>
                        <id>75</id>
                        <criticality><reject/></criticality>
                        <value>
                            <GUMMEI>
                                <pLMN-Identity>22 F2 10</pLMN-Identity>
                                <mME-Group-ID>80 00</mME-Group-ID>
                                <mME-Code>01</mME-Code>
                            </GUMMEI>
                        </value>
                    </InitialUEMessage-IEs>
                </protocolIEs>
            </InitialUEMessage>
        </value>
    </initiatingMessage>
</S1AP-PDU>
[0m[SCTP]   Successfully sent 164 bytes on stream 1 for assoc_id 903
[0m[0m[93m[RLC]   /home/eurecom/panos/NR_RRC_harq_hacks/openairinterface5g/openair2/LAYER2/rlc_v2/rlc_entity_am.c:941:generate_status: warning: cannot generate status PDU, not enough room
[0m[0m[93m[RLC]   /home/eurecom/panos/NR_RRC_harq_hacks/openairinterface5g/openair2/LAYER2/rlc_v2/rlc_entity_am.c:941:generate_status: warning: cannot generate status PDU, not enough room
[0m[0m[93m[RLC]   /home/eurecom/panos/NR_RRC_harq_hacks/openairinterface5g/openair2/LAYER2/rlc_v2/rlc_entity_am.c:941:generate_status: warning: cannot generate status PDU, not enough room
[0m[0m[93m[RLC]   /home/eurecom/panos/NR_RRC_harq_hacks/openairinterface5g/openair2/LAYER2/rlc_v2/rlc_entity_am.c:941:generate_status: warning: cannot generate status PDU, not enough room
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   Received notification for sd 86, type 32777
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   [903][86] Msg of length 32 received from port 36412, on stream 1, PPID 18
[0m[0m[RRC]   [eNB 0] Received S1AP_DOWNLINK_NAS: ue_initial_id 1, eNB_ue_s1ap_id 420141
[0m[0m[RRC]   sent RRC_DCCH_DATA_REQ to TASK_PDCP_ENB
[0m[0m[1;31m[PHY]   fill_ulsch UE_id 0 nb_rb = 0
[0m[0m[93m[MAC]   [eNB 0][PUSCH 3] CC_id 0 752.3 ULSCH in error in round 0, ul_cqi 146, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 752.8 ULSCH in error in round 0, ul_cqi 152, UE_id 0, RNTI 43eb (len 63)
[0m<S1AP-PDU>
    <initiatingMessage>
        <procedureCode>13</procedureCode>
        <criticality><ignore/></criticality>
        <value>
            <UplinkNASTransport>
                <protocolIEs>
                    <UplinkNASTransport-IEs>
                        <id>0</id>
                        <criticality><reject/></criticality>
                        <value>
                            <MME-UE-S1AP-ID>553648130</MME-UE-S1AP-ID>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>8</id>
                        <criticality><reject/></criticality>
                        <value>
                            <ENB-UE-S1AP-ID>420141</ENB-UE-S1AP-ID>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>26</id>
                        <criticality><reject/></criticality>
                        <value>
                            <NAS-PDU>
                                17 A8 76 C5 F5 05 07 56 08 29 22 10 10 00 00 11 
                                04
                            </NAS-PDU>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>100</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <EUTRAN-CGI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <cell-ID>
                                    0000000011100000000100000000
                                </cell-ID>
                            </EUTRAN-CGI>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>67</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <TAI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <tAC>00 01</tAC>
                            </TAI>
                        </value>
                    </UplinkNASTransport-IEs>
                </protocolIEs>
            </UplinkNASTransport>
        </value>
    </initiatingMessage>
</S1AP-PDU>
[0m[SCTP]   Successfully sent 68 bytes on stream 1 for assoc_id 903
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   Received notification for sd 86, type 32777
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   [903][86] Msg of length 65 received from port 36412, on stream 1, PPID 18
[0m[0m[RRC]   [eNB 0] Received S1AP_DOWNLINK_NAS: ue_initial_id 1, eNB_ue_s1ap_id 420141
[0m[0m[RRC]   sent RRC_DCCH_DATA_REQ to TASK_PDCP_ENB
[0m[0m[1;31m[PHY]   fill_ulsch UE_id 0 nb_rb = 0
[0m[0m[93m[MAC]   [eNB 0][PUSCH 4] CC_id 0 761.2 ULSCH in error in round 0, ul_cqi 158, UE_id 0, RNTI 43eb (len 63)
[0m[0m[1;31m[PHY]   fill_ulsch UE_id 0 nb_rb = 0
[0m[0m[1;31m[PHY]   fill_ulsch UE_id 0 nb_rb = 0
[0m[0m[MAC]   UE  rnti 43eb : in synch, PHR 40 dB DL CQI 15 PUSCH SNR 10 PUCCH SNR 10
[0m<S1AP-PDU>
    <initiatingMessage>
        <procedureCode>13</procedureCode>
        <criticality><ignore/></criticality>
        <value>
            <UplinkNASTransport>
                <protocolIEs>
                    <UplinkNASTransport-IEs>
                        <id>0</id>
                        <criticality><reject/></criticality>
                        <value>
                            <MME-UE-S1AP-ID>553648130</MME-UE-S1AP-ID>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>8</id>
                        <criticality><reject/></criticality>
                        <value>
                            <ENB-UE-S1AP-ID>420141</ENB-UE-S1AP-ID>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>26</id>
                        <criticality><reject/></criticality>
                        <value>
                            <NAS-PDU>
                                17 9B EE 3B BF 06 07 53 08 ED CA A1 31 56 26 D7 
                                E1
                            </NAS-PDU>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>100</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <EUTRAN-CGI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <cell-ID>
                                    0000000011100000000100000000
                                </cell-ID>
                            </EUTRAN-CGI>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>67</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <TAI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <tAC>00 01</tAC>
                            </TAI>
                        </value>
                    </UplinkNASTransport-IEs>
                </protocolIEs>
            </UplinkNASTransport>
        </value>
    </initiatingMessage>
</S1AP-PDU>
[0m[SCTP]   Successfully sent 68 bytes on stream 1 for assoc_id 903
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   Received notification for sd 86, type 32777
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   [903][86] Msg of length 51 received from port 36412, on stream 1, PPID 18
[0m[0m[RRC]   [eNB 0] Received S1AP_DOWNLINK_NAS: ue_initial_id 1, eNB_ue_s1ap_id 420141
[0m[0m[RRC]   sent RRC_DCCH_DATA_REQ to TASK_PDCP_ENB
[0m<S1AP-PDU>
    <initiatingMessage>
        <procedureCode>13</procedureCode>
        <criticality><ignore/></criticality>
        <value>
            <UplinkNASTransport>
                <protocolIEs>
                    <UplinkNASTransport-IEs>
                        <id>0</id>
                        <criticality><reject/></criticality>
                        <value>
                            <MME-UE-S1AP-ID>553648130</MME-UE-S1AP-ID>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>8</id>
                        <criticality><reject/></criticality>
                        <value>
                            <ENB-UE-S1AP-ID>420141</ENB-UE-S1AP-ID>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>26</id>
                        <criticality><reject/></criticality>
                        <value>
                            <NAS-PDU>47 86 59 47 B7 00 07 5E</NAS-PDU>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>100</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <EUTRAN-CGI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <cell-ID>
                                    0000000011100000000100000000
                                </cell-ID>
                            </EUTRAN-CGI>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>67</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <TAI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <tAC>00 01</tAC>
                            </TAI>
                        </value>
                    </UplinkNASTransport-IEs>
                </protocolIEs>
            </UplinkNASTransport>
        </value>
    </initiatingMessage>
</S1AP-PDU>
[0m[SCTP]   Successfully sent 59 bytes on stream 1 for assoc_id 903
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   Received notification for sd 86, type 32777
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   [903][86] Msg of length 38 received from port 36412, on stream 1, PPID 18
[0m[0m[RRC]   [eNB 0] Received S1AP_DOWNLINK_NAS: ue_initial_id 1, eNB_ue_s1ap_id 420141
[0m[0m[RRC]   sent RRC_DCCH_DATA_REQ to TASK_PDCP_ENB
[0m<S1AP-PDU>
    <initiatingMessage>
        <procedureCode>13</procedureCode>
        <criticality><ignore/></criticality>
        <value>
            <UplinkNASTransport>
                <protocolIEs>
                    <UplinkNASTransport-IEs>
                        <id>0</id>
                        <criticality><reject/></criticality>
                        <value>
                            <MME-UE-S1AP-ID>553648130</MME-UE-S1AP-ID>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>8</id>
                        <criticality><reject/></criticality>
                        <value>
                            <ENB-UE-S1AP-ID>420141</ENB-UE-S1AP-ID>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>26</id>
                        <criticality><reject/></criticality>
                        <value>
                            <NAS-PDU>
                                27 F5 4A 60 81 01 02 1F DA 28 09 03 6F 61 69 04 
                                69 70 76 34
                            </NAS-PDU>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>100</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <EUTRAN-CGI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <cell-ID>
                                    0000000011100000000100000000
                                </cell-ID>
                            </EUTRAN-CGI>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>67</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <TAI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <tAC>00 01</tAC>
                            </TAI>
                        </value>
                    </UplinkNASTransport-IEs>
                </protocolIEs>
            </UplinkNASTransport>
        </value>
    </initiatingMessage>
</S1AP-PDU>
[0m[SCTP]   Successfully sent 71 bytes on stream 1 for assoc_id 903
[0m[0m[1;31m[PHY]   fill_ulsch UE_id 0 nb_rb = 0
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   Received notification for sd 86, type 32777
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   [903][86] Msg of length 235 received from port 36412, on stream 1, PPID 18
[0m[0m[S1AP]   Received NAS message with the E_RAB setup procedure
[0m[0m[RRC]   [eNB 0] Received S1AP_INITIAL_CONTEXT_SETUP_REQ: ue_initial_id 1, eNB_ue_s1ap_id 420141, nb_of_e_rabs 1
[0m[0m[GTPV1U]   Configured GTPu address : c712a8c0
[0m[0m[GTPV1U]   Copied to create_tunnel_resp tunnel: index 0 target gNB ip 192.168.18.199 length 4 gtp teid 3396329693
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 43eb] rrc_eNB_process_GTPV1U_CREATE_TUNNEL_RESP tunnel (3396329693, 3396329693) bearer UE context index 0, msg index 0, id 5, gtp addr len 4 
[0m[0m[RRC]   [eNB 0][UE 43eb] Selected security algorithms (0x7f9f9400213c): 0, 2, changed
[0m[0m[RRC]   [eNB 0][UE 43eb] Saved security key 107FB5D1A79727631F15C38738093134AAF72931EA06D9495605EDB00D8D8044
[0m[0m[RRC]   [0m
KeNB:10 7f b5 d1 a7 97 27 63 1f 15 c3 87 38 09 31 34 aa f7 29 31 ea 06 d9 49 56 05 ed b0 0d 8d 80 44 
[0m[RRC]   [0m
KRRCenc:1b 33 28 35 5a 74 f3 6a 05 c6 cf 34 e9 be 54 63 7b a8 5a 48 1d 72 54 67 ae b0 12 a4 1d 3b 7d 86 
[0m[RRC]   [0m
KRRCint:ba a3 e0 18 79 1e 68 44 c6 60 dd c9 a8 8c 65 c2 e8 74 09 da 28 d6 f2 d9 6f ad da 41 d7 ec 8e 71 
[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 43eb] Logical Channel DL-DCCH, Generate SecurityModeCommand (bytes 3)
[0m[0m[RRC]   calling rrc_data_req :securityModeCommand
[0m[0m[RRC]   sent RRC_DCCH_DATA_REQ to TASK_PDCP_ENB
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 43eb] received securityModeComplete on UL-DCCH 1 from UE
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 43eb] Logical Channel DL-DCCH, Generate UECapabilityEnquiry (bytes 3)
[0m[0m[RRC]   sent RRC_DCCH_DATA_REQ to TASK_PDCP_ENB
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 43eb] received ueCapabilityInformation on UL-DCCH 1 from UE
[0m[0m[RRC]   got UE capabilities for UE 43eb
[0m[0m[93m[RRC]   drx_Configuration parameter is NULL, cannot configure local UE parameters or CDRX is deactivated
[0m[0m[RRC]   [eNB 0] frame 0: requesting A2, A3, A4, and A5 event reporting
[0m<S1AP-PDU>
    <initiatingMessage>
        <procedureCode>22</procedureCode>
        <criticality><ignore/></criticality>
        <value>
            <UECapabilityInfoIndication>
                <protocolIEs>
                    <UECapabilityInfoIndicationIEs>
                        <id>0</id>
                        <criticality><reject/></criticality>
                        <value>
                            <MME-UE-S1AP-ID>553648130</MME-UE-S1AP-ID>
                        </value>
                    </UECapabilityInfoIndicationIEs>
                    <UECapabilityInfoIndicationIEs>
                        <id>8</id>
                        <criticality><reject/></criticality>
                        <value>
                            <ENB-UE-S1AP-ID>420141</ENB-UE-S1AP-ID>
                        </value>
                    </UECapabilityInfoIndicationIEs>
                    <UECapabilityInfoIndicationIEs>
                        <id>74</id>
                        <criticality><reject/></criticality>
                        <value>
                            <UERadioCapability>
                                04 43 DA 01 08 87 7D DB 80 51 81 80 01 04 0C 20 
                                71 63 08 11 24 4C C1 93 67 0F A1 4A 99 3A 85 AF 
                                CC 58 FF FF FF 95 FF EC 7F FF FF CA FF F6 3F FF 
                                FF E5 7F FB 1F FF FF F2 BF FD 8F FF FF F9 5F FE 
                                C7 FF FF FC AF FF 63 FF FF FE 57 FF B1 FF FF FF 
                                2B FF D8 FF FF FF 95 FF EC 7F FF FF CA FF F6 3F 
                                FF FF E5 7F FB 1F FF FF F2 BF FD 8F FF FF F9 5F 
                                FE C7 FF FF FC AF FF 63 FF FF FE 57 FF B1 FF FF 
                                FF 2B FF D8 FF FF FF 95 FF EC 7F FF FF CA FF F6 
                                3F FF FF E5 7F FB 1F FF FF F2 BF FD 8F FF FF F9 
                                5F FE C7 FF FF FC AF FF 63 FF FF FE 57 FF B1 FF 
                                FF FF 2B FF D8 FF FF FF 95 FF DF F3 FF AF A2 0C 
                                00 8C 85 3C 10 65 3A 54 95 1F C0 77 7E 00 00 00 
                                00 02 04 BD 80 00 00 08 09 DF 00 00 00 02 F5 C0 
                                0C 00 A0 04 00 04 00 A0 06 00 48 20 0C 10 06 08 
                                03 04 01 82 00 C1 08 60 84 30 42 18 21 0A 08 03 
                                04 01 82 00 C1 00 60 84 30 42 18 20 0C 10 06 08 
                                03 04 01 82 00 A1 80 01 04 30 00 20 86 00 04 10 
                                C0 00 82 18 00 10 43 00 02 08 40 00 61 00 01 84 
                                00 82 10 00 18 40 08 21 00 01 84 00 82 10 00 18 
                                40 08 21 00 01 84 00 82 10 02 08 60 08 43 0C 01 
                                08 61 80 21 0C 30 04 21 84 00 86 10 02 18 40 08 
                                61 00 21 84 00 86 10 02 18 60 08 43 0C 01 08 61 
                                80 21 0C 30 04 21 84 00 86 10 02 18 40 08 61 00 
                                21 84 00 86 10 02 18 41 08 61 04 21 84 10 86 08 
                                43 04 21 82 10 C1 08 60 04 84 00 86 10 02 18 40 
                                08 61 00 21 84 00 86 10 02 18 21 0C 10 86 10 00 
                                18 40 00 60 80 30 03 00 25 A0 7D 54 6C 1E 00 00 
                                35 81 8C 00 08 20 60 00 02 08 18 20 00 80 06 10 
                                00 20 81 86 00 08 00 62 00 02 00 18 E0 00 80 06 
                                58 00 20 01 98 00 08 00 68 00 02 00 1A 20 00 80 
                                06 90 00 20 01 A6 00 08 00 6C 00 02 00 1B 20 00 
                                80 06 D8 00 20 00 B8 10 00 5F 08 00 70 80 02 00 
                                1C A0 00 82 07 30 00 20 01 CE 00 08 20 74 00 02 
                                08 0D A1 00 0F F0 00 40 05 7C 20 63 00 02 08 3B 
                                60 00 80 8C 10 41 5B 08 18 C0 00 82 0E 98 00 20 
                                23 04 10 54 C2 06 30 00 20 83 8C 00 08 28 41 04 
                                14 60 83 84 00 08 20 E3 00 02 0A 00 41 05 18 20 
                                E0 00 02 08 2B E1 03 00 00 10 01 DB 00 04 04 00 
                                82 0A D8 40 C0 00 04 10 74 C0 01 01 00 20 82 A6 
                                10 30 00 01 04 1C 20 00 41 40 08 20 A1 04 1C 00 
                                00 41 05 7C 20 61 00 02 08 3B 60 00 80 84 10 41 
                                5B 08 18 40 00 82 0E 98 00 20 21 04 10 54 C2 06 
                                10 00 20 82 BE 10 34 C0 01 00 35 F0 81 A6 00 08 
                                08 C1 05 08 20 06 BE 10 14 C2 06 30 00 20 A1 04 
                                00 D7 C2 02 98 40 46 08 38 40 00 80 1A F8 40 D3 
                                00 04 04 60 82 80 10 03 5F 08 0A 61 03 18 00 10 
                                50 02 00 6B E1 01 4C 20 23 04 1C 00 00 40 09 7C 
                                20 69 80 02 02 30 41 09 7C 20 29 84 0C 60 00 41 
                                09 7C 20 63 00 02 0A 10 48 09 7C 20 63 00 02 02 
                                10 49 09 7C 20 23 04 1C 20 00 48 09 7C 20 23 04 
                                0C 20 00 49 09 7C 20 63 00 02 0A 10 40 09 7C 20 
                                63 00 02 02 10 41 09 7C 20 23 04 1C 20 00 40 09 
                                7C 20 23 04 0C 20 00 41 09 7C 20 63 00 02 0A 00 
                                40 09 7C 20 23 04 1C 00 00 40 0F 6C 00 10 11 82 
                                0A 10 41 40 08 21 AD 84 0C 60 00 41 42 08 28 01 
                                04 35 B0 80 8C 10 70 80 01 05 00 20 86 B6 10 11 
                                82 0A 10 41 C0 00 04 10 B6 C0 01 01 18 20 A1 04 
                                10 96 C2 06 30 00 20 A1 04 10 96 C2 02 30 41 C2 
                                00 04 10 B6 C0 01 01 18 20 A0 04 10 96 C2 06 30 
                                00 20 A0 04 10 96 C2 02 30 41 C0 00 04 10 F4 C0 
                                01 01 18 20 A1 04 14 00 82 1A 98 40 C6 00 04 14 
                                20 82 80 10 43 53 08 08 C1 07 08 00 10 50 02 08 
                                6A 61 01 18 20 A1 04 1C 00 00 41 0B 4C 00 10 11 
                                82 0A 10 41 09 4C 20 63 00 02 0A 10 41 09 4C 20 
                                23 04 1C 20 00 41 0B 4C 00 10 11 82 0A 00 41 09 
                                4C 20 63 00 02 0A 00 41 09 4C 20 23 04 1C 00 00 
                                41 0B 18 00 10 50 82 0A 00 41 09 18 20 E1 00 02 
                                0A 00 41 09 18 20 A1 04 1C 00 00 41 07 18 04 12 
                                50 82 08 28 C1 27 08 00 10 41 C6 00 04 14 20 92 
                                0A 30 41 C2 01 04 90 31 80 41 24 25 F0 81 A6 00 
                                08 08 01 00 25 F0 80 A6 10 30 00 01 00 2D B0 00 
                                40 42 08 28 01 04 25 B0 81 84 00 08 28 01 04 25 
                                B0 80 84 10 70 00 01 04 2D 30 00 40 42 08 28 01 
                                04 25 30 81 84 00 08 28 01 04 25 30 80 84 10 70 
                                00 01 04 1C 20 00 41 40 09 20 A1 04 1C 00 00 49 
                                09 7C 20 69 80 02 02 10 41 09 7C 20 29 84 0C 20 
                                00 41 05 7C 20 61 00 02 48 18 40 20 92 07 28 08 
                                24 EB B1 FF FF FF 2B FF D8 FF FF FF 95 FF EC 7F 
                                FF FF CA FF F6 3F FF FF E5 7F FB 1F FF FF F2 BF 
                                FD 8F FF FF F9 5F FE C7 FF FF FC AF FF 63 FF FF 
                                FE 57 FF B1 FF FF FF 2B FF D8 FF FF FF 95 FF EC 
                                7F FF FF CA FF F6 3F FF FF E5 7F FB 1F FF FF F2 
                                BF FD 8F FF FF F9 5F FE C7 FF FF FC AF FF 63 FF 
                                FF FE 57 FF B1 FF FF FF 2B FF D8 FF FF FF 95 FF 
                                EC 7F FF FF CA FF F6 3F FF FF E5 7F FB 1F FF FF 
                                F2 BF FD 8F FF FF F9 5F FE C7 FF FF FC AF FF 63 
                                FF FF FE 57 FF B1 FF FF FF 2B FF D8 FF FF FF 95 
                                FF EC 7F FF FF CA FF F6 3F FF FF E5 7F FB 1F FF 
                                FF F2 BF FD 8F FF FF F9 5F FE C7 FF FF FC AF FF 
                                63 FF FF FE 57 FF B1 FF FF FF 2B FF D8 FF FF FF 
                                95 FF EC 7F FF FF CA FF F6 3F FF FF E5 7F FB 1F 
                                FF FF F2 BF FD 8F FF FF F9 5F FE C7 FF FF FC AF 
                                FF 63 FF FF FE 57 FF B1 FF FF FF 2B FF D8 FF FF 
                                FF 95 FF EC 7F FF FF CA FF F6 3F FF FF E5 7F FB 
                                1F FF FF F2 BF FD 8F FF FF F9 5F FE C7 FF FF FC 
                                AF FF 63 FF FF FE 57 FF B1 FF FF FF 2B FF D8 FF 
                                FF FF 95 FF EC 7F FF FF CA FF F6 3F FF FF E5 7F 
                                FB 1F FF FF F2 BF FD 8F FF FF F9 5F FE C7 FF FF 
                                FC AF FF 63 FF FF FE 57 FF B1 FF FF FF 2B FF D8 
                                FF FF FF 95 FF EC 7F FF FF CA FF F6 3F FF FF E5 
                                7F FB 1F FF FF F2 BF FD 8F FF FF F9 5F FE C7 FF 
                                FF FC AF FF 63 FF FF FE 57 FF B1 FF FF FF 2B FF 
                                D8 FF FF FF 95 FF EC 7F FF FF CA FF F6 3F FF FF 
                                E5 7F FB 1F FF FF F2 BF FD 8F FF FF F9 5F FE C7 
                                FF FF FC AF FF 63 FF FF FE 57 FF B1 FF FF FF 2B 
                                FF D8 FF FF FF 95 FF EC 7F FF FF CA FF F6 3F FF 
                                FF E5 7F FB 1F FF FF F2 BF FD 8F FF FF F9 5F FE 
                                C7 FF FF FC AF FF 63 FF FF FE 57 FF B1 FF FF FF 
                                2B FF D8 FF FF FF 95 FF EC 7F FF FF CA FF F6 3F 
                                FF FF E5 7F FB 1F FF FF F2 BF FD 8F FF FF F9 5F 
                                FE C7 FF FF FC AF FF 63 FF FF FE 57 FF B1 FF FF 
                                FF 2B FF D8 FF FF FF 95 FF EC 7F FF FF CA FF F6 
                                3F FF FF E5 7F FB 1F FF FF F2 BF FD 8F FF FF F9 
                                5F FE C7 FF FF FC AF FF 63 FF FF FE 57 FF B1 FF 
                                FF FF 2B FF D8 FF FF FF 95 FF EC 7F FF FF CA FF 
                                F6 3F FF FF E5 7F FB 1F FF FF F2 BF FD 8F FF FF 
                                F9 5F FE C7 FF FF FC AF FF 63 FF FF FE 57 FF B1 
                                FF FF FF 2B FF D8 FF FF FF 95 FF EC 7F FF FF CA 
                                FF F6 3F FF FF E5 7F F6 CE C0 00 0F D8 81 B3 B0 
                                00 00 8F 9D 80 00 1A C0 00 00 08 78 78 BC 5E 1E 
                                1E 1E 1D 0F 0E 43 C3 A1 E1 E1 E1 E1 C0 00 08 78 
                                78 78 71 17 8B C5 E1 E1 E1 E1 E1 E1 E1 E2 F1 78 
                                BC 3C 3C 3C 3C 39 17 00 01 F5 80 00 00 00 00 00 
                                00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
                                00 00 00 80 82 00 80 20 08 02 00 80 20 08 02 00 
                                80 20 08 02 00 80 20 08 02 00 80 20 08 02 00 80 
                                60 01 80 06 00 18 00 60 01 80 04 00 40 04 00 40 
                                04 00 40 04 00 40 04 00 40 04 00 40 06 00 18 00 
                                60 01 80 04 00 40 04 00 40 04 00 40 06 00 18 00 
                                60 01 80 04 00 40 04 00 40 04 00 40 04 00 40 04 
                                00 20 08 02 00 80 00 40 04 00 40 04 00 40 04 00 
                                40 04 00 20 08 04 00 40 02 00 00 1F 04 01 20 03 
                                E6 57 9A 04 01 4B 1F FF FF FF FF FF FE 69 4B BC 
                                50 0F 80 04 20 09 86 00 00 00 00 00 05 50 92 48 
                                81 01 00 02 F2 42 0B 51 40 01 34 00 00 00
                            </UERadioCapability>
                        </value>
                    </UECapabilityInfoIndicationIEs>
                </protocolIEs>
        [0m[RRC]   RRCConnectionReconfiguration Encoded 1796 bits (225 bytes)
[0m[0m[RRC]   [eNB 0] Frame 0, Logical Channel DL-DCCH, Generate LTE_RRCConnectionReconfiguration (bytes 225, UE id 43eb)
[0m    </UECapabilityInfoIndication>[0m[RRC]   sent RRC_DCCH_DATA_REQ to TASK_PDCP_ENB
[0m
        </value>
    </initiatingMessage>[0m[PDCP]   [FRAME 00000][eNB][MOD 00][RNTI 43eb][SRB 02]  Action ADD  LCID 2 (SRB id 2) configured with SN size 5 bits and RLC AM
[0m
</S1AP-PDU>
[0m[PDCP]   [FRAME 00000][eNB][MOD 00][RNTI 43eb][DRB 01]  Action ADD  LCID 3 (DRB id 1) configured with SN size 12 bits and RLC AM
[0m[0m[SCTP]   Successfully sent 2206 bytes on stream 1 for assoc_id 903
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   Received notification for sd 86, type 32777
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 43eb] UE State = RRC_RECONFIGURED (default DRB, xid 2)
[0m[0m[PDCP]   [FRAME 00000][eNB][MOD 00][RNTI 43eb][SRB 02]  Action MODIFY LCID 2 RB id 2 reconfigured with SN size 5 and RLC AM 
[0m[0m[PDCP]   [FRAME 00000][eNB][MOD 00][RNTI 43eb][DRB 01]  Action MODIFY LCID 3 RB id 1 reconfigured with SN size 1 and RLC AM 
[0m[0m[RRC]   [eNB 0] Frame  0 CC 0 : SRB2 is now active
[0m[0m[RRC]   [eNB 0] Frame  0 : Logical Channel UL-DCCH, Received LTE_RRCConnectionReconfigurationComplete from UE rnti 43eb, reconfiguring DRB 1/LCID 3
[0m[0m[RRC]   [eNB 0] Frame  0 : Logical Channel UL-DCCH, Received LTE_RRCConnectionReconfigurationComplete from UE 0, reconfiguring DRB 1/LCID 3
[0m[0m[MAC]   UE 0 RNTI 43eb adding LC 3 idx 2 to scheduling control (total 3)
[0m[0m[MAC]   Added physicalConfigDedicated 0x7f9f600085d0 for 0.0
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 43eb] Logical Channel DL-DCCH, Generate NR UECapabilityEnquiry (bytes 27)
[0m[0m[RRC]   sent RRC_DCCH_DATA_REQ to TASK_PDCP_ENB
[0m[0m[S1AP]   initial_ctxt_resp_p: e_rab ID 5, enb_addr 192.168.18.199, SIZE 4 
[0m<S1AP-PDU>
    <initiatingMessage>
        <procedureCode>13</procedureCode>
        <criticality><ignore/></criticality>
        <value>
            <UplinkNASTransport>
                <protocolIEs>
                    <UplinkNASTransport-IEs>
                        <id>0</id>
                        <criticality><reject/></criticality>
                        <value>
                            <MME-UE-S1AP-ID>553648130</MME-UE-S1AP-ID>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>8</id>
                        <criticality><reject/></criticality>
                        <value>
                            <ENB-UE-S1AP-ID>420141</ENB-UE-S1AP-ID>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>26</id>
                        <criticality><reject/></criticality>
                        <value>
                            <NAS-PDU>27 22 5C 78 F3 02 07 43 00 03 52 00 C2</NAS-PDU>
                        </value[0m[SCTP]   Successfully sent 43 bytes on stream 1 for assoc_id 903
[0m>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>100</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <EUTRAN-CGI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <cell-ID>
                                    0000000011100000000100000000
                                </cell-ID>
                            </EUTRAN-CGI>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>67</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <TAI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <tAC>00 01</tAC>
                            </TAI>
                        </value>
                    </UplinkNASTransport-IEs>
                </protocolIEs>
            </UplinkNASTransport>
        </value>
    </initiatingMessage>
</S1AP-PDU>
[0m[SCTP]   Successfully sent 64 bytes on stream 1 for assoc_id 903
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 43eb] received ueCapabilityInformation on UL-DCCH 1 from UE
[0m[0m[RRC]   got UE capabilities for UE 43eb
[0m[0m[93m[MAC]   [eNB 0][PUSCH 7] CC_id 0 796.7 ULSCH in error in round 0, ul_cqi 152, UE_id 0, RNTI 43eb (len 63)
[0m[0m[RRC]   [eNB 0] frame 0 subframe 0: UE rnti 43eb switching to NSA mode
[0m[0m[RRC]   Read in 2056 bytes for uecap
[0m<X2AP-PDU>
    <initiatingMessage>
        <procedureCode>27</procedureCode>
        <criticality><reject/></criticality>
        <value>
            <SgNBAdditionRequest>
                <protocolIEs>
                    <SgNBAdditionRequest-IEs>
                        <id>111</id>
                        <criticality><reject/></criticality>
                        <value>
                            <UE-X2AP-ID>0</UE-X2AP-ID>
                        </value>
                    </SgNBAdditionRequest-IEs>
                    <SgNBAdditionRequest-IEs>
                        <id>248</id>
                        <criticality><reject/></criticality>
                        <value>
                            <NRUESecurityCapabilities>
                                <nRencryptionAlgorithms>
                                    0000000000000000
                                </nRencryptionAlgorithms>
                                <nRintegrityProtectionAlgorithms>
                                    0000000000000000
                                </nRintegrityProtectionAlgorithms>
                            </NRUESecurityCapabilities>
                        </value>
                    </SgNBAdditionRequest-IEs>
                    <SgNBAdditionRequest-IEs>
                        <id>203</id>
                        <criticality><reject/></criticality>
                        <value>
                            <SgNBSecurityKey>
                                0000000000000000000000000000000000000000000000000000000000000000
                                0000000000000000000000000000000000000000000000000000000000000000
                                0000000000000000000000000000000000000000000000000000000000000000
                                0000000000000000000000000000000000000000000000000000000000000000
                            </SgNBSecurityKey>
                        </value>
                    </SgNBAdditionRequest-IEs>
                    <SgNBAdditionRequest-IEs>
                        <id>204</id>
                        <criticality><reject/></criticality>
                        <value>
                            <UEAggregateMaximumBitRate>
                                <uEaggregateMaximumBitRateDownlink>100000000</uEaggregateMaximumBitRateDownlink>
                                <uEaggregateMaximumBitRateUplink>100000000</uEaggregateMaximumBitRateUplink>
                            </UEAggregateMaximumBitRate>
                        </value>
                    </SgNBAdditionRequest-IEs>
                    <SgNBAdditionRequest-IEs>
                        <id>205</id>
                        <criticality><reject/></criticality>
                        <value>
                            <E-RABs-ToBeAdded-SgNBAddReqList>
                                <ProtocolIE-Single-Container>
                                    <id>209</id>
                                    <criticality><ignore/></criticality>
                                    <value>
                                        <E-RABs-ToBeAdded-SgNBAddReq-Item>
                                            <e-RAB-ID>5</e-RAB-ID>
                                            <drb-ID>1</drb-ID>
                                            <en-DC-ResourceConfiguration>
                                                <pDCPatSgNB><present/></pDCPatSgNB>
                                                <mCGresources><not-present/></mCGresources>
                                                <sCGresources><not-present/></sCGresources>
                                            </en-DC-ResourceConfiguration>
                                            <resource-configuration>
                                                <sgNBPDCPpresent>
                                                    <full-E-RAB-Level-QoS-Parameters>
                                                        <qCI>1</qCI>
                                                        <allocationAndRetentionPriority>
                                                            <priorityLevel>15</priorityLevel>
                                                            <pre-emptionCapability><shall-not-trigger-pre-emption/></pre-emptionCapability>
                                                            <pre-emptionVulnerability><not-pre-emptable/></pre-emptionVulnerability>
                                                        </allocationAndRetentionPriority>
                                                    </full-E-RAB-Level-QoS-Parameters>
                                                    <s1-UL-GTPtunnelEndpoint>
                                                        <transportLayerAddress>
                                                            11000000101010000001001001100011
                                                        </transportLayerAddress>
                                                        <gTP-TEID>00 00 00 02</gTP-TEID>
                                                    </s1-UL-GTPtunnelEndpoint>
                                                </sgNBPDCPpresent>
                                            </resource-configuration>
                                        </E-RABs-ToBeAdded-SgNBAddReq-Item>
                                    </value>
                                </ProtocolIE-Single-Container>
                            </E-RABs-ToBeAdded-SgNBAddReqList>
                        </value>
                    </SgNBAdditionRequest-IEs>
                    <SgNBAdditionRequest-IEs>
                        <id>206</id>
                        <criticality><reject/></criticality>
                        <value>
                            <MeNBtoSgNBContainer>
                                3A 03 08 78 8D DB 80 51 81 80 01 04 0C 20 71 63 
                                08 11 24 4C C1 93 67 0F A1 4A 99 3A 85 AF CC 58 
                                FF FF FF 95 FF EC 7F FF FF CA FF F6 3F FF FF E5 
                                7F FB 1F FF FF F2 BF FD 8F FF FF F9 5F FE C7 FF 
                                FF FC AF FF 63 FF FF FE 57 FF B1 FF FF FF 2B FF 
                                D8 FF FF FF 95 FF EC 7F FF FF CA FF F6 3F FF FF 
                                E5 7F FB 1F FF FF F2 BF FD 8F FF FF F9 5F FE C7 
                                FF FF FC AF FF 63 FF FF FE 57 FF B1 FF FF FF 2B 
                                FF D8 FF FF FF 95 FF EC 7F FF FF CA FF F6 3F FF 
                                FF E5 7F FB 1F FF FF F2 BF FD 8F FF FF F9 5F FE 
                                C7 FF FF FC AF FF 63 FF FF FE 57 FF B1 FF FF FF 
                                2B FF D8 FF FF FF 95 FF DF F3 FF AF A2 0C 00 8C 
                                85 3C 10 65 3A 54 97 1F C0 68 FE 00 00 00 00 02 
                                04 BD 80 00 00 08 09 DF 00 00 00 02 EE C0 0C 00 
                                A0 04 00 04 00 A0 06 00 48 20 0C 10 06 08 03 04 
                                01 82 10 C1 08 60 84 30 42 18 20 0C 10 06 08 43 
                                04 21 82 00 C1 00 60 80 30 40 18 20 0C 10 06 18 
                                02 10 C3 00 42 18 60 08 43 0C 01 08 61 80 21 0C 
                                30 04 21 86 00 84 30 C0 10 86 10 02 18 40 08 61 
                                00 21 84 00 86 10 02 18 40 08 61 00 21 84 00 86 
                                10 02 18 20 0C 10 06 18 02 10 C3 00 42 18 60 08 
                                43 0C 01 08 61 00 21 84 00 86 10 02 18 41 08 61 
                                04 21 84 10 86 10 42 18 41 08 61 04 21 84 10 86 
                                10 42 18 41 08 60 84 30 42 18 21 0C 10 86 00 61 
                                00 21 84 00 86 10 02 18 40 08 61 00 21 84 00 86 
                                08 43 04 21 82 00 C1 00 60 04 B4 7D 54 6C 1E 00 
                                00 2E 81 8C 00 08 20 60 00 02 08 18 20 00 80 06 
                                10 00 20 81 86 00 08 00 62 00 02 00 18 E0 00 80 
                                06 58 00 20 01 98 00 08 00 68 00 02 00 1A 20 00 
                                80 06 90 00 20 01 A6 00 08 00 6C 00 02 00 1B 20 
                                00 80 06 D8 00 20 00 B8 10 00 5F 08 00 70 80 02 
                                00 1C A0 00 82 07 30 00 20 01 CE 00 08 20 74 00 
                                02 08 0D A1 00 0F F0 00 40 07 4C 00 10 11 82 08 
                                2A 61 03 18 00 10 41 C7 00 04 04 60 82 0A 38 40 
                                C6 00 04 10 71 80 01 05 08 20 82 8C 10 70 80 01 
                                04 1C 60 00 41 40 08 20 A3 04 1C 00 00 41 07 4C 
                                00 10 10 02 08 2A 61 03 00 00 10 41 C2 00 04 14 
                                00 82 0A 10 41 C0 00 04 10 76 C0 01 01 08 20 82 
                                B6 10 30 80 01 04 1D 30 00 40 42 08 20 A9 84 0C 
                                20 00 41 07 1C 00 10 10 82 08 28 E1 03 08 00 10 
                                43 D3 00 04 04 60 82 84 12 50 02 08 6A 61 03 18 
                                00 10 50 82 4A 00 41 0D 4C 20 23 04 1C 20 00 49 
                                40 08 21 A9 84 04 60 82 84 12 70 00 01 04 3D 30 
                                00 40 46 08 28 41 05 00 20 86 A6 10 31 80 01 05 
                                08 20 A0 04 10 D4 C2 02 30 41 C2 00 04 14 00 82 
                                1A 98 40 46 08 28 41 07 00 00 10 42 D3 00 04 04 
                                60 82 84 12 42 53 08 18 C0 00 82 84 12 42 53 08 
                                08 C1 07 08 00 12 42 D3 00 04 04 60 82 84 10 42 
                                53 08 18 C0 00 82 84 10 42 53 08 08 C1 07 08 00 
                                10 42 D3 00 04 04 60 82 80 10 42 53 08 18 C0 00 
                                82 80 10 42 53 08 08 C1 07 00 00 10 41 D3 00 04 
                                04 60 92 0A 98 40 C6 00 04 90 F1 C0 01 01 18 20 
                                A1 04 14 00 82 1A 38 40 C6 00 04 14 20 82 80 10 
                                43 47 08 08 C1 07 08 00 10 50 02 08 68 E1 01 18 
                                20 A1 04 1C 00 00 41 0B 1C 00 10 11 82 0A 10 41 
                                09 1C 20 63 00 02 0A 10 41 09 1C 20 23 04 1C 20 
                                00 41 0B 18 00 12 50 82 0A 00 41 09 18 24 E1 00 
                                02 0A 00 41 09 18 24 A1 04 1C 00 00 41 0B 18 00 
                                10 50 82 4A 00 41 09 18 20 E1 00 02 4A 00 41 09 
                                18 20 A1 04 9C 00 00 41 0B 18 00 10 50 82 0A 00 
                                41 09 18 20 E1 00 02 0A 00 41 09 18 20 A1 04 1C 
                                00 00 41 07 18 04 12 50 82 08 28 C1 27 08 00 10 
                                41 C6 00 04 14 20 92 0A 30 41 C2 01 04 90 31 80 
                                41 24 2D 30 00 40 42 09 28 01 04 25 30 81 84 00 
                                09 28 01 04 25 30 80 84 12 70 00 01 04 2D 30 00 
                                40 42 08 28 01 04 25 30 81 84 00 08 28 01 04 25 
                                30 80 84 10 70 00 01 04 1C 20 10 49 40 08 20 A1 
                                04 9C 00 00 41 07 4C 00 10 10 82 48 2A 61 03 08 
                                00 12 40 C2 01 04 9B B6 3F FF FF E5 7F FB 1F FF 
                                FF F2 BF FD 8F FF FF F9 5F FE C7 FF FF FC AF FF 
                                63 FF FF FE 57 FF B1 FF FF FF 2B FF D8 FF FF FF 
                                95 FF EC 7F FF FF CA FF F6 3F FF FF E5 7F FB 1F 
                                FF FF F2 BF FD 8F FF FF F9 5F FE C7 FF FF FC AF 
                                FF 63 FF FF FE 57 FF B1 FF FF FF 2B FF D8 FF FF 
                                FF 95 FF EC 7F FF FF CA FF F6 3F FF FF E5 7F FB 
                                1F FF FF F2 BF FD 8F FF FF F9 5F FE C7 FF FF FC 
                                AF FF 63 FF FF FE 57 FF B1 FF FF FF 2B FF D8 FF 
                                FF FF 95 FF EC 7F FF FF CA FF F6 3F FF FF E5 7F 
                                FB 1F FF FF F2 BF FD 8F FF FF F9 5F FE C7 FF FF 
                                FC AF FF 63 FF FF FE 57 FF B1 FF FF FF 2B FF D8 
                                FF FF FF 95 FF EC 7F FF FF CA FF F6 3F FF FF E5 
                                7F FB 1F FF FF F2 BF FD 8F FF FF F9 5F FE C7 FF 
                                FF FC AF FF 63 FF FF FE 57 FF B1 FF FF FF 2B FF 
                                D8 FF FF FF 95 FF EC 7F FF FF CA FF F6 3F FF FF 
                                E5 7F FB 1F FF FF F2 BF FD 8F FF FF F9 5F FE C7 
                                FF FF FC AF FF 63 FF FF FE 57 FF B1 FF FF FF 2B 
                                FF D8 FF FF FF 95 FF EC 7F FF FF CA FF F6 3F FF 
                                FF E5 7F FB 1F FF FF F2 BF FD 8F FF FF F9 5F FE 
                                C7 FF FF FC AF FF 63 FF FF FE 57 FF B1 FF FF FF 
                                2B FF D8 FF FF FF 95 FF EC 7F FF FF CA FF F6 3F 
                                FF FF E5 7F FB 1F FF FF F2 BF FD 8F FF FF F9 5F 
                                FE C7 FF FF FC AF FF 63 FF FF FE 57 FF B1 FF FF 
                                FF 2B FF D8 FF FF FF 95 FF EC 7F FF FF CA FF F6 
                                3F FF FF E5 7F FB 1F FF FF F2 BF FD 8F FF FF F9 
                                5F FE C7 FF FF FC AF FF 63 FF FF FE 57 FF B1 FF 
                                FF FF 2B FF D8 FF FF FF 95 FF EC 7F FF FF CA FF 
                                F6 3F FF FF E5 7F FB 1F FF FF F2 BF FD 8F FF FF 
                                F9 5F FE C7 FF FF FC AF FF 63 FF FF FE 57 FF B1 
                                FF FF FF 2B FF D8 FF FF FF 95 FF EC 7F FF FF CA 
                                FF F6 3F FF FF E5 7F FB 1F FF FF F2 BF FD 8F FF 
                                FF F9 5F FE C7 FF FF FC AF FF 63 FF FF FE 57 FF 
                                B1 FF FF FF 2B FF D8 FF FF FF 95 FF EC 7F FF FF 
                                CA FF F6 3F FF FF E5 7F FB 1F FF FF F2 BF FD 8F 
                                FF FF F9 5F FE C7 FF FF FC AF FF 63 FF FF FE 57 
                                FF B1 FF FF FF 2B FF B6 76 00 00 7E C4 0D 9D 80 
                                00 04 7C EC 00 00 BA 00 00 00 8B C5 E2 F1 78 78 
                                78 78 72 1E 1E 1E 1E 1E 1E 3F 8F C2 1E 1E 1E 1E 
                                1E 1E 1E 1E 1E 1E 2F 17 8B 90 F0 F0 F0 F1 78 BC 
                                5E 1E 1E 1E 1E 1E 1E 1E 1E 1E 1E 1C 8B 80 0F 74 
                                00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
                                00 00 00 00 00 00 00 00 04 04 10 04 01 00 40 10 
                                04 01 00 40 10 04 01 00 40 10 04 01 00 40 10 04 
                                03 00 0C 00 30 00 C0 03 00 0C 00 30 00 C0 02 00 
                                20 02 00 20 02 00 20 02 00 20 02 00 10 04 03 00 
                                0C 00 30 00 C0 02 00 20 02 00 20 02 00 20 02 00 
                                20 02 00 20 02 00 20 01 00 40 10 04 00 02 00 20 
                                02 00 20 02 00 20 01 00 40 10 04 00 3E 08 02 40 
                                07 CC AF 34 08 02 96 3F FF FF FF FF FF FC D2 97 
                                78 A0 1F 00 08 40 13 0C 00 00 00 00 00 0A A1 34 
                                91 02 02 00 05 E4 84 12 E2 80 02 6B C0 C0 04 00 
                                01 04 10 40 00 28 C8 00 00 08 80 00 05 58 E1 00 
                                00 00 01 4F 7E 03 02 00 00 01 40 48 07 06 0E 22 
                                0C 00 02 13 60 10 73 E4 20 F0 00 82 40 31 10 00 
                                A0 58 9B A0 21 94 34 08 81 07 41 86 04 C0 42 54 
                                41 01 00 80 06 08 1C 1C 22 03 C8 0F 00 20 1A 02 
                                6E 26 F0 00 09 00 00 00 00 72 A6 80 00 80 00 02 
                                0C 30 00 1A 55 30 62 00 11 C0 48 16 0C 01 C4 D0 
                                00 00 00 40 04 03 40 4D 01 04 40 41 4E 9C 00 02 
                                00 01 00 80 80 10 02 00
                            </MeNBtoSgNBContainer>
                        </value>
                    </SgNBAdditionRequest-IEs>
                </protocolIEs>
            </SgNBAdditionRequest>
        </value>
    </initiatingMessage>
</X2AP-PDU>
[0m[SCTP]   Successfully sent 2161 bytes on stream 0 for assoc_id 904
[0m[0m[SCTP]   Found data for descriptor 95
[0m[0m[SCTP]   Received notification for sd 95, type 32777
[0m[0m[SCTP]   Found data for descriptor 95
[0m[0m[SCTP]   [904][95] Msg of length 371 received from port 36422, on stream 0, PPID 27
[0m<X2AP-PDU>
    <successfulOutcome>
        <procedureCode>27</procedureCode>
        <criticality><reject/></criticality>
        <value>
            <SgNBAdditionRequestAcknowledge>
                <protocolIEs>
                    <SgNBAdditionRequestAcknowledge-IEs>
                        <id>111</id>
                        <criticality><reject/></criticality>
                        <value>
                            <UE-X2AP-ID>0</UE-X2AP-ID>
                        </value>
                    </SgNBAdditionRequestAcknowledge-IEs>
                    <SgNBAdditionRequestAcknowledge-IEs>
                        <id>207</id>
                        <criticality><reject/></criticality>
                        <value>
                            <SgNB-UE-X2AP-ID>0</SgNB-UE-X2AP-ID>
                        </value>
                    </SgNBAdditionRequestAcknowledge-IEs>
                    <SgNBAdditionRequestAcknowledge-IEs>
                        <id>210</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <E-RABs-Admitted-ToBeAdded-SgNBAddReqAckList>
                                <ProtocolIE-Single-Container>
                                    <id>213</id>
                                    <criticality><ignore/></criticality>
                                    <value>
                                        <E-RABs-Admitted-ToBeAdded-SgNBAddReqAck-Item>
                                            <e-RAB-ID>5</e-RAB-ID>
                                            <en-DC-ResourceConfiguration>
                                                <pDCPatSgNB><present/></pDCPatSgNB>
                                                <mCGresources><not-present/></mCGresources>
                                                <sCGresources><not-present/></sCGresources>
                                            </en-DC-ResourceConfiguration>
                                            <resource-configuration>
                                                <sgNBPDCPpresent>
                                                    <s1-DL-GTPtunnelEndpoint>
                                                        <transportLayerAddress>
                                                            11000000101010000001001011000110
                                                        </transportLayerAddress>
                                                        <gTP-TEID>92 CC 30 02</gTP-TEID>
                                                    </s1-DL-GTPtunnelEndpoint>
                                                </sgNBPDCPpresent>
                                            </resource-configuration>
                                        </E-RABs-Admitted-ToBeAdded-SgNBAddReqAck-Item>
                                    </value>
                                </ProtocolIE-Single-Container>
                            </E-RABs-Admitted-ToBeAdded-SgNBAddReqAckList>
                        </value>
                    </SgNBAdditionRequestAcknowledge-IEs>
                    <SgNBAdditionRequestAcknowledge-IEs>
                        <id>211</id>
                        <criticality><reject/></criticality>
                        <value>
                            <SgNBtoMeNBContainer>
                                18 04 09 A8 44 09 92 E2 07 8E 01 90 43 7E 30 D0 
                                41 E6 41 C8 54 1E 21 00 83 2B A1 6E 63 00 1A 4E 
                                47 C0 13 49 C4 00 00 00 26 96 18 DE 35 00 05 38 
                                05 10 0D 60 1B 40 39 D2 02 68 00 01 34 E4 E1 8D 
                                E3 2A 31 00 0D 66 66 BE E4 E0 24 BC A1 5B C2 C5 
                                8F 68 9C 2E 00 50 E0 18 04 21 60 3B 00 91 19 1F 
                                5E 24 62 00 1A CC CD 00 03 F0 DB 00 10 1C 02 D9 
                                00 92 00 20 24 04 63 2C E1 96 65 14 0F FF F8 00 
                                00 00 08 70 00 41 03 08 14 30 73 70 44 30 00 00 
                                80 80 1A 70 0A 20 1A C0 36 80 72 CA 80 40 FF FF 
                                80 00 00 00 87 00 04 10 30 81 43 07 0D C2 10 C0 
                                00 08 05 90 01 01 20 23 25 61 52 C0 E1 04 16 0E 
                                0C 10 E1 00 71 28 1C 00 00 20 5E F4 01 00 02 00 
                                00 0F 40 01 41 00 19 73 86 59 95 18 80 06 B3 33 
                                5F 72 70 12 5E 50 AD E1 62 C7 B4 4E 17 00 28 70 
                                6A A4 1A 80 81 04 42 0C 20 30 08 C0 03 40 43 00 
                                0C 01 8A 17 B4 08 28 5E C9 07 91 A2 B3 80 00 40 
                                00 7F 42 10 84 00 80 40 25 81 C2 08 2C 1C 18 21 
                                C2 00 E2 50 38 00 00 40 BD E8 02 00 04 00 00 1E 
                                80 02 82 00 70 01 01 88 00 40 A0 49 40 BC 16 00 
                                60 00
                            </SgNBtoMeNBContainer>
                        </value>
                    </SgNBAdditionRequestAcknowledge-IEs>
                </protocolIEs>
            </SgNBAdditionRequestAcknowledge>
        </value>
    </successfulOutcome>
</X2AP-PDU>
[0m[X2AP]   x2ap_eNB_decode_successfuloutcome_message!
[0m[0m[X2AP]   X2AP Association id: 904 
[0m322:  
<CG-Config>
    <criticalExtensions>
        <c1>
            <cg-Config>
                <scg-CellGroupConfig>
                    08 81 32 5C 40 F1 C0 32 08 6F C6 1A 08 3C C8 39 
                    0A 83 C4 20 10 65 74 2D CC 60 03 49 C8 F8 02 69 
                    38 80 00 00 04 D2 C3 1B C6 A0 00 A7 00 A2 01 AC 
                    03 68 07 3A 40 4D 00 00 26 9C 9C 31 BC 65 46 20 
                    01 AC CC D7 DC 9C 04 97 94 2B 78 58 B1 ED 13 85 
                    C0 0A 1C 03 00 84 2C 07 60 12 23 23 EB C4 8C 40 
                    03 59 99 A0 00 7E 1B 60 02 03 80 5B 20 12 40 04 
                    04 80 8C 65 9C 32 CC A2 81 FF FF 00 00 00 01 0E 
                    00 08 20 61 02 86 0E 6E 08 86 00 00 10 10 03 4E 
                    01 44 03 58 06 D0 0E 59 50 08 1F FF F0 00 00 00 
                    10 E0 00 82 06 10 28 60 E1 B8 42 18 00 01 00 B2 
                    00 20 24 04 64 AC 2A 58 1C 20 82 C1 C1 82 1C 20 
                    0E 25 03 80 00 04 0B DE 80 20 00 40 00 01 E8 00 
                    28 20 03 2E 70 CB 32 A3 10 00 D6 66 6B EE 4E 02 
                    4B CA 15 BC 2C 58 F6 89 C2 E0 05 0E 0D 54 83 50 
                    10 20 88 41 84 06 01 18 00 68 08 60 01 80 31 42 
                    F6 81 05 0B D9 20 F2 34 56 70 00 08 00 0F E8 42 
                    10 80 10 08 04 B0 38 41 05 83 83 04 38 40 1C 4A 
                    07 00 00 08 17 BD 00 40 00 80 00 03 D0 00 50 40 
                    0E 00 20 31 00
                </scg-CellGroupConfig>
                <scg-RB-Config>14 09 28 17 82 C0 0C 00</scg-RB-Config>
            </cg-Config>
        </c1>
    </criticalExtensions>
</CG-Config>
[0m[RRC]   Dumping scg_CellGroupConfig: 309[ 
[0m[RRC]   Dumping scg_RB_Config: 8[0m1409281782c00c00
[0m[RRC]   Dumping nr_SecondaryCellGroupConfig: 309[ 
[0m[RRC]   Dumping nr_RadioBearerConfig1: 8[0m1409281782c00c00
len = 336
 22 02 8c 00 23 08 10 00 ac 24 a0 82 1e 32 04 d4 22 04 c9 71 03 c7 00 c8 21 bf 18 68 20 f3 20 e4 2a 0f 10 80 41 95 d0 b7 31 80 0d 27 23 e0 09 a4 e2 00 00 00 13 4b 0c 6f 1a 80 02 9c 02 88 06 b0 0d a0 1c e9 01 34 00 00 9a 72 70 c6 f1 95 18 80 06 b3 33 5f 72 70 12 5e 50 ad e1 62 c7 b4 4e 17 00 28 70 0c 02 10 b0 1d 80 48 8c 8f af 12 31 00 0d 66 66 80 01 f8 6d 80 08 0e 01 6c 80 49 00 10 12 02 31 96 70 cb 32 8a 07 ff fc 00 00 00 04 38 00 20 81 84 0a 18 39 b8 22 18 00 00 40 40 0d 38 05 10 0d 60 1b 40 39 65 40 20 7f ff c0 00 00 00 43 80 02 08 18 40 a1 83 86 e1 08 60 00 04 02 c8 00 80 90 11 92 b0 a9 60 70 82 0b 07 06 08 70 80 38 94 0e 00 00 10 2f 7a 00 80 01 00 00 07 a0 00 a0 80 0c b9 c3 2c ca 8c 40 03 59 99 af b9 38 09 2f 28 56 f0 b1 63 da 27 0b 80 14 38 35 52 0d 40 40 82 21 06 10 18 04 60 01 a0 21 80 06 00 c5 0b da 04 14 2f 64 83 c8 d1 59 c0 00 20 00 3f a1 08 42 00 40 20 12 c0 e1 04 16 0e 0c 10 e1 00 71 28 1c 00 00 20 5e f4 01 00 02 00 00 0f 40 01 41 00 38 00 80 c4 00 00 00 20 50 24 a0 5e 0b 00 30 00
[0m[RRC]   sent RRC_DCCH_DATA_REQ to TASK_PDCP_ENB
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 43eb] UE State = RRC_RECONFIGURED (default DRB, xid 1)
[0m[0m[RRC]   E-RAB modification indication: nb nb_of_e_rabs 1 status 4
[0m[0m[RRC]   S1AP_E_RAB_MODIFICATION_IND: sending the message: nb_of_erabstobemodified 1, total e_rabs 1, index 1
[0m<S1AP-PDU>
    <initiatingMessage>
        <procedureCode>50</procedureCode>
        <criticality><reject/></criticality>
        <value>
            <E-RABModificationIndication>
                <protocolIEs>
                    <E-RABModificationIndicationIEs>
                        <id>0</id>
                        <criticality><reject/></criticality>
                        <value>
                            <MME-UE-S1AP-ID>553648130</MME-UE-S1AP-ID>
                        </value>
                    </E-RABModificationIndicationIEs>
                    <E-RABModificationIndicationIEs>
                        <id>8</id>
                        <criticality><reject/></criticality>
                        <value>
                            <ENB-UE-S1AP-ID>420141</ENB-UE-S1AP-ID>
                        </value>
                    </E-RABModificationIndicationIEs>
                    <E-RABModificationIndicationIEs>
                        <id>199</id>
                        <criticality><reject/></criticality>
                        <value>
                            <E-RABToBeModifiedListBearerModInd>
                                <ProtocolIE-SingleContainer>
                                    <id>200</id>
                                    <criticality><reject/></criticality>
                                    <value>
                                        <E-RABToBeModifiedItemBearerModInd>
                                            <e-RAB-ID>5</e-RAB-ID>
                                            <transportLayerAddress>
                                                11000000101010000001001011000110
                                            </transportLayerAddress>
                                            <dL-GTP-TEID>92 CC 30 02</dL-GTP-TEID>
                                        </E-RABToBeModifiedItemBearerModInd>
                                    </value>
                                </ProtocolIE-SingleContainer>
                            </E-RABToBeModifiedListBearerModInd>
                        </value>
                    </E-RABModificationIndicationIEs>
                </protocolIEs>
            </E-RABModificationIndication>
        </value>
    </initiatingMessage>
</S1AP-PDU>
[0m[S1AP]   Size of encoded message: 43 
[0m[0m[S1AP]   initial context setup response: failed e_rab ID 5
[0m[0m[SCTP]   Successfully sent 43 bytes on stream 1 for assoc_id 903
[0m[0m[1;31m[SCTP]   Sctp_sendmsg failed: Message too long
[0m[0m[GTPV1U]   NW_GTP_END_MARKER
[0m[0m[93m[PDCP]   Handed SDU is of size 0! Ignoring...
[0m[0m[93m[GTPV1U]   PDCP data request failed, cause: [UE:43eb]RB is not configured!
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   Received notification for sd 86, type 32777
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   [903][86] Msg of length 34 received from port 36412, on stream 1, PPID 18
[0m[0m[93m[S1AP]   Implementation of S1AP E-RAB Modification confirm handler is pending...
[0m[0m[93m[MAC]   [eNB 0][PUSCH 1] CC_id 0 874.5 ULSCH in error in round 0, ul_cqi 158, UE_id 0, RNTI 43eb (len 63)
[0m[0m[MAC]   UE  rnti 43eb : in synch, PHR 40 dB DL CQI 15 PUSCH SNR 18 PUCCH SNR 15
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[MAC]   UE  rnti 43eb : in synch, PHR 40 dB DL CQI 15 PUSCH SNR 15 PUCCH SNR 16
[0m[0m[RRC]   UE rnti 43eb failure timer 0/8
[0m[0m[PHY]   prach_I0 = 0.0 dB
[0m[0m[PHY]   max_I0 19, min_I0 12
[0m[0m[93m[MAC]   [eNB 0][PUSCH 4] CC_id 0 73.2 ULSCH in error in round 0, ul_cqi 159, UE_id 0, RNTI 43eb (len 63)
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[93m[MAC]   [eNB 0][PUSCH 7] CC_id 0 114.3 ULSCH in error in round 0, ul_cqi 165, UE_id 0, RNTI 43eb (len 63)
[0m[0m[MAC]   UE  rnti 43eb : in synch, PHR 40 dB DL CQI 15 PUSCH SNR 13 PUCCH SNR 10
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 218.4 ULSCH in error in round 0, ul_cqi 158, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 6] CC_id 0 226.2 ULSCH in error in round 0, ul_cqi 164, UE_id 0, RNTI 43eb (len 63)
[0m[0m[MAC]   UE  rnti 43eb : in synch, PHR 40 dB DL CQI 15 PUSCH SNR 13 PUCCH SNR 13
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[MAC]   UE  rnti 43eb : in synch, PHR 40 dB DL CQI 15 PUSCH SNR 19 PUCCH SNR 15
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[MAC]   UE  rnti 43eb : in synch, PHR 40 dB DL CQI 15 PUSCH SNR 18 PUCCH SNR 13
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[MAC]   UE  rnti 43eb : in synch, PHR 40 dB DL CQI 15 PUSCH SNR 13 PUCCH SNR 15
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[93m[MAC]   [eNB 0][PUSCH 2] CC_id 0 753.0 ULSCH in error in round 0, ul_cqi 164, UE_id 0, RNTI 43eb (len 63)
[0m[0m[MAC]   UE  rnti 43eb : in synch, PHR 40 dB DL CQI 15 PUSCH SNR 18 PUCCH SNR 15
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[MAC]   UE  rnti 43eb : in synch, PHR 40 dB DL CQI 15 PUSCH SNR 15 PUCCH SNR 16
[0m<S1AP-PDU>
    <initiatingMessage>
        <procedureCode>13</procedureCode>
        <criticality><ignore/></criticality>
        <value>
            <UplinkNASTransport>
                <protocolIEs>
                    <UplinkNASTransport-IEs>
                        <id>0</id>
                        <criticality><reject/></criticality>
                        <value>
                            <MME-UE-S1AP-ID>553648130</MME-UE-S1AP-ID>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>8</id>
                        <criticality><reject/></criticality>
                        <value>
                            <ENB-UE-S1AP-ID>420141</ENB-UE-S1AP-ID>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>26</id>
                        <criticality><reject/></criticality>
                        <value>
                            <NAS-PDU>
                                27 D6 DB 4F 5E 03 07 45 0B 0B F6 22 F2 10 80 00 
                                01 00 00 00 37
                            </NAS-PDU>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>100</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <EUTRAN-CGI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <cell-ID>
                                    0000000011100000000100000000
                                </cell-ID>
                            </EUTRAN-CGI>
                        </value>
                    </UplinkNASTransport-IEs>
                    <UplinkNASTransport-IEs>
                        <id>67</id>
                        <criticality><ignore/></criticality>
                        <value>
                            <TAI>
                                <pLMNidentity>22 F2 10</pLMNidentity>
                                <tAC>00 01</tAC>
                            </TAI>
                        </value>
                    </UplinkNASTransport-IEs>
                </protocolIEs>
            </UplinkNASTransport>
        </value>
    </initiatingMessage>
</S1AP-PDU>
[0m[SCTP]   Successfully sent 72 bytes on stream 1 for assoc_id 903
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   Received notification for sd 86, type 32777
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   [903][86] Msg of length 25 received from port 36412, on stream 1, PPID 18
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 43eb] Logical Channel DL-DCCH, Generate RRCConnectionRelease (bytes 3)
[0m[0m[RRC]   sent RRC_DCCH_DATA_REQ to TASK_PDCP_ENB
[0m[0m[93m[MAC]   [eNB 0][PUSCH 3] CC_id 0 927.5 ULSCH in error in round 0, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 3] CC_id 0 928.3 ULSCH in error in round 1, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 3] CC_id 0 929.1 ULSCH in error in round 2, ul_cqi 112, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 3] CC_id 0 929.9 ULSCH in error in round 3, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 3] CC_id 0 930.7 ULSCH in error in round 0, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 3] CC_id 0 931.5 ULSCH in error in round 1, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 3] CC_id 0 932.3 ULSCH in error in round 2, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 3] CC_id 0 933.1 ULSCH in error in round 3, ul_cqi 128, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 3] CC_id 0 933.9 ULSCH in error in round 0, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 3] CC_id 0 934.7 ULSCH in error in round 1, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 3] CC_id 0 935.5 ULSCH in error in round 2, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 3] CC_id 0 936.3 ULSCH in error in round 3, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 936.8 ULSCH in error in round 0, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 937.6 ULSCH in error in round 1, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 938.4 ULSCH in error in round 2, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 939.2 ULSCH in error in round 3, ul_cqi 112, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 940.0 ULSCH in error in round 0, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 940.8 ULSCH in error in round 1, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 941.6 ULSCH in error in round 2, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 942.4 ULSCH in error in round 3, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 943.2 ULSCH in error in round 0, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 944.0 ULSCH in error in round 1, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 944.8 ULSCH in error in round 2, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 945.6 ULSCH in error in round 3, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 946.4 ULSCH in error in round 0, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 947.2 ULSCH in error in round 1, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 948.0 ULSCH in error in round 2, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 948.8 ULSCH in error in round 3, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 949.6 ULSCH in error in round 0, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 950.4 ULSCH in error in round 1, ul_cqi 112, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 951.2 ULSCH in error in round 2, ul_cqi 112, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 952.0 ULSCH in error in round 3, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 952.8 ULSCH in error in round 0, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 953.6 ULSCH in error in round 1, ul_cqi 112, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 954.4 ULSCH in error in round 2, ul_cqi 112, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 955.2 ULSCH in error in round 3, ul_cqi 112, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 956.0 ULSCH in error in round 0, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 956.8 ULSCH in error in round 1, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 957.6 ULSCH in error in round 2, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 958.4 ULSCH in error in round 3, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 959.2 ULSCH in error in round 0, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 960.0 ULSCH in error in round 1, ul_cqi 112, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 960.8 ULSCH in error in round 2, ul_cqi 122, UE_id 0, RNTI 43eb (len 63)
[0m[0m[93m[MAC]   [eNB 0][PUSCH 0] CC_id 0 961.6 ULSCH in error in round 3, ul_cqi 116, UE_id 0, RNTI 43eb (len 63)
[0m[0m[MAC]   UE 0 rnti 43eb: UL Failure timer 1 
[0m[0m[93m[RRC]   S1AP removed entry in hashtable s1ap_id2_s1ap_ids for eNB_ue_s1ap_id 420141
[0m[0m[93m[RRC]   S1AP removed entry in hashtable initial_id2_s1ap_ids for ue_initial_id 1
[0m[0m[93m[S1AP]   Removed UE context eNB_ue_s1ap_id 420141
[0m[0m[SCTP]   Successfully sent 24 bytes on stream 1 for assoc_id 903
[0m[0m[RRC]   Removing UE 43eb instance after UE_CONTEXT_RELEASE_Complete (ue_release_timer_rrc timeout)
[0m[0m[93m[RRC]   [eNB 0] Removing UE RNTI 43eb
[0m[0m[RRC]   Put UE 43eb into freeList
[0m[0m[RRC]   clean_eNb_dlsch dlsch[2] UE 43eb 
[0m[0m[MAC]   clean eNb uci_vars[0] UE 43eb 
[0m[0m[MAC]   clean eNb uci_vars[1] UE 43eb 
[0m[0m[MAC]   clean eNb uci_vars[2] UE 43eb 
[0m[0m[MAC]   clean eNb uci_vars[3] UE 43eb 
[0m[0m[RRC]   remove UE 43eb from ul_config_pdu_list 0/1
[0m[0m[MAC]   Removing UE 0 from Primary CC_id 0 (rnti 43eb)
[0m[0m[PDCP]   remove uid is 0/0 43eb
[0m[0m[RRC]   [FRAME 00000][eNB][MOD 00][RNTI 43eb] Removed UE context
[0m[0m[RRC]   [release_UE_in_freeList] remove UE 43eb from freeList
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[SCTP]   Found data for descriptor 86
[0m[0m[SCTP]   Received notification for sd 86, type 32777
[0m[0m[PHY]   prach_I0 = 0.0 dB
[0m[0m[PHY]   max_I0 18, min_I0 12
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m[0m[X2AP]   X2 has 1 process ongoing
[0m