
EUTRA-RRC-Definitions DEFINITIONS AUTOMATIC TAGS ::=

BEGIN


BCCH-BCH-Message ::= SEQUENCE {
	message					BCCH-BCH-MessageType
}

BCCH-BCH-MessageType ::=						MasterInformationBlock


BCCH-DL-SCH-Message ::= SEQUENCE {
	message					BCCH-DL-SCH-MessageType
}

BCCH-DL-SCH-MessageType ::= CHOICE {
	c1						CHOICE {
		systemInformation						SystemInformation,
		systemInformationBlockType1				SystemInformationBlockType1
	},
	messageClassExtension	SEQUENCE {}
}


MCCH-Message ::= 		SEQUENCE {
	message					MCCH-MessageType
}

MCCH-MessageType ::= CHOICE {
	c1							CHOICE {
		mbsfnAreaConfiguration-r9		MBSFNAreaConfiguration-r9
	},
	messageClassExtension	SEQUENCE {}
}


PCCH-Message ::= SEQUENCE {
	message					PCCH-MessageType
}

PCCH-MessageType ::= CHOICE {
	c1						CHOICE {
		paging									Paging
	},
	messageClassExtension	SEQUENCE {}
}


DL-CCCH-Message ::= SEQUENCE {
	message					DL-CCCH-MessageType
}

DL-CCCH-MessageType ::= CHOICE {
	c1						CHOICE {
		rrcConnectionReestablishment			RRCConnectionReestablishment,
		rrcConnectionReestablishmentReject		RRCConnectionReestablishmentReject,
		rrcConnectionReject						RRCConnectionReject,
		rrcConnectionSetup						RRCConnectionSetup
	},
	messageClassExtension	SEQUENCE {}
}


DL-DCCH-Message ::= SEQUENCE {
	message					DL-DCCH-MessageType
}

DL-DCCH-MessageType ::= CHOICE {
	c1						CHOICE {
		csfbParametersResponseCDMA2000			CSFBParametersResponseCDMA2000,
		dlInformationTransfer					DLInformationTransfer,
		handoverFromEUTRAPreparationRequest		HandoverFromEUTRAPreparationRequest,
		mobilityFromEUTRACommand				MobilityFromEUTRACommand,
		rrcConnectionReconfiguration			RRCConnectionReconfiguration,
		rrcConnectionRelease					RRCConnectionRelease,
		securityModeCommand						SecurityModeCommand,
		ueCapabilityEnquiry						UECapabilityEnquiry,
		counterCheck							CounterCheck,
		ueInformationRequest-r9					UEInformationRequest-r9,
		spare6 NULL, spare5 NULL, spare4 NULL,
		spare3 NULL, spare2 NULL, spare1 NULL
	},
	messageClassExtension	SEQUENCE {}
}


UL-CCCH-Message ::= SEQUENCE {
	message					UL-CCCH-MessageType
}

UL-CCCH-MessageType ::= CHOICE {
	c1						CHOICE {
		rrcConnectionReestablishmentRequest		RRCConnectionReestablishmentRequest,
		rrcConnectionRequest					RRCConnectionRequest
	},
	messageClassExtension	SEQUENCE {}
}


UL-DCCH-Message ::= SEQUENCE {
	message					UL-DCCH-MessageType
}

UL-DCCH-MessageType ::= CHOICE {
	c1						CHOICE {
		csfbParametersRequestCDMA2000			CSFBParametersRequestCDMA2000,
		measurementReport						MeasurementReport,
		rrcConnectionReconfigurationComplete	RRCConnectionReconfigurationComplete,
		rrcConnectionReestablishmentComplete	RRCConnectionReestablishmentComplete,
		rrcConnectionSetupComplete				RRCConnectionSetupComplete,
		securityModeComplete					SecurityModeComplete,
		securityModeFailure						SecurityModeFailure,
		ueCapabilityInformation					UECapabilityInformation,
ulHandoverPreparationTransfer			ULHandoverPreparationTransfer,
		ulInformationTransfer					ULInformationTransfer,
		counterCheckResponse					CounterCheckResponse,
		ueInformationResponse-r9				UEInformationResponse-r9,
		proximityIndication-r9					ProximityIndication-r9,
				spare3 NULL, spare2 NULL, spare1 NULL
	},
	messageClassExtension	SEQUENCE {}
}


CounterCheck ::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			counterCheck-r8						CounterCheck-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

CounterCheck-r8-IEs ::=	SEQUENCE {
	drb-CountMSB-InfoList				DRB-CountMSB-InfoList,
	nonCriticalExtension				CounterCheck-v8a0-IEs							OPTIONAL
}

CounterCheck-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}

DRB-CountMSB-InfoList ::=		SEQUENCE (SIZE (1..maxDRB)) OF DRB-CountMSB-Info

DRB-CountMSB-Info ::=	SEQUENCE {
	drb-Identity					DRB-Identity,
	countMSB-Uplink					INTEGER(0..33554431),
	countMSB-Downlink				INTEGER(0..33554431)
}


CounterCheckResponse ::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		counterCheckResponse-r8				CounterCheckResponse-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

CounterCheckResponse-r8-IEs ::=	SEQUENCE {
	drb-CountInfoList					DRB-CountInfoList,
	nonCriticalExtension				CounterCheckResponse-v8a0-IEs							OPTIONAL
}

CounterCheckResponse-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

DRB-CountInfoList ::=			SEQUENCE (SIZE (0..maxDRB)) OF DRB-CountInfo

DRB-CountInfo ::=	SEQUENCE {
	drb-Identity					DRB-Identity,
	count-Uplink					INTEGER(0..4294967295),
	count-Downlink					INTEGER(0..4294967295)
}


CSFBParametersRequestCDMA2000 ::= SEQUENCE {
	criticalExtensions					CHOICE {
		csfbParametersRequestCDMA2000-r8	CSFBParametersRequestCDMA2000-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

CSFBParametersRequestCDMA2000-r8-IEs ::= SEQUENCE {
	nonCriticalExtension				CSFBParametersRequestCDMA2000-v8a0-IEs						OPTIONAL
}

CSFBParametersRequestCDMA2000-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


CSFBParametersResponseCDMA2000 ::= SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions						CHOICE {
		csfbParametersResponseCDMA2000-r8		CSFBParametersResponseCDMA2000-r8-IEs,
		criticalExtensionsFuture				SEQUENCE {}
	}
}

CSFBParametersResponseCDMA2000-r8-IEs ::= SEQUENCE {
	rand									RAND-CDMA2000,
	mobilityParameters						MobilityParametersCDMA2000,
	nonCriticalExtension					CSFBParametersResponseCDMA2000-v8a0-IEs						OPTIONAL
}

CSFBParametersResponseCDMA2000-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}


DLInformationTransfer ::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			dlInformationTransfer-r8			DLInformationTransfer-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

DLInformationTransfer-r8-IEs ::=	SEQUENCE {
	dedicatedInfoType					CHOICE {
		dedicatedInfoNAS					DedicatedInfoNAS,
		dedicatedInfoCDMA2000-1XRTT			DedicatedInfoCDMA2000,
		dedicatedInfoCDMA2000-HRPD			DedicatedInfoCDMA2000
	},
	nonCriticalExtension				DLInformationTransfer-v8a0-IEs						OPTIONAL
}

DLInformationTransfer-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}


HandoverFromEUTRAPreparationRequest ::= SEQUENCE {
	rrc-TransactionIdentifier		RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			handoverFromEUTRAPreparationRequest-r8
												HandoverFromEUTRAPreparationRequest-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

HandoverFromEUTRAPreparationRequest-r8-IEs ::= SEQUENCE {
	cdma2000-Type					CDMA2000-Type,
	rand							RAND-CDMA2000				OPTIONAL,  -- Cond cdma2000-Type
	mobilityParameters				MobilityParametersCDMA2000	OPTIONAL,  -- Cond cdma2000-Type
	nonCriticalExtension				HandoverFromEUTRAPreparationRequest-v890-IEs	OPTIONAL
}

HandoverFromEUTRAPreparationRequest-v890-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING				OPTIONAL,	-- Need OP
	nonCriticalExtension				HandoverFromEUTRAPreparationRequest-v920-IEs	OPTIONAL
}

HandoverFromEUTRAPreparationRequest-v920-IEs ::= SEQUENCE {
	concurrPrepCDMA2000-HRPD-r9		BOOLEAN						OPTIONAL,	-- Cond cdma2000-Type
	nonCriticalExtension				SEQUENCE {}					OPTIONAL	-- Need OP
}


MasterInformationBlock ::=			SEQUENCE {
	dl-Bandwidth						ENUMERATED {
											n6, n15, n25, n50, n75, n100},
	phich-Config						PHICH-Config,
	systemFrameNumber					BIT STRING (SIZE (8)),
	spare								BIT STRING (SIZE (10))
}



MBSFNAreaConfiguration-r9 ::=		SEQUENCE {
	commonSF-Alloc-r9					CommonSF-AllocPatternList-r9,
	commonSF-AllocPeriod-r9				ENUMERATED {
												rf4, rf8, rf16, rf32, rf64, rf128, rf256},
	pmch-InfoList-r9					PMCH-InfoList-r9,
	nonCriticalExtension				MBSFNAreaConfiguration-v930-IEs			OPTIONAL
}

MBSFNAreaConfiguration-v930-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}

CommonSF-AllocPatternList-r9 ::=	SEQUENCE (SIZE (1..maxMBSFN-Allocations)) OF MBSFN-SubframeConfig


MeasurementReport ::=				SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			measurementReport-r8				MeasurementReport-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

MeasurementReport-r8-IEs ::=		SEQUENCE {
	measResults							MeasResults,
	nonCriticalExtension				MeasurementReport-v8a0-IEs							OPTIONAL
}

MeasurementReport-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


MobilityFromEUTRACommand ::=		SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE{
			mobilityFromEUTRACommand-r8		MobilityFromEUTRACommand-r8-IEs,
			mobilityFromEUTRACommand-r9 		MobilityFromEUTRACommand-r9-IEs,
			spare2 NULL, spare1 	NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

MobilityFromEUTRACommand-r8-IEs ::=	SEQUENCE {
	cs-FallbackIndicator				BOOLEAN,
	purpose								CHOICE{
		handover							Handover,
		cellChangeOrder						CellChangeOrder
	},
	nonCriticalExtension				MobilityFromEUTRACommand-v8a0-IEs							OPTIONAL
}

MobilityFromEUTRACommand-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				MobilityFromEUTRACommand-v8d0-IEs	OPTIONAL
}

MobilityFromEUTRACommand-v8d0-IEs ::= SEQUENCE {
	bandIndicator						BandIndicatorGERAN			OPTIONAL,	-- Cond GERAN
	nonCriticalExtension				SEQUENCE {}					OPTIONAL	-- Need OP
}

MobilityFromEUTRACommand-r9-IEs ::=	SEQUENCE {
	cs-FallbackIndicator				BOOLEAN,
	purpose								CHOICE{
		handover							Handover,
		cellChangeOrder						CellChangeOrder,
		e-CSFB-r9							E-CSFB-r9,
		...
	},
	nonCriticalExtension				MobilityFromEUTRACommand-v930-IEs							OPTIONAL
}

MobilityFromEUTRACommand-v930-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				MobilityFromEUTRACommand-v960-IEs	OPTIONAL
}

MobilityFromEUTRACommand-v960-IEs ::= SEQUENCE {
	bandIndicator						BandIndicatorGERAN			OPTIONAL,	-- Cond GERAN
	nonCriticalExtension				SEQUENCE {}					OPTIONAL	-- Need OP
}

Handover ::=						SEQUENCE {
	targetRAT-Type						ENUMERATED {
											utra, geran, cdma2000-1XRTT, cdma2000-HRPD,
											spare4,	spare3, spare2, spare1, ...},
	targetRAT-MessageContainer			OCTET STRING,
	nas-SecurityParamFromEUTRA			OCTET STRING (SIZE (1)) 	OPTIONAL,  	-- Cond UTRAGERAN
	systemInformation					SI-OrPSI-GERAN				OPTIONAL	-- Cond PSHO
}

CellChangeOrder ::=				SEQUENCE {
	t304								ENUMERATED {
											ms100, ms200, ms500, ms1000,
											ms2000, ms4000, ms8000, spare1},
	targetRAT-Type						CHOICE {
			geran							SEQUENCE {
				physCellId						PhysCellIdGERAN,
				carrierFreq						CarrierFreqGERAN,
				networkControlOrder				BIT STRING (SIZE (2)) 		OPTIONAL,	-- Need OP
				systemInformation				SI-OrPSI-GERAN				OPTIONAL	-- Need OP
			},
			...
	}
}

SI-OrPSI-GERAN ::=					CHOICE {
	si									SystemInfoListGERAN,
	psi									SystemInfoListGERAN
}

E-CSFB-r9 ::=						SEQUENCE {
	messageContCDMA2000-1XRTT-r9		OCTET STRING		OPTIONAL, 	-- Need ON
	mobilityCDMA2000-HRPD-r9			ENUMERATED {
											handover, redirection
										}					OPTIONAL,	-- Need OP
	messageContCDMA2000-HRPD-r9		OCTET STRING		OPTIONAL, 	-- Cond concHO
	redirectCarrierCDMA2000-HRPD-r9	CarrierFreqCDMA2000	OPTIONAL	-- Cond concRedir
}


Paging ::=					SEQUENCE {
	pagingRecordList				PagingRecordList 					OPTIONAL,	-- Need ON
	systemInfoModification			ENUMERATED {true}					OPTIONAL,	-- Need ON
	etws-Indication					ENUMERATED {true}					OPTIONAL,	-- Need ON
	nonCriticalExtension				Paging-v890-IEs						OPTIONAL
}

Paging-v890-IEs ::=			SEQUENCE {
	lateNonCriticalExtension		OCTET STRING							OPTIONAL,	-- Need OP
	nonCriticalExtension			Paging-v920-IEs							OPTIONAL
}

Paging-v920-IEs ::=			SEQUENCE {
	cmas-Indication-r9				ENUMERATED {true}					OPTIONAL,	-- Need ON
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}

PagingRecordList ::=				SEQUENCE (SIZE (1..maxPageRec)) OF PagingRecord

PagingRecord ::=					SEQUENCE {
	ue-Identity							PagingUE-Identity,
	cn-Domain							ENUMERATED	{ps, cs},
	...
}

PagingUE-Identity ::=				CHOICE {
	s-TMSI								S-TMSI,
	imsi								IMSI,
	...
}

IMSI ::=							SEQUENCE (SIZE (6..21)) OF IMSI-Digit

IMSI-Digit ::=						INTEGER (0..9)


ProximityIndication-r9 ::= SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			proximityIndication-r9				ProximityIndication-r9-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
			},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

ProximityIndication-r9-IEs ::= SEQUENCE {
	type-r9								ENUMERATED {entering, leaving},
	carrierFreq-r9						CHOICE {
		eutra-r9							ARFCN-ValueEUTRA,
		utra-r9								ARFCN-ValueUTRA,
		...,
		eutra2-v9e0							ARFCN-ValueEUTRA-v9e0
	},
	nonCriticalExtension				ProximityIndication-v930-IEs							OPTIONAL
}

ProximityIndication-v930-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


RRCConnectionReconfiguration ::=	SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE{
			rrcConnectionReconfiguration-r8		RRCConnectionReconfiguration-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReconfiguration-r8-IEs ::= SEQUENCE {
	measConfig							MeasConfig						OPTIONAL,	-- Need ON
	mobilityControlInfo					MobilityControlInfo				OPTIONAL,	-- Cond HO
	dedicatedInfoNASList				SEQUENCE (SIZE(1..maxDRB)) OF
											DedicatedInfoNAS			OPTIONAL,	-- Cond nonHO
	radioResourceConfigDedicated		RadioResourceConfigDedicated	OPTIONAL, -- Cond HO-toEUTRA
	securityConfigHO					SecurityConfigHO				OPTIONAL,	-- Cond HO
	nonCriticalExtension				RRCConnectionReconfiguration-v890-IEs	OPTIONAL
}

RRCConnectionReconfiguration-v890-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,	-- Need OP
	nonCriticalExtension			RRCConnectionReconfiguration-v920-IEs		OPTIONAL
}

RRCConnectionReconfiguration-v920-IEs ::= SEQUENCE {
	otherConfig-r9						OtherConfig-r9					OPTIONAL,	-- Need ON
	fullConfig-r9						ENUMERATED {true}				OPTIONAL, 	-- Cond HO-Reestab
	nonCriticalExtension				SEQUENCE {}						OPTIONAL	-- Need OP
}

SecurityConfigHO ::=				SEQUENCE {
	handoverType						CHOICE {
		intraLTE							SEQUENCE {
			securityAlgorithmConfig				SecurityAlgorithmConfig		OPTIONAL,	-- Cond fullConfig
			keyChangeIndicator					BOOLEAN,
			nextHopChainingCount				NextHopChainingCount
		},
		interRAT							SEQUENCE {
			securityAlgorithmConfig				SecurityAlgorithmConfig,
			nas-SecurityParamToEUTRA			OCTET STRING (SIZE(6))
		}
	},
	...
}



RRCConnectionReconfigurationComplete ::= SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		rrcConnectionReconfigurationComplete-r8
											RRCConnectionReconfigurationComplete-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReconfigurationComplete-r8-IEs ::= SEQUENCE {
	nonCriticalExtension				RRCConnectionReconfigurationComplete-v8a0-IEs							OPTIONAL
}

RRCConnectionReconfigurationComplete-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


RRCConnectionReestablishment ::=	SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE{
			rrcConnectionReestablishment-r8		RRCConnectionReestablishment-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 	NULL,
			spare3 NULL, spare2 NULL, spare1 	NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReestablishment-r8-IEs ::= SEQUENCE {
	radioResourceConfigDedicated		RadioResourceConfigDedicated,
	nextHopChainingCount				NextHopChainingCount,
	nonCriticalExtension				RRCConnectionReestablishment-v8a0-IEs							OPTIONAL
}

RRCConnectionReestablishment-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}


RRCConnectionReestablishmentComplete ::= SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		rrcConnectionReestablishmentComplete-r8
											RRCConnectionReestablishmentComplete-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReestablishmentComplete-r8-IEs ::= SEQUENCE {
	nonCriticalExtension				RRCConnectionReestablishmentComplete-v920-IEs						OPTIONAL
}

RRCConnectionReestablishmentComplete-v920-IEs ::= SEQUENCE {
	rlf-InfoAvailable-r9				ENUMERATED {true}				OPTIONAL,
	nonCriticalExtension				RRCConnectionReestablishmentComplete-v8a0-IEs						OPTIONAL
}

RRCConnectionReestablishmentComplete-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


RRCConnectionReestablishmentReject ::= SEQUENCE {
	criticalExtensions					CHOICE {
		rrcConnectionReestablishmentReject-r8
											RRCConnectionReestablishmentReject-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReestablishmentReject-r8-IEs ::= SEQUENCE {
	nonCriticalExtension				RRCConnectionReestablishmentReject-v8a0-IEs							OPTIONAL
}

RRCConnectionReestablishmentReject-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}


RRCConnectionReestablishmentRequest ::= SEQUENCE {
	criticalExtensions					CHOICE {
		rrcConnectionReestablishmentRequest-r8
											RRCConnectionReestablishmentRequest-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReestablishmentRequest-r8-IEs ::= SEQUENCE {
	ue-Identity							ReestabUE-Identity,
	reestablishmentCause				ReestablishmentCause,
	spare								BIT STRING (SIZE (2))
}

ReestabUE-Identity ::=				SEQUENCE {
	c-RNTI								C-RNTI,
	physCellId							PhysCellId,
	shortMAC-I							ShortMAC-I
}

ReestablishmentCause ::=			ENUMERATED {
										reconfigurationFailure, handoverFailure,
										otherFailure, spare1}


RRCConnectionReject ::=				SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			rrcConnectionReject-r8				RRCConnectionReject-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReject-r8-IEs ::=		SEQUENCE {
	waitTime							INTEGER (1..16),
	nonCriticalExtension				RRCConnectionReject-v8a0-IEs							OPTIONAL
}

RRCConnectionReject-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}


RRCConnectionRelease ::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			rrcConnectionRelease-r8				RRCConnectionRelease-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionRelease-r8-IEs ::=		SEQUENCE {
	releaseCause						ReleaseCause,
	redirectedCarrierInfo				RedirectedCarrierInfo				OPTIONAL,	-- Need ON
	idleModeMobilityControlInfo			IdleModeMobilityControlInfo			OPTIONAL,	-- Need OP
	nonCriticalExtension				RRCConnectionRelease-v890-IEs		OPTIONAL
}

RRCConnectionRelease-v890-IEs ::=	SEQUENCE {
	lateNonCriticalExtension			OCTET STRING (CONTAINING RRCConnectionRelease-v9e0-IEs)	OPTIONAL,	-- Need OP
	nonCriticalExtension				RRCConnectionRelease-v920-IEs		OPTIONAL
}

RRCConnectionRelease-v9e0-IEs ::= SEQUENCE {
	redirectedCarrierInfo-v9e0			RedirectedCarrierInfo-v9e0			OPTIONAL,	-- Cond NoRedirect-r8
	idleModeMobilityControlInfo-v9e0	IdleModeMobilityControlInfo-v9e0	OPTIONAL,	-- Cond IdleInfoEUTRA
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}

RRCConnectionRelease-v920-IEs ::=	SEQUENCE {
	cellInfoList-r9					CHOICE {
		geran-r9						CellInfoListGERAN-r9,
		utra-FDD-r9						CellInfoListUTRA-FDD-r9,
		utra-TDD-r9						CellInfoListUTRA-TDD-r9,
		...
	}															OPTIONAL,	-- Cond Redirection
	nonCriticalExtension			SEQUENCE {}				OPTIONAL	-- Need OP
}

ReleaseCause ::=				ENUMERATED {loadBalancingTAUrequired,
											other,spare2,spare1}

RedirectedCarrierInfo ::=			CHOICE {
	eutra								ARFCN-ValueEUTRA,
	geran								CarrierFreqsGERAN,
	utra-FDD							ARFCN-ValueUTRA,
	utra-TDD							ARFCN-ValueUTRA,
	cdma2000-HRPD						CarrierFreqCDMA2000,
	cdma2000-1xRTT						CarrierFreqCDMA2000,
	...
}

RedirectedCarrierInfo-v9e0 ::=			SEQUENCE {
	eutra-v9e0								ARFCN-ValueEUTRA-v9e0
}

IdleModeMobilityControlInfo ::=		SEQUENCE {
	freqPriorityListEUTRA				FreqPriorityListEUTRA			OPTIONAL,		-- Need ON
	freqPriorityListGERAN				FreqsPriorityListGERAN			OPTIONAL,		-- Need ON
	freqPriorityListUTRA-FDD			FreqPriorityListUTRA-FDD		OPTIONAL,		-- Need ON
	freqPriorityListUTRA-TDD			FreqPriorityListUTRA-TDD		OPTIONAL,		-- Need ON
	bandClassPriorityListHRPD			BandClassPriorityListHRPD		OPTIONAL,		-- Need ON
	bandClassPriorityList1XRTT			BandClassPriorityList1XRTT		OPTIONAL,		-- Need ON
	t320								ENUMERATED {
											min5, min10, min20, min30, min60, min120, min180,
											spare1}						OPTIONAL,		-- Need OR
	...
}

IdleModeMobilityControlInfo-v9e0 ::=	SEQUENCE {
	freqPriorityListEUTRA-v9e0			SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA-v9e0
}

FreqPriorityListEUTRA ::=			SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA

FreqPriorityEUTRA ::=				SEQUENCE {
	carrierFreq							ARFCN-ValueEUTRA,
	cellReselectionPriority				CellReselectionPriority
}

FreqPriorityEUTRA-v9e0 ::=			SEQUENCE {
	carrierFreq-v9e0					ARFCN-ValueEUTRA-v9e0		OPTIONAL	-- Cond EARFCN-max
}

FreqsPriorityListGERAN ::=			SEQUENCE (SIZE (1..maxGNFG)) OF FreqsPriorityGERAN

FreqsPriorityGERAN ::=				SEQUENCE {
	carrierFreqs						CarrierFreqsGERAN,
	cellReselectionPriority				CellReselectionPriority
}

FreqPriorityListUTRA-FDD ::=		SEQUENCE (SIZE (1..maxUTRA-FDD-Carrier)) OF FreqPriorityUTRA-FDD

FreqPriorityUTRA-FDD ::=			SEQUENCE {
	carrierFreq							ARFCN-ValueUTRA,
	cellReselectionPriority				CellReselectionPriority
}

FreqPriorityListUTRA-TDD ::=		SEQUENCE (SIZE (1..maxUTRA-TDD-Carrier)) OF FreqPriorityUTRA-TDD

FreqPriorityUTRA-TDD ::=			SEQUENCE {
	carrierFreq							ARFCN-ValueUTRA,
	cellReselectionPriority				CellReselectionPriority
}

BandClassPriorityListHRPD ::=		SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandClassPriorityHRPD

BandClassPriorityHRPD ::=			SEQUENCE {
	bandClass							BandclassCDMA2000,
	cellReselectionPriority				CellReselectionPriority
}

BandClassPriorityList1XRTT ::=	SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandClassPriority1XRTT

BandClassPriority1XRTT ::=			SEQUENCE {
	bandClass							BandclassCDMA2000,
	cellReselectionPriority				CellReselectionPriority
}

CellInfoListGERAN-r9 ::=		SEQUENCE (SIZE (1..maxCellInfoGERAN-r9)) OF CellInfoGERAN-r9

CellInfoGERAN-r9 ::=				SEQUENCE {
	physCellId-r9						PhysCellIdGERAN,
	carrierFreq-r9						CarrierFreqGERAN,
	systemInformation-r9				SystemInfoListGERAN
}

CellInfoListUTRA-FDD-r9 ::=			SEQUENCE (SIZE (1..maxCellInfoUTRA-r9)) OF CellInfoUTRA-FDD-r9

CellInfoUTRA-FDD-r9 ::=				SEQUENCE {
	physCellId-r9						PhysCellIdUTRA-FDD,
	utra-BCCH-Container-r9				OCTET STRING
}

CellInfoListUTRA-TDD-r9 ::=			SEQUENCE (SIZE (1..maxCellInfoUTRA-r9)) OF CellInfoUTRA-TDD-r9

CellInfoUTRA-TDD-r9 ::=				SEQUENCE {
	physCellId-r9						PhysCellIdUTRA-TDD,
	utra-BCCH-Container-r9				OCTET STRING
}


RRCConnectionRequest ::=			SEQUENCE {
	criticalExtensions					CHOICE {
		rrcConnectionRequest-r8				RRCConnectionRequest-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionRequest-r8-IEs ::=		SEQUENCE {
	ue-Identity							InitialUE-Identity,
	establishmentCause					EstablishmentCause,
	spare								BIT STRING (SIZE (1))
}

InitialUE-Identity ::=				CHOICE {
	s-TMSI								S-TMSI,
	randomValue							BIT STRING (SIZE (40))
}

EstablishmentCause ::=				ENUMERATED {
										emergency, highPriorityAccess, mt-Access, mo-Signalling,
										mo-Data, spare3, spare2, spare1}


RRCConnectionSetup ::=				SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			rrcConnectionSetup-r8				RRCConnectionSetup-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionSetup-r8-IEs ::=		SEQUENCE {
	radioResourceConfigDedicated		RadioResourceConfigDedicated,
	nonCriticalExtension				RRCConnectionSetup-v8a0-IEs							OPTIONAL
}

RRCConnectionSetup-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}


RRCConnectionSetupComplete ::=		SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE{
			rrcConnectionSetupComplete-r8		RRCConnectionSetupComplete-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionSetupComplete-r8-IEs ::= SEQUENCE {
	selectedPLMN-Identity				INTEGER (1..6),
	registeredMME						RegisteredMME						OPTIONAL,
	dedicatedInfoNAS					DedicatedInfoNAS,
	nonCriticalExtension				RRCConnectionSetupComplete-v8a0-IEs							OPTIONAL
}

RRCConnectionSetupComplete-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

RegisteredMME ::=					SEQUENCE {
	plmn-Identity						PLMN-Identity						OPTIONAL,
	mmegi								BIT STRING (SIZE (16)),
	mmec								MMEC
}


SecurityModeCommand ::=				SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE{
			securityModeCommand-r8				SecurityModeCommand-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

SecurityModeCommand-r8-IEs ::=		SEQUENCE {
	securityConfigSMC					SecurityConfigSMC,
	nonCriticalExtension				SecurityModeCommand-v8a0-IEs							OPTIONAL
}

SecurityModeCommand-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}

SecurityConfigSMC ::=					SEQUENCE {
	securityAlgorithmConfig					SecurityAlgorithmConfig,
	...
}


SecurityModeComplete ::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		securityModeComplete-r8				SecurityModeComplete-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

SecurityModeComplete-r8-IEs ::=		SEQUENCE {
	nonCriticalExtension				SecurityModeComplete-v8a0-IEs							OPTIONAL
}

SecurityModeComplete-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


SecurityModeFailure ::=				SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		securityModeFailure-r8				SecurityModeFailure-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

SecurityModeFailure-r8-IEs ::=		SEQUENCE {
	nonCriticalExtension				SecurityModeFailure-v8a0-IEs							OPTIONAL
}

SecurityModeFailure-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


SystemInformation ::=				SEQUENCE {
	criticalExtensions					CHOICE {
		systemInformation-r8				SystemInformation-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}
SystemInformation-r8-IEs ::=		SEQUENCE {
	sib-TypeAndInfo						SEQUENCE (SIZE (1..maxSIB)) OF CHOICE {
		sib2								SystemInformationBlockType2,
		sib3								SystemInformationBlockType3,
		sib4								SystemInformationBlockType4,
		sib5								SystemInformationBlockType5,
		sib6								SystemInformationBlockType6,
		sib7								SystemInformationBlockType7,
		sib8								SystemInformationBlockType8,
		sib9								SystemInformationBlockType9,
		sib10								SystemInformationBlockType10,
		sib11								SystemInformationBlockType11,
		...,
		sib12-v920							SystemInformationBlockType12-r9,
		sib13-v920							SystemInformationBlockType13-r9
	},
	nonCriticalExtension				SystemInformation-v8a0-IEs							OPTIONAL
}

SystemInformation-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}


SystemInformationBlockType1 ::=		SEQUENCE {
	cellAccessRelatedInfo				SEQUENCE {
		plmn-IdentityList					PLMN-IdentityList,
		trackingAreaCode					TrackingAreaCode,
		cellIdentity						CellIdentity,
		cellBarred							ENUMERATED {barred, notBarred},
		intraFreqReselection				ENUMERATED {allowed, notAllowed},
		csg-Indication						BOOLEAN,
		csg-Identity						CSG-Identity			OPTIONAL	-- Need OR
	},
	cellSelectionInfo					SEQUENCE {
		q-RxLevMin							Q-RxLevMin,
		q-RxLevMinOffset					INTEGER (1..8)			OPTIONAL	-- Need OP
	},
	p-Max								P-Max						OPTIONAL,			-- Need OP
	freqBandIndicator					FreqBandIndicator,
	schedulingInfoList					SchedulingInfoList,
	tdd-Config							TDD-Config					OPTIONAL,	-- Cond TDD
	si-WindowLength						ENUMERATED {
											ms1, ms2, ms5, ms10, ms15, ms20,
											ms40},
	systemInfoValueTag					INTEGER (0..31),
	nonCriticalExtension				SystemInformationBlockType1-v890-IEs					OPTIONAL
}

SystemInformationBlockType1-v890-IEs::=	SEQUENCE {
	lateNonCriticalExtension				OCTET STRING (CONTAINING SystemInformationBlockType1-v8h0-IEs)			OPTIONAL,	-- Need OP
	nonCriticalExtension					SystemInformationBlockType1-v920-IEs	OPTIONAL
}

SystemInformationBlockType1-v8h0-IEs ::=	SEQUENCE {
	multiBandInfoList					MultiBandInfoList		OPTIONAL,	-- Need OR
	nonCriticalExtension				SystemInformationBlockType1-v9e0-IEs	OPTIONAL	-- Need OP
}

SystemInformationBlockType1-v9e0-IEs ::= SEQUENCE {
	freqBandIndicator-v9e0				FreqBandIndicator-v9e0		OPTIONAL,	-- Cond FBI-max
	multiBandInfoList-v9e0				MultiBandInfoList-v9e0		OPTIONAL,	-- Cond mFBI-max
	nonCriticalExtension				SEQUENCE {}					OPTIONAL	-- Need OP
}

SystemInformationBlockType1-v920-IEs ::=	SEQUENCE {
	ims-EmergencySupport-r9			ENUMERATED {true}				OPTIONAL,	-- Need OR
	cellSelectionInfo-v920				CellSelectionInfo-v920				OPTIONAL,	-- Cond RSRQ
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}

PLMN-IdentityList ::=					SEQUENCE (SIZE (1..6)) OF PLMN-IdentityInfo

PLMN-IdentityInfo ::=					SEQUENCE {
	plmn-Identity							PLMN-Identity,
	cellReservedForOperatorUse				ENUMERATED {reserved, notReserved}
}

SchedulingInfoList ::= SEQUENCE (SIZE (1..maxSI-Message)) OF SchedulingInfo

SchedulingInfo ::=	SEQUENCE {
	si-Periodicity						ENUMERATED {
											rf8, rf16, rf32, rf64, rf128, rf256, rf512},
	sib-MappingInfo						SIB-MappingInfo
}

SIB-MappingInfo ::= SEQUENCE (SIZE (0..maxSIB-1)) OF SIB-Type

SIB-Type ::=						ENUMERATED {
										sibType3, sibType4, sibType5, sibType6,
										sibType7, sibType8, sibType9, sibType10,
										sibType11, sibType12-v920, sibType13-v920, spare5,
										spare4, spare3, spare2, spare1, ...}

CellSelectionInfo-v920 ::=			SEQUENCE {
	q-QualMin-r9						Q-QualMin-r9,
	q-QualMinOffset-r9					INTEGER (1..8)						OPTIONAL	-- Need OP
}


UECapabilityEnquiry ::=				SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			ueCapabilityEnquiry-r8				UECapabilityEnquiry-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UECapabilityEnquiry-r8-IEs ::=		SEQUENCE {
	ue-CapabilityRequest				UE-CapabilityRequest,
	nonCriticalExtension				UECapabilityEnquiry-v8a0-IEs							OPTIONAL
}

UECapabilityEnquiry-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}

UE-CapabilityRequest ::=		SEQUENCE (SIZE (1..maxRAT-Capabilities)) OF RAT-Type


UECapabilityInformation ::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE{
			ueCapabilityInformation-r8			UECapabilityInformation-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UECapabilityInformation-r8-IEs ::=	SEQUENCE {
	ue-CapabilityRAT-ContainerList		UE-CapabilityRAT-ContainerList,
	nonCriticalExtension				UECapabilityInformation-v8a0-IEs							OPTIONAL
}

UECapabilityInformation-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


UEInformationRequest-r9		::=				SEQUENCE {
	rrc-TransactionIdentifier		RRC-TransactionIdentifier,
	criticalExtensions				CHOICE {
		c1								CHOICE {
			ueInformationRequest-r9				UEInformationRequest-r9-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UEInformationRequest-r9-IEs ::=		SEQUENCE {
	rach-ReportReq-r9							BOOLEAN,
	rlf-ReportReq-r9							BOOLEAN,
	nonCriticalExtension					UEInformationRequest-v930-IEs					OPTIONAL
}

UEInformationRequest-v930-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	nonCriticalExtension				SEQUENCE {}							OPTIONAL	-- Need OP
}


UEInformationResponse-r9	::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1								CHOICE {
			ueInformationResponse-r9				UEInformationResponse-r9-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture				SEQUENCE {}
	}
}

UEInformationResponse-r9-IEs ::=		SEQUENCE {
	rach-Report-r9							SEQUENCE {
		numberOfPreamblesSent-r9				INTEGER (1..200),
		contentionDetected-r9					BOOLEAN
	}																OPTIONAL,
	rlfReport-r9							RLF-Report-r9			OPTIONAL,
	nonCriticalExtension					UEInformationResponse-v930-IEs				OPTIONAL
}

UEInformationResponse-v930-IEs ::=	SEQUENCE {
	lateNonCriticalExtension			OCTET STRING (CONTAINING UEInformationResponse-v9e0-IEs)		OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

UEInformationResponse-v9e0-IEs ::= SEQUENCE {
	rlf-Report-v9e0						RLF-Report-v9e0					OPTIONAL,
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}

RLF-Report-r9 ::= 					SEQUENCE {
	measResultLastServCell-r9				SEQUENCE {
		rsrpResult-r9							RSRP-Range,
		rsrqResult-r9							RSRQ-Range			OPTIONAL
	},
	measResultNeighCells-r9				SEQUENCE {
		measResultListEUTRA-r9					MeasResultList2EUTRA-r9		OPTIONAL,
		measResultListUTRA-r9					MeasResultList2UTRA-r9		OPTIONAL,
		measResultListGERAN-r9					MeasResultListGERAN			OPTIONAL,
		measResultsCDMA2000-r9					MeasResultList2CDMA2000-r9	OPTIONAL
	}																OPTIONAL,
	...
}

RLF-Report-v9e0 ::= 				SEQUENCE {
	measResultListEUTRA-v9e0			MeasResultList2EUTRA-v9e0
}

MeasResultList2EUTRA-r9 ::=				SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2EUTRA-r9

MeasResultList2EUTRA-v9e0 ::=			SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2EUTRA-v9e0

MeasResult2EUTRA-r9 ::=				SEQUENCE {
	carrierFreq-r9						ARFCN-ValueEUTRA,
	measResultList-r9					MeasResultListEUTRA
}

MeasResult2EUTRA-v9e0 ::=				SEQUENCE {
	carrierFreq-v9e0						ARFCN-ValueEUTRA-v9e0		OPTIONAL
}

MeasResultList2UTRA-r9 ::=			SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2UTRA-r9

MeasResult2UTRA-r9 ::=				SEQUENCE {
	carrierFreq-r9						ARFCN-ValueUTRA,
	measResultList-r9					MeasResultListUTRA
}

MeasResultList2CDMA2000-r9 ::=		SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2CDMA2000-r9

MeasResult2CDMA2000-r9 ::= 			SEQUENCE {
	carrierFreq-r9							CarrierFreqCDMA2000,
	measResultList-r9						MeasResultsCDMA2000
}


ULHandoverPreparationTransfer ::=	SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			ulHandoverPreparationTransfer-r8		ULHandoverPreparationTransfer-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture				SEQUENCE {}
	}
}

ULHandoverPreparationTransfer-r8-IEs ::= SEQUENCE {
	cdma2000-Type						CDMA2000-Type,
	meid								BIT STRING (SIZE (56))	OPTIONAL,
	dedicatedInfo						DedicatedInfoCDMA2000,
	nonCriticalExtension				ULHandoverPreparationTransfer-v8a0-IEs							OPTIONAL
}

ULHandoverPreparationTransfer-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


ULInformationTransfer ::=			SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			ulInformationTransfer-r8			ULInformationTransfer-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

ULInformationTransfer-r8-IEs ::=	SEQUENCE {
	dedicatedInfoType			CHOICE {
		dedicatedInfoNAS					DedicatedInfoNAS,
		dedicatedInfoCDMA2000-1XRTT			DedicatedInfoCDMA2000,
		dedicatedInfoCDMA2000-HRPD			DedicatedInfoCDMA2000
	},
	nonCriticalExtension				ULInformationTransfer-v8a0-IEs							OPTIONAL
}

ULInformationTransfer-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


SystemInformationBlockType2 ::=		SEQUENCE {
	ac-BarringInfo						SEQUENCE {
		ac-BarringForEmergency				BOOLEAN,
		ac-BarringForMO-Signalling			AC-BarringConfig				OPTIONAL,	-- Need OP
		ac-BarringForMO-Data				AC-BarringConfig				OPTIONAL	-- Need OP
	}																		OPTIONAL,	-- Need OP
	radioResourceConfigCommon			RadioResourceConfigCommonSIB,
	ue-TimersAndConstants				UE-TimersAndConstants,
	freqInfo							SEQUENCE {
		ul-CarrierFreq						ARFCN-ValueEUTRA				OPTIONAL,	-- Need OP
		ul-Bandwidth						ENUMERATED {n6, n15, n25, n50, n75, n100}
																			OPTIONAL,	-- Need OP
		additionalSpectrumEmission			AdditionalSpectrumEmission
	},
	mbsfn-SubframeConfigList			MBSFN-SubframeConfigList			OPTIONAL, 	-- Need OR
	timeAlignmentTimerCommon			TimeAlignmentTimer,
	...,
	lateNonCriticalExtension		OCTET STRING (CONTAINING SystemInformationBlockType2-v8h0-IEs)						OPTIONAL,	-- Need OP
	[[	ssac-BarringForMMTEL-Voice-r9		AC-BarringConfig				OPTIONAL,	-- Need OP
		ssac-BarringForMMTEL-Video-r9		AC-BarringConfig				OPTIONAL	-- Need OP
	]]
}

SystemInformationBlockType2-v8h0-IEs ::=	SEQUENCE {
	multiBandInfoList				SEQUENCE (SIZE (1..maxMultiBands)) OF AdditionalSpectrumEmission	OPTIONAL,	-- Need OR
	nonCriticalExtension			SystemInformationBlockType2-v9e0-IEs	OPTIONAL	-- Need OP
}

SystemInformationBlockType2-v9e0-IEs ::= SEQUENCE {
	ul-CarrierFreq-v9e0					ARFCN-ValueEUTRA-v9e0		OPTIONAL,	-- Cond ul-FreqMax
	nonCriticalExtension				SEQUENCE {}					OPTIONAL	-- Need OP
}

AC-BarringConfig ::=				SEQUENCE {
	ac-BarringFactor					ENUMERATED {
											p00, p05, p10, p15, p20, p25, p30, p40,
											p50, p60, p70, p75, p80, p85, p90, p95},
	ac-BarringTime						ENUMERATED {s4, s8, s16, s32, s64, s128, s256, s512},
	ac-BarringForSpecialAC				BIT STRING (SIZE(5))
}

MBSFN-SubframeConfigList ::= 		SEQUENCE (SIZE (1..maxMBSFN-Allocations)) OF MBSFN-SubframeConfig


SystemInformationBlockType3 ::=		SEQUENCE {
	cellReselectionInfoCommon			SEQUENCE {
		q-Hyst								ENUMERATED {
												dB0, dB1, dB2, dB3, dB4, dB5, dB6, dB8, dB10,
												dB12, dB14, dB16, dB18, dB20, dB22, dB24},
		speedStateReselectionPars			SEQUENCE {
			mobilityStateParameters				MobilityStateParameters,
			q-HystSF						SEQUENCE {
				sf-Medium						ENUMERATED {
														dB-6, dB-4, dB-2, dB0},
				sf-High							ENUMERATED {
														dB-6, dB-4, dB-2, dB0}
			}
		}																OPTIONAL		-- Need OP
	},
	cellReselectionServingFreqInfo		SEQUENCE {
		s-NonIntraSearch					ReselectionThreshold		OPTIONAL,		-- Need OP
		threshServingLow					ReselectionThreshold,
		cellReselectionPriority				CellReselectionPriority
	},
	intraFreqCellReselectionInfo		SEQUENCE {
		q-RxLevMin							Q-RxLevMin,
		p-Max								P-Max						OPTIONAL,		-- Need OP
		s-IntraSearch						ReselectionThreshold		OPTIONAL,		-- Need OP
		allowedMeasBandwidth				AllowedMeasBandwidth		OPTIONAL,		-- Need OP
		presenceAntennaPort1				PresenceAntennaPort1,
		neighCellConfig						NeighCellConfig,
		t-ReselectionEUTRA					T-Reselection,
		t-ReselectionEUTRA-SF				SpeedStateScaleFactors		OPTIONAL		-- Need OP
	},
	...,
	lateNonCriticalExtension				OCTET STRING			OPTIONAL,	-- Need OP
	[[	s-IntraSearch-v920					SEQUENCE {
			s-IntraSearchP-r9					ReselectionThreshold,
			s-IntraSearchQ-r9					ReselectionThresholdQ-r9
		}																OPTIONAL,		-- Need OP
		s-NonIntraSearch-v920				SEQUENCE {
			s-NonIntraSearchP-r9				ReselectionThreshold,
			s-NonIntraSearchQ-r9				ReselectionThresholdQ-r9
		}																OPTIONAL,		-- Need OP
		q-QualMin-r9						Q-QualMin-r9				OPTIONAL,		-- Need OP
		threshServingLowQ-r9				ReselectionThresholdQ-r9	OPTIONAL		-- Need OP
	]]
}


SystemInformationBlockType4 ::=		SEQUENCE {
	intraFreqNeighCellList				IntraFreqNeighCellList		OPTIONAL,	-- Need OR
	intraFreqBlackCellList				IntraFreqBlackCellList				OPTIONAL,	-- Need OR
	csg-PhysCellIdRange					PhysCellIdRange				OPTIONAL,	-- Cond CSG
	...,
	lateNonCriticalExtension				OCTET STRING				OPTIONAL		-- Need OP
}

IntraFreqNeighCellList ::=		SEQUENCE (SIZE (1..maxCellIntra)) OF IntraFreqNeighCellInfo

IntraFreqNeighCellInfo ::=		SEQUENCE {
	physCellId								PhysCellId,
	q-OffsetCell							Q-OffsetRange,
	...
}

IntraFreqBlackCellList ::=		SEQUENCE (SIZE (1..maxCellBlack)) OF PhysCellIdRange


SystemInformationBlockType5 ::=		SEQUENCE {
	interFreqCarrierFreqList			InterFreqCarrierFreqList,
	...,
	lateNonCriticalExtension				OCTET STRING	(CONTAINING SystemInformationBlockType5-v8h0-IEs)				OPTIONAL	-- Need OP
}

SystemInformationBlockType5-v8h0-IEs ::=	SEQUENCE {
	interFreqCarrierFreqList-v8h0 SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v8h0				 OPTIONAL,	-- Need OP
	nonCriticalExtension			SystemInformationBlockType5-v9e0-IEs	OPTIONAL	-- Need OP
}

SystemInformationBlockType5-v9e0-IEs ::=	SEQUENCE {
	interFreqCarrierFreqList-v9e0	SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v9e0				OPTIONAL,	-- Need OR
	nonCriticalExtension			SEQUENCE {}							OPTIONAL	-- Need OP
}

InterFreqCarrierFreqList ::=		SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo

InterFreqCarrierFreqInfo ::=	SEQUENCE {
	dl-CarrierFreq						ARFCN-ValueEUTRA,
	q-RxLevMin							Q-RxLevMin,
	p-Max								P-Max							OPTIONAL,		-- Need OP
	t-ReselectionEUTRA					T-Reselection,
	t-ReselectionEUTRA-SF				SpeedStateScaleFactors			OPTIONAL,		-- Need OP
	threshX-High						ReselectionThreshold,
	threshX-Low							ReselectionThreshold,
	allowedMeasBandwidth				AllowedMeasBandwidth,
	presenceAntennaPort1				PresenceAntennaPort1,
	cellReselectionPriority				CellReselectionPriority			OPTIONAL,		-- Need OP
	neighCellConfig						NeighCellConfig,
	q-OffsetFreq						Q-OffsetRange					DEFAULT dB0,
	interFreqNeighCellList				InterFreqNeighCellList			OPTIONAL, 		-- Need OR
	interFreqBlackCellList				InterFreqBlackCellList			OPTIONAL, 		-- Need OR
	...,
	[[	q-QualMin-r9					Q-QualMin-r9					OPTIONAL,		-- Need OP
		threshX-Q-r9					SEQUENCE {
			threshX-HighQ-r9				ReselectionThresholdQ-r9,
			threshX-LowQ-r9					ReselectionThresholdQ-r9
		}																OPTIONAL		-- Cond RSRQ
	]]
}

InterFreqCarrierFreqInfo-v8h0 ::=		SEQUENCE {
	multiBandInfoList					MultiBandInfoList				OPTIONAL	-- Need OR
}

InterFreqCarrierFreqInfo-v9e0 ::=	SEQUENCE {
	dl-CarrierFreq-v9e0					ARFCN-ValueEUTRA-v9e0	OPTIONAL,	-- Cond dl-FreqMax
	multiBandInfoList-v9e0				MultiBandInfoList-v9e0	OPTIONAL	-- Need OR
}

InterFreqNeighCellList ::=			SEQUENCE (SIZE (1..maxCellInter)) OF InterFreqNeighCellInfo

InterFreqNeighCellInfo ::=			SEQUENCE {
	physCellId							PhysCellId,
	q-OffsetCell						Q-OffsetRange
}

InterFreqBlackCellList ::=			SEQUENCE (SIZE (1..maxCellBlack)) OF PhysCellIdRange


SystemInformationBlockType6 ::=		SEQUENCE {
	carrierFreqListUTRA-FDD				CarrierFreqListUTRA-FDD			OPTIONAL, 		-- Need OR
	carrierFreqListUTRA-TDD				CarrierFreqListUTRA-TDD			OPTIONAL, 		-- Need OR
	t-ReselectionUTRA					T-Reselection,
	t-ReselectionUTRA-SF				SpeedStateScaleFactors			OPTIONAL,		-- Need OP
	...,
	lateNonCriticalExtension			OCTET STRING	(CONTAINING SystemInformationBlockType6-v8h0-IEs)					OPTIONAL	-- Need OP
}

SystemInformationBlockType6-v8h0-IEs ::=	SEQUENCE {
	carrierFreqListUTRA-FDD-v8h0 SEQUENCE (SIZE (1..maxUTRA-FDD-Carrier)) OF CarrierFreqInfoUTRA-FDD-v8h0 OPTIONAL,	-- Need OR
	nonCriticalExtension			SEQUENCE {}							OPTIONAL	-- Need OP
}

CarrierFreqListUTRA-FDD ::=		SEQUENCE (SIZE (1..maxUTRA-FDD-Carrier)) OF CarrierFreqUTRA-FDD

CarrierFreqUTRA-FDD ::=				SEQUENCE {
	carrierFreq							ARFCN-ValueUTRA,
	cellReselectionPriority				CellReselectionPriority			OPTIONAL, 		-- Need OP
	threshX-High						ReselectionThreshold,
	threshX-Low							ReselectionThreshold,
	q-RxLevMin							INTEGER (-60..-13),
	p-MaxUTRA							INTEGER (-50..33),
	q-QualMin							INTEGER (-24..0),
	...,
	[[	threshX-Q-r9					SEQUENCE {
			threshX-HighQ-r9				ReselectionThresholdQ-r9,
			threshX-LowQ-r9					ReselectionThresholdQ-r9
		}																OPTIONAL		-- Cond RSRQ
	]]
}

CarrierFreqInfoUTRA-FDD-v8h0 ::=			SEQUENCE {
	multiBandInfoList					SEQUENCE (SIZE (1..maxMultiBands)) OF FreqBandIndicator-UTRA-FDD				OPTIONAL	-- Need OR
}


CarrierFreqListUTRA-TDD ::=		SEQUENCE (SIZE (1..maxUTRA-TDD-Carrier)) OF CarrierFreqUTRA-TDD

CarrierFreqUTRA-TDD ::=				SEQUENCE {
	carrierFreq							ARFCN-ValueUTRA,
	cellReselectionPriority				CellReselectionPriority			OPTIONAL, 		-- Need OP
	threshX-High						ReselectionThreshold,
	threshX-Low							ReselectionThreshold,
	q-RxLevMin							INTEGER (-60..-13),
	p-MaxUTRA							INTEGER (-50..33),
	...
}

FreqBandIndicator-UTRA-FDD ::=				INTEGER (1..86)


SystemInformationBlockType7 ::=		SEQUENCE {
	t-ReselectionGERAN					T-Reselection,
	t-ReselectionGERAN-SF				SpeedStateScaleFactors				OPTIONAL,	-- Need OR
	carrierFreqsInfoList				CarrierFreqsInfoListGERAN			OPTIONAL,	-- Need OR
	...,
	lateNonCriticalExtension				OCTET STRING				OPTIONAL		-- Need OP
}

CarrierFreqsInfoListGERAN ::=			SEQUENCE (SIZE (1..maxGNFG)) OF CarrierFreqsInfoGERAN

CarrierFreqsInfoGERAN ::=			SEQUENCE {
	carrierFreqs						CarrierFreqsGERAN,
	commonInfo							SEQUENCE {
		cellReselectionPriority				CellReselectionPriority			OPTIONAL,	-- Need OP
		ncc-Permitted						BIT STRING (SIZE (8)),
		q-RxLevMin							INTEGER (0..45),
		p-MaxGERAN							INTEGER (0..39)					OPTIONAL,	-- Need OP
		threshX-High						ReselectionThreshold,
		threshX-Low							ReselectionThreshold
	},
	...
}


SystemInformationBlockType8 ::=		SEQUENCE {
	systemTimeInfo						SystemTimeInfoCDMA2000				OPTIONAL,	-- Need OR
	searchWindowSize					INTEGER (0..15)						OPTIONAL,	-- Need OR
	parametersHRPD						SEQUENCE {
		preRegistrationInfoHRPD				PreRegistrationInfoHRPD,
		cellReselectionParametersHRPD		CellReselectionParametersCDMA2000	OPTIONAL -- Need OR
	}																		OPTIONAL,	-- Need OR
	parameters1XRTT						SEQUENCE {
		csfb-RegistrationParam1XRTT			CSFB-RegistrationParam1XRTT		OPTIONAL,	-- Need OP
		longCodeState1XRTT					BIT STRING (SIZE (42))			OPTIONAL,	-- Need OR
		cellReselectionParameters1XRTT		CellReselectionParametersCDMA2000	OPTIONAL -- Need OR
	}																		OPTIONAL,	-- Need OR
	...,
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,	-- Need OP
	[[	csfb-SupportForDualRxUEs-r9			BOOLEAN							OPTIONAL,	-- Need OR
		cellReselectionParametersHRPD-v920	CellReselectionParametersCDMA2000-v920	OPTIONAL,	-- Cond NCL-HRPD
		cellReselectionParameters1XRTT-v920	CellReselectionParametersCDMA2000-v920	OPTIONAL,	-- Cond NCL-1XRTT
		csfb-RegistrationParam1XRTT-v920	CSFB-RegistrationParam1XRTT-v920 		OPTIONAL,	-- Cond REG-1XRTT
		ac-BarringConfig1XRTT-r9			AC-BarringConfig1XRTT-r9		OPTIONAL 	-- Cond REG-1XRTT
	]]
}

CellReselectionParametersCDMA2000 ::= SEQUENCE {
	bandClassList						BandClassListCDMA2000,
	neighCellList						NeighCellListCDMA2000,
	t-ReselectionCDMA2000      			T-Reselection,
	t-ReselectionCDMA2000-SF			SpeedStateScaleFactors				OPTIONAL	-- Need OP
}

CellReselectionParametersCDMA2000-v920 ::= SEQUENCE {
	neighCellList-v920						NeighCellListCDMA2000-v920
}

NeighCellListCDMA2000 ::=			SEQUENCE (SIZE (1..16)) OF NeighCellCDMA2000

NeighCellCDMA2000 ::=	SEQUENCE {
	bandClass							BandclassCDMA2000,
	neighCellsPerFreqList				NeighCellsPerBandclassListCDMA2000
}

NeighCellsPerBandclassListCDMA2000 ::= SEQUENCE (SIZE (1..16)) OF NeighCellsPerBandclassCDMA2000

NeighCellsPerBandclassCDMA2000 ::=	SEQUENCE {
	arfcn								ARFCN-ValueCDMA2000,
	physCellIdList						PhysCellIdListCDMA2000
}

NeighCellListCDMA2000-v920 ::=		SEQUENCE (SIZE (1..16)) OF NeighCellCDMA2000-v920

NeighCellCDMA2000-v920 ::=			SEQUENCE {
	neighCellsPerFreqList-v920			NeighCellsPerBandclassListCDMA2000-v920
}

NeighCellsPerBandclassListCDMA2000-v920 ::= SEQUENCE (SIZE (1..16)) OF NeighCellsPerBandclassCDMA2000-v920

NeighCellsPerBandclassCDMA2000-v920 ::=	SEQUENCE {
	physCellIdList-v920					PhysCellIdListCDMA2000-v920
}

PhysCellIdListCDMA2000 ::=			SEQUENCE (SIZE (1..16)) OF PhysCellIdCDMA2000

PhysCellIdListCDMA2000-v920 ::=		SEQUENCE (SIZE (0..24)) OF PhysCellIdCDMA2000

BandClassListCDMA2000 ::=			SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandClassInfoCDMA2000

BandClassInfoCDMA2000 ::=	SEQUENCE {
	bandClass							BandclassCDMA2000,
	cellReselectionPriority				CellReselectionPriority				OPTIONAL,	-- Need OP
	threshX-High						INTEGER (0..63),
	threshX-Low							INTEGER (0..63),
	...
}

AC-BarringConfig1XRTT-r9 ::=		SEQUENCE {
	ac-Barring0to9-r9					INTEGER (0..63),
	ac-Barring10-r9						INTEGER (0..7),
	ac-Barring11-r9						INTEGER (0..7),
	ac-Barring12-r9						INTEGER (0..7),
	ac-Barring13-r9						INTEGER (0..7),
	ac-Barring14-r9						INTEGER (0..7),
	ac-Barring15-r9						INTEGER (0..7),
	ac-BarringMsg-r9					INTEGER (0..7),
	ac-BarringReg-r9					INTEGER (0..7),
	ac-BarringEmg-r9					INTEGER (0..7)
}


SystemInformationBlockType9 ::=		SEQUENCE {
	hnb-Name							OCTET STRING (SIZE(1..48))		OPTIONAL,	-- Need OR
	...,
	lateNonCriticalExtension				OCTET STRING				OPTIONAL		-- Need OP
}


SystemInformationBlockType10 ::=	SEQUENCE {
	messageIdentifier					BIT STRING (SIZE (16)),
	serialNumber						BIT STRING (SIZE (16)),
	warningType							OCTET STRING (SIZE (2)),
	dummy								OCTET STRING (SIZE (50))		OPTIONAL,		-- Need OP
	...,
	lateNonCriticalExtension				OCTET STRING				OPTIONAL		-- Need OP
}


SystemInformationBlockType11 ::=	SEQUENCE {
	messageIdentifier					BIT STRING (SIZE (16)),
	serialNumber						BIT STRING (SIZE (16)),
	warningMessageSegmentType			ENUMERATED {notLastSegment, lastSegment},
	warningMessageSegmentNumber			INTEGER (0..63),
	warningMessageSegment				OCTET STRING,
	dataCodingScheme					OCTET STRING (SIZE (1)) 		OPTIONAL, 	-- Cond Segment1
	...,
	lateNonCriticalExtension				OCTET STRING				OPTIONAL		-- Need OP
}


SystemInformationBlockType12-r9 ::=	SEQUENCE {
	messageIdentifier-r9				BIT STRING (SIZE (16)),
	serialNumber-r9						BIT STRING (SIZE (16)),
	warningMessageSegmentType-r9		ENUMERATED {notLastSegment, lastSegment},
	warningMessageSegmentNumber-r9		INTEGER (0..63),
	warningMessageSegment-r9			OCTET STRING,
	dataCodingScheme-r9					OCTET STRING (SIZE (1)) 		OPTIONAL, 	-- Cond Segment1
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,	-- Need OP
	...
}


SystemInformationBlockType13-r9 ::=	SEQUENCE {
	mbsfn-AreaInfoList-r9				MBSFN-AreaInfoList-r9,
	notificationConfig-r9				MBMS-NotificationConfig-r9,
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,	-- Need OP
	...
}


AntennaInfoCommon ::=				SEQUENCE {
	antennaPortsCount					ENUMERATED {an1, an2, an4, spare1}
}

AntennaInfoDedicated ::=			SEQUENCE {
	transmissionMode					ENUMERATED {
											tm1, tm2, tm3, tm4, tm5, tm6,
											tm7, tm8-v920},
	codebookSubsetRestriction			CHOICE {
		n2TxAntenna-tm3						BIT STRING (SIZE (2)),
		n4TxAntenna-tm3						BIT STRING (SIZE (4)),
		n2TxAntenna-tm4						BIT STRING (SIZE (6)),
		n4TxAntenna-tm4						BIT STRING (SIZE (64)),
		n2TxAntenna-tm5						BIT STRING (SIZE (4)),
		n4TxAntenna-tm5						BIT STRING (SIZE (16)),
		n2TxAntenna-tm6						BIT STRING (SIZE (4)),
		n4TxAntenna-tm6						BIT STRING (SIZE (16))
	}		OPTIONAL, 															-- Cond TM
	ue-TransmitAntennaSelection			CHOICE{
		release							NULL,
		setup							ENUMERATED {closedLoop, openLoop}
	}
}

AntennaInfoDedicated-v920 ::=		SEQUENCE {
	codebookSubsetRestriction-v920		CHOICE {
		n2TxAntenna-tm8-r9					BIT STRING (SIZE (6)),
		n4TxAntenna-tm8-r9					BIT STRING (SIZE (32))
	}		OPTIONAL 															-- Cond TM8
}


CQI-ReportConfig ::=				SEQUENCE {
	cqi-ReportModeAperiodic			ENUMERATED {
											rm12, rm20, rm22, rm30, rm31,
											spare3, spare2, spare1} OPTIONAL, 			-- Need OR
	nomPDSCH-RS-EPRE-Offset				INTEGER (-1..6),
	cqi-ReportPeriodic				CQI-ReportPeriodic	OPTIONAL 				-- Need ON
}

CQI-ReportConfig-v920 ::=		SEQUENCE {
	cqi-Mask-r9						ENUMERATED {setup}		OPTIONAL,		-- Cond cqi-Setup
	pmi-RI-Report-r9				ENUMERATED {setup}		OPTIONAL		-- Cond PMIRI
}

CQI-ReportPeriodic ::=		CHOICE {
	release							NULL,
	setup							SEQUENCE {
		cqi-PUCCH-ResourceIndex				INTEGER (0.. 1185),
		cqi-pmi-ConfigIndex					INTEGER (0..1023),
		cqi-FormatIndicatorPeriodic			CHOICE {
			widebandCQI							NULL,
			subbandCQI							SEQUENCE {
				k									INTEGER (1..4)
			}
		},
		ri-ConfigIndex						INTEGER (0..1023) 	OPTIONAL, 				-- Need OR
		simultaneousAckNackAndCQI			BOOLEAN
	}
}


DRB-Identity ::=					INTEGER (1..32)


LogicalChannelConfig ::=			SEQUENCE {
	ul-SpecificParameters				SEQUENCE {
		priority							INTEGER (1..16),
		prioritisedBitRate					ENUMERATED {
												kBps0, kBps8, kBps16, kBps32, kBps64, kBps128,
												kBps256, infinity, spare8, spare7, spare6,
												spare5, spare4, spare3, spare2, spare1},
		bucketSizeDuration					ENUMERATED {
												ms50, ms100, ms150, ms300, ms500, ms1000, spare2,
												spare1},
		logicalChannelGroup					INTEGER (0..3)			OPTIONAL			-- Need OR
	}		OPTIONAL,																	-- Cond UL
	...,
	[[	logicalChannelSR-Mask-r9			ENUMERATED {setup}		OPTIONAL		-- Cond SRmask
	]]
}


MAC-MainConfig ::=					SEQUENCE {
	ul-SCH-Config						SEQUENCE {
		maxHARQ-Tx							ENUMERATED {
												n1, n2, n3, n4, n5, n6, n7, n8,
												n10, n12, n16, n20, n24, n28,
												spare2, spare1}		OPTIONAL,	-- Need ON
		periodicBSR-Timer					ENUMERATED {
												sf5, sf10, sf16, sf20, sf32, sf40, sf64, sf80,
												sf128, sf160, sf320, sf640, sf1280, sf2560,
												infinity, spare1}	OPTIONAL,	-- Need ON
		retxBSR-Timer						ENUMERATED {
												sf320, sf640, sf1280, sf2560, sf5120,
												sf10240, spare2, spare1},
		ttiBundling							BOOLEAN
	}																OPTIONAL, 	-- Need ON
	drx-Config							DRX-Config					OPTIONAL,	-- Need ON
	timeAlignmentTimerDedicated			TimeAlignmentTimer,
	phr-Config							CHOICE {
		release								NULL,
		setup								SEQUENCE {
			periodicPHR-Timer					ENUMERATED {sf10, sf20, sf50, sf100, sf200,
															sf500, sf1000, infinity},
			prohibitPHR-Timer					ENUMERATED {sf0, sf10, sf20, sf50, sf100,
																sf200, sf500, sf1000},
			dl-PathlossChange					ENUMERATED {dB1, dB3, dB6, infinity}
		}
	}																OPTIONAL,	-- Need ON
	...,
	[[	sr-ProhibitTimer-r9					INTEGER (0..7)			OPTIONAL	-- Need ON
	]]
}

DRX-Config ::=						CHOICE {
	release								NULL,
	setup								SEQUENCE {
		onDurationTimer						ENUMERATED {
												psf1, psf2, psf3, psf4, psf5, psf6,
												psf8, psf10, psf20, psf30, psf40,
												psf50, psf60, psf80, psf100,
												psf200},
		drx-InactivityTimer					ENUMERATED {
												psf1, psf2, psf3, psf4, psf5, psf6,
												psf8, psf10, psf20, psf30, psf40,
												psf50, psf60, psf80, psf100,
												psf200, psf300, psf500, psf750,
												psf1280, psf1920, psf2560, spare10,
												spare9, spare8, spare7, spare6,
												spare5, spare4, spare3, spare2,
												spare1},
		drx-RetransmissionTimer				ENUMERATED {
												psf1, psf2, psf4, psf6, psf8, psf16,
												psf24, psf33},
		longDRX-CycleStartOffset		CHOICE {
			sf10							INTEGER(0..9),
			sf20							INTEGER(0..19),
			sf32							INTEGER(0..31),
			sf40							INTEGER(0..39),
			sf64							INTEGER(0..63),
			sf80							INTEGER(0..79),
			sf128							INTEGER(0..127),
			sf160							INTEGER(0..159),
			sf256							INTEGER(0..255),
			sf320							INTEGER(0..319),
			sf512							INTEGER(0..511),
			sf640							INTEGER(0..639),
			sf1024							INTEGER(0..1023),
			sf1280							INTEGER(0..1279),
			sf2048							INTEGER(0..2047),
			sf2560							INTEGER(0..2559)
		},
		shortDRX							SEQUENCE {
			shortDRX-Cycle						ENUMERATED	{
													sf2, sf5, sf8, sf10, sf16, sf20,
													sf32, sf40, sf64, sf80, sf128, sf160,
													sf256, sf320, sf512, sf640},
			drxShortCycleTimer					INTEGER (1..16)
		}		OPTIONAL													-- Need OR
	}
}


PDCP-Config ::=						SEQUENCE {
	discardTimer						ENUMERATED {
											ms50, ms100, ms150, ms300, ms500,
											ms750, ms1500, infinity
	}															OPTIONAL,			-- Cond Setup
	rlc-AM								SEQUENCE {
		statusReportRequired				BOOLEAN
	}															OPTIONAL,			-- Cond Rlc-AM
	rlc-UM								SEQUENCE {
		pdcp-SN-Size						ENUMERATED {len7bits, len12bits}
	}															OPTIONAL,			-- Cond Rlc-UM
	headerCompression					CHOICE {
		notUsed								NULL,
		rohc								SEQUENCE {
			maxCID								INTEGER (1..16383)				DEFAULT 15,
			profiles							SEQUENCE {
				profile0x0001						BOOLEAN,
				profile0x0002						BOOLEAN,
				profile0x0003						BOOLEAN,
				profile0x0004						BOOLEAN,
				profile0x0006						BOOLEAN,
				profile0x0101						BOOLEAN,
				profile0x0102						BOOLEAN,
				profile0x0103						BOOLEAN,
				profile0x0104						BOOLEAN
			},
			...
		}
	},
	...
}


PDSCH-ConfigCommon ::=		SEQUENCE {
	referenceSignalPower				INTEGER (-60..50),
	p-b									INTEGER (0..3)
}

PDSCH-ConfigDedicated::=		SEQUENCE {
	p-a									ENUMERATED {
											dB-6, dB-4dot77, dB-3, dB-1dot77,
											dB0, dB1, dB2, dB3}
}


PHICH-Config ::=					SEQUENCE {
	phich-Duration						ENUMERATED {normal, extended},
	phich-Resource						ENUMERATED {oneSixth, half, one, two}
}


PhysicalConfigDedicated ::=		SEQUENCE {
	pdsch-ConfigDedicated				PDSCH-ConfigDedicated			OPTIONAL,		-- Need ON
	pucch-ConfigDedicated				PUCCH-ConfigDedicated			OPTIONAL,		-- Need ON
	pusch-ConfigDedicated				PUSCH-ConfigDedicated			OPTIONAL,		-- Need ON
	uplinkPowerControlDedicated		UplinkPowerControlDedicated		OPTIONAL,		-- Need ON
	tpc-PDCCH-ConfigPUCCH				TPC-PDCCH-Config 				OPTIONAL,		-- Need ON
	tpc-PDCCH-ConfigPUSCH				TPC-PDCCH-Config 				OPTIONAL,		-- Need ON
	cqi-ReportConfig					CQI-ReportConfig				OPTIONAL,		-- Need ON
	soundingRS-UL-ConfigDedicated		SoundingRS-UL-ConfigDedicated	OPTIONAL,		-- Need ON
	antennaInfo							CHOICE {
		explicitValue						AntennaInfoDedicated,
		defaultValue						NULL
	}		OPTIONAL,																	-- Need ON
	schedulingRequestConfig			SchedulingRequestConfig		OPTIONAL, 			-- Need ON
	...,
	[[	cqi-ReportConfig-v920				CQI-ReportConfig-v920		OPTIONAL,		-- Need ON
		antennaInfo-v920					AntennaInfoDedicated-v920	OPTIONAL		-- Need ON
	]]
}


P-Max ::=				INTEGER (-30..33)


PRACH-ConfigSIB ::=				SEQUENCE {
	rootSequenceIndex					INTEGER (0..837),
	prach-ConfigInfo					PRACH-ConfigInfo
}

PRACH-Config ::=					SEQUENCE {
	rootSequenceIndex					INTEGER (0..837),
	prach-ConfigInfo					PRACH-ConfigInfo					OPTIONAL	-- Need ON
}

PRACH-ConfigInfo ::=				SEQUENCE {
	prach-ConfigIndex					INTEGER (0..63),
	highSpeedFlag						BOOLEAN,
	zeroCorrelationZoneConfig			INTEGER (0..15),
	prach-FreqOffset					INTEGER (0..94)
}


PresenceAntennaPort1 ::=				BOOLEAN


PUCCH-ConfigCommon ::=				SEQUENCE {
	deltaPUCCH-Shift					ENUMERATED {ds1, ds2, ds3},
	nRB-CQI								INTEGER (0..98),
	nCS-AN								INTEGER (0..7),
	n1PUCCH-AN							INTEGER (0..2047)
}

PUCCH-ConfigDedicated ::=			SEQUENCE {
	ackNackRepetition					CHOICE{
		release								NULL,
		setup								SEQUENCE {
			repetitionFactor					ENUMERATED {n2, n4, n6, spare1},
			n1PUCCH-AN-Rep						INTEGER (0..2047)
		}
	},
	tdd-AckNackFeedbackMode				ENUMERATED {bundling, multiplexing}	OPTIONAL	-- Cond TDD
}


PUSCH-ConfigCommon ::=				SEQUENCE {
	pusch-ConfigBasic					SEQUENCE {
		n-SB								INTEGER (1..4),
		hoppingMode							ENUMERATED {interSubFrame, intraAndInterSubFrame},
		pusch-HoppingOffset					INTEGER (0..98),
		enable64QAM							BOOLEAN
	},
	ul-ReferenceSignalsPUSCH			UL-ReferenceSignalsPUSCH
}

PUSCH-ConfigDedicated ::=			SEQUENCE {
	betaOffset-ACK-Index					INTEGER (0..15),
	betaOffset-RI-Index					INTEGER (0..15),
	betaOffset-CQI-Index					INTEGER (0..15)
}

UL-ReferenceSignalsPUSCH ::=		SEQUENCE {
	groupHoppingEnabled					BOOLEAN,
	groupAssignmentPUSCH				INTEGER (0..29),
	sequenceHoppingEnabled				BOOLEAN,
	cyclicShift							INTEGER (0..7)
}


RACH-ConfigCommon ::=		SEQUENCE {
	preambleInfo						SEQUENCE {
		numberOfRA-Preambles				ENUMERATED {
												n4, n8, n12, n16 ,n20, n24, n28,
												n32, n36, n40, n44, n48, n52, n56,
												n60, n64},
		preamblesGroupAConfig				SEQUENCE {
			sizeOfRA-PreamblesGroupA			ENUMERATED {
													n4, n8, n12, n16 ,n20, n24, n28,
													n32, n36, n40, n44, n48, n52, n56,
													n60},
			messageSizeGroupA					ENUMERATED {b56, b144, b208, b256},
			messagePowerOffsetGroupB			ENUMERATED {
													minusinfinity, dB0, dB5, dB8, dB10, dB12,
													dB15, dB18},
			...
		}			OPTIONAL													-- Need OP
	},
	powerRampingParameters				SEQUENCE {
		powerRampingStep					ENUMERATED {dB0, dB2,dB4, dB6},
		preambleInitialReceivedTargetPower	ENUMERATED {
												dBm-120, dBm-118, dBm-116, dBm-114, dBm-112,
												dBm-110, dBm-108, dBm-106, dBm-104, dBm-102,
												dBm-100, dBm-98, dBm-96, dBm-94,
												dBm-92, dBm-90}
	},
	ra-SupervisionInfo					SEQUENCE {
		preambleTransMax					ENUMERATED {
												n3, n4, n5, n6, n7,	n8, n10, n20, n50,
												n100, n200},
		ra-ResponseWindowSize				ENUMERATED {
												sf2, sf3, sf4, sf5, sf6, sf7,
												sf8, sf10},
		mac-ContentionResolutionTimer		ENUMERATED {
												sf8, sf16, sf24, sf32, sf40, sf48,
												sf56, sf64}
	},
	maxHARQ-Msg3Tx						INTEGER (1..8),
	...
}


RACH-ConfigDedicated ::=		SEQUENCE {
	ra-PreambleIndex					INTEGER (0..63),
	ra-PRACH-MaskIndex					INTEGER (0..15)
}


RadioResourceConfigCommonSIB ::=	SEQUENCE {
	rach-ConfigCommon					RACH-ConfigCommon,
	bcch-Config 						BCCH-Config,
	pcch-Config 						PCCH-Config,
	prach-Config						PRACH-ConfigSIB,
	pdsch-ConfigCommon					PDSCH-ConfigCommon,
	pusch-ConfigCommon					PUSCH-ConfigCommon,
	pucch-ConfigCommon					PUCCH-ConfigCommon,
	soundingRS-UL-ConfigCommon			SoundingRS-UL-ConfigCommon,
	uplinkPowerControlCommon			UplinkPowerControlCommon,
	ul-CyclicPrefixLength				UL-CyclicPrefixLength,
	...
}

RadioResourceConfigCommon ::=		SEQUENCE {
	rach-ConfigCommon					RACH-ConfigCommon					OPTIONAL,	-- Need ON
	prach-Config						PRACH-Config,
	pdsch-ConfigCommon					PDSCH-ConfigCommon					OPTIONAL,	-- Need ON
	pusch-ConfigCommon					PUSCH-ConfigCommon,
	phich-Config						PHICH-Config						OPTIONAL,	-- Need ON
	pucch-ConfigCommon					PUCCH-ConfigCommon					OPTIONAL,	-- Need ON
	soundingRS-UL-ConfigCommon			SoundingRS-UL-ConfigCommon			OPTIONAL,	-- Need ON
	uplinkPowerControlCommon			UplinkPowerControlCommon			OPTIONAL,	-- Need ON
	antennaInfoCommon					AntennaInfoCommon			OPTIONAL,	-- Need ON
	p-Max								P-Max								OPTIONAL,	-- Need OP
	tdd-Config							TDD-Config							OPTIONAL,	-- Cond TDD
	ul-CyclicPrefixLength				UL-CyclicPrefixLength,
	...
}

BCCH-Config ::=						SEQUENCE {
	modificationPeriodCoeff				ENUMERATED {n2, n4, n8, n16}
}

PCCH-Config ::=						SEQUENCE {
	defaultPagingCycle					ENUMERATED {
											rf32, rf64, rf128, rf256},
	nB									ENUMERATED {
											fourT, twoT, oneT, halfT, quarterT, oneEighthT,
											oneSixteenthT, oneThirtySecondT}
}

UL-CyclicPrefixLength ::=			ENUMERATED {len1, len2}


RadioResourceConfigDedicated ::=		SEQUENCE {
	srb-ToAddModList					SRB-ToAddModList			OPTIONAL, 		-- Cond HO-Conn
	drb-ToAddModList					DRB-ToAddModList			OPTIONAL, 		-- Cond HO-toEUTRA
	drb-ToReleaseList					DRB-ToReleaseList			OPTIONAL, 		-- Need ON
	mac-MainConfig						CHOICE {
			explicitValue					MAC-MainConfig,
			defaultValue					NULL
	}		OPTIONAL,																-- Cond HO-toEUTRA2
	sps-Config							SPS-Config 					OPTIONAL,		-- Need ON
	physicalConfigDedicated				PhysicalConfigDedicated		OPTIONAL,		-- Need ON
	...,
	[[	rlf-TimersAndConstants-r9			RLF-TimersAndConstants-r9		OPTIONAL	-- Need ON
	]]
}

SRB-ToAddModList ::=				SEQUENCE (SIZE (1..2)) OF SRB-ToAddMod

SRB-ToAddMod ::=	SEQUENCE {
	srb-Identity						INTEGER (1..2),
	rlc-Config							CHOICE {
		explicitValue						RLC-Config,
		defaultValue						NULL
	}		OPTIONAL,																-- Cond Setup
	logicalChannelConfig				CHOICE {
		explicitValue						LogicalChannelConfig,
		defaultValue						NULL
	}		OPTIONAL,																-- Cond Setup
	...
}

DRB-ToAddModList ::=				SEQUENCE (SIZE (1..maxDRB)) OF DRB-ToAddMod

DRB-ToAddMod ::=	SEQUENCE {
	eps-BearerIdentity					INTEGER (0..15)			OPTIONAL,		-- Cond DRB-Setup
	drb-Identity						DRB-Identity,
	pdcp-Config							PDCP-Config				OPTIONAL,		-- Cond PDCP
	rlc-Config							RLC-Config				OPTIONAL,		-- Cond Setup
	logicalChannelIdentity				INTEGER (3..10)			OPTIONAL,		-- Cond DRB-Setup
	logicalChannelConfig				LogicalChannelConfig	OPTIONAL,		-- Cond Setup
	...
}

DRB-ToReleaseList ::=				SEQUENCE (SIZE (1..maxDRB)) OF DRB-Identity


RLC-Config ::=				CHOICE {
	am									SEQUENCE {
		ul-AM-RLC							UL-AM-RLC,
		dl-AM-RLC							DL-AM-RLC
	},
	um-Bi-Directional					SEQUENCE {
		ul-UM-RLC							UL-UM-RLC,
		dl-UM-RLC							DL-UM-RLC
	},
	um-Uni-Directional-UL				SEQUENCE {
		ul-UM-RLC							UL-UM-RLC
	},
	um-Uni-Directional-DL				SEQUENCE {
		dl-UM-RLC							DL-UM-RLC
	},
	...
}

UL-AM-RLC ::=						SEQUENCE {
	t-PollRetransmit					T-PollRetransmit,
	pollPDU								PollPDU,
	pollByte							PollByte,
	maxRetxThreshold					ENUMERATED {
											t1, t2, t3, t4, t6, t8, t16, t32}
}

DL-AM-RLC ::=						SEQUENCE {
	t-Reordering						T-Reordering,
	t-StatusProhibit					T-StatusProhibit
}

UL-UM-RLC ::=						SEQUENCE {
	sn-FieldLength						SN-FieldLength
}

DL-UM-RLC ::=						SEQUENCE {
	sn-FieldLength						SN-FieldLength,
	t-Reordering						T-Reordering
}

SN-FieldLength ::=					ENUMERATED {size5, size10}

T-PollRetransmit ::=				ENUMERATED {
										ms5, ms10, ms15, ms20, ms25, ms30, ms35,
										ms40, ms45, ms50, ms55, ms60, ms65, ms70,
										ms75, ms80, ms85, ms90, ms95, ms100, ms105,
										ms110, ms115, ms120, ms125, ms130, ms135,
										ms140, ms145, ms150, ms155, ms160, ms165,
										ms170, ms175, ms180, ms185, ms190, ms195,
										ms200, ms205, ms210, ms215, ms220, ms225,
										ms230, ms235, ms240, ms245, ms250, ms300,
										ms350, ms400, ms450, ms500, spare9, spare8,
										spare7, spare6, spare5, spare4, spare3,
										spare2, spare1}

PollPDU ::=							ENUMERATED {
										p4, p8, p16, p32, p64, p128, p256, pInfinity}

PollByte ::=						ENUMERATED {
										kB25, kB50, kB75, kB100, kB125, kB250, kB375,
										kB500, kB750, kB1000, kB1250, kB1500, kB2000,
										kB3000, kBinfinity, spare1}

T-Reordering ::=					ENUMERATED {
										ms0, ms5, ms10, ms15, ms20, ms25, ms30, ms35,
										ms40, ms45, ms50, ms55, ms60, ms65, ms70,
										ms75, ms80, ms85, ms90, ms95, ms100, ms110,
										ms120, ms130, ms140, ms150, ms160, ms170,
										ms180, ms190, ms200, spare1}

T-StatusProhibit ::=				ENUMERATED {
										ms0, ms5, ms10, ms15, ms20, ms25, ms30, ms35,
										ms40, ms45, ms50, ms55, ms60, ms65, ms70,
										ms75, ms80, ms85, ms90, ms95, ms100, ms105,
										ms110, ms115, ms120, ms125, ms130, ms135,
										ms140, ms145, ms150, ms155, ms160, ms165,
										ms170, ms175, ms180, ms185, ms190, ms195,
										ms200, ms205, ms210, ms215, ms220, ms225,
										ms230, ms235, ms240, ms245, ms250, ms300,
										ms350, ms400, ms450, ms500, spare8, spare7,
										spare6, spare5, spare4, spare3, spare2,
										spare1}


RLF-TimersAndConstants-r9 ::=			CHOICE {
	release									NULL,
	setup									SEQUENCE {
		t301-r9								ENUMERATED {
												ms100, ms200, ms300, ms400, ms600, ms1000, ms1500,
												ms2000},
		t310-r9								ENUMERATED {
												ms0, ms50, ms100, ms200, ms500, ms1000, ms2000},
		n310-r9								ENUMERATED {
												n1, n2, n3, n4, n6, n8, n10, n20},
		t311-r9								ENUMERATED {
												ms1000, ms3000, ms5000, ms10000, ms15000,
												ms20000, ms30000},
		n311-r9								ENUMERATED {
												n1, n2, n3, n4, n5, n6, n8, n10},
		...
	}
}


SchedulingRequestConfig ::=		CHOICE {
	release								NULL,
	setup								SEQUENCE {
		sr-PUCCH-ResourceIndex				INTEGER (0..2047),
		sr-ConfigIndex						INTEGER (0..157),
		dsr-TransMax						ENUMERATED {
												n4, n8, n16, n32, n64, spare3, spare2, spare1}
	}
}


SoundingRS-UL-ConfigCommon ::=		CHOICE {
	release								NULL,
	setup								SEQUENCE {
		srs-BandwidthConfig					ENUMERATED {bw0, bw1, bw2, bw3, bw4, bw5, bw6, bw7},
		srs-SubframeConfig					ENUMERATED {
												sc0, sc1, sc2, sc3, sc4, sc5, sc6, sc7,
												sc8, sc9, sc10, sc11, sc12, sc13, sc14, sc15},
		ackNackSRS-SimultaneousTransmission	BOOLEAN,
		srs-MaxUpPts						ENUMERATED {true}			OPTIONAL	-- Cond TDD
	}
}

SoundingRS-UL-ConfigDedicated ::=	CHOICE{
	release								NULL,
	setup								SEQUENCE {
		srs-Bandwidth						ENUMERATED {bw0, bw1, bw2, bw3},
		srs-HoppingBandwidth				ENUMERATED {hbw0, hbw1, hbw2, hbw3},
		freqDomainPosition					INTEGER (0..23),
		duration							BOOLEAN,
		srs-ConfigIndex						INTEGER (0..1023),
		transmissionComb					INTEGER (0..1),
		cyclicShift							ENUMERATED {cs0, cs1, cs2, cs3, cs4, cs5, cs6, cs7}
	}
}



SPS-Config ::=	SEQUENCE {
	semiPersistSchedC-RNTI			C-RNTI					OPTIONAL,			-- Need OR
	sps-ConfigDL					SPS-ConfigDL			OPTIONAL,			-- Need ON
	sps-ConfigUL					SPS-ConfigUL			OPTIONAL			-- Need ON
}

SPS-ConfigDL ::=	CHOICE{
	release							NULL,
	setup							SEQUENCE {
		semiPersistSchedIntervalDL			ENUMERATED {
												sf10, sf20, sf32, sf40, sf64, sf80,
												sf128, sf160, sf320, sf640, spare6,
												spare5, spare4, spare3, spare2,
												spare1},
		numberOfConfSPS-Processes			INTEGER (1..8),
		n1-PUCCH-AN-PersistentList			N1-PUCCH-AN-PersistentList,
		...
	}
}

SPS-ConfigUL ::=	CHOICE {
	release							NULL,
	setup							SEQUENCE {
		semiPersistSchedIntervalUL			ENUMERATED {
												sf10, sf20, sf32, sf40, sf64, sf80,
												sf128, sf160, sf320, sf640, spare6,
												spare5, spare4, spare3, spare2,
												spare1},
		implicitReleaseAfter				ENUMERATED {e2, e3, e4, e8},
		p0-Persistent						SEQUENCE {
			p0-NominalPUSCH-Persistent			INTEGER (-126..24),
			p0-UE-PUSCH-Persistent				INTEGER (-8..7)
		}		OPTIONAL,												-- Need OP
		twoIntervalsConfig					ENUMERATED {true}			OPTIONAL,	-- Cond TDD
		...
	}
}

N1-PUCCH-AN-PersistentList ::=		SEQUENCE (SIZE (1..4)) OF INTEGER (0..2047)


TDD-Config ::=						SEQUENCE {
	subframeAssignment					ENUMERATED {
											sa0, sa1, sa2, sa3, sa4, sa5, sa6},
	specialSubframePatterns				ENUMERATED {
											ssp0, ssp1, ssp2, ssp3, ssp4,ssp5, ssp6, ssp7,
											ssp8}
}


TimeAlignmentTimer ::=					ENUMERATED {
												sf500, sf750, sf1280, sf1920, sf2560, sf5120,
												sf10240, infinity}

TPC-PDCCH-Config ::=					CHOICE {
	release								NULL,
	setup								SEQUENCE {
		tpc-RNTI							BIT STRING (SIZE (16)),
		tpc-Index							TPC-Index
	}
}

TPC-Index ::=							CHOICE {
	indexOfFormat3							INTEGER (1..15),
	indexOfFormat3A							INTEGER (1..31)
}


UplinkPowerControlCommon ::=		SEQUENCE {
	p0-NominalPUSCH						INTEGER (-126..24),
	alpha								ENUMERATED {al0, al04, al05, al06, al07, al08, al09, al1},
	p0-NominalPUCCH						INTEGER (-127..-96),
	deltaFList-PUCCH					DeltaFList-PUCCH,
	deltaPreambleMsg3					INTEGER (-1..6)
}

UplinkPowerControlDedicated ::=		SEQUENCE {
	p0-UE-PUSCH							INTEGER (-8..7),
	deltaMCS-Enabled					ENUMERATED {en0, en1},
	accumulationEnabled					BOOLEAN,
	p0-UE-PUCCH							INTEGER (-8..7),
	pSRS-Offset							INTEGER (0..15),
	filterCoefficient					FilterCoefficient					DEFAULT fc4
}

DeltaFList-PUCCH ::=				SEQUENCE {
	deltaF-PUCCH-Format1				ENUMERATED {deltaF-2, deltaF0, deltaF2},
	deltaF-PUCCH-Format1b				ENUMERATED {deltaF1, deltaF3, deltaF5},
	deltaF-PUCCH-Format2				ENUMERATED {deltaF-2, deltaF0, deltaF1, deltaF2},
	deltaF-PUCCH-Format2a				ENUMERATED {deltaF-2, deltaF0, deltaF2},
	deltaF-PUCCH-Format2b				ENUMERATED {deltaF-2, deltaF0, deltaF2}
}


NextHopChainingCount ::=					INTEGER (0..7)


SecurityAlgorithmConfig ::=			SEQUENCE {
	cipheringAlgorithm					ENUMERATED {
											eea0, eea1, eea2, spare5, spare4, spare3,
											spare2, spare1, ...},
	integrityProtAlgorithm				ENUMERATED {
											eia0-v920, eia1, eia2, spare5, spare4, spare3,
											spare2, spare1, ...}
}


ShortMAC-I ::=						BIT STRING (SIZE (16))


AdditionalSpectrumEmission ::=		INTEGER (1..32)


ARFCN-ValueCDMA2000 ::=			INTEGER (0..2047)


ARFCN-ValueEUTRA ::=				INTEGER (0..maxEARFCN)

ARFCN-ValueEUTRA-v9e0 ::=			INTEGER (maxEARFCN-Plus1..maxEARFCN2)

ARFCN-ValueEUTRA-r9 ::=			INTEGER (0..maxEARFCN2)


ARFCN-ValueGERAN ::=			INTEGER (0..1023)


ARFCN-ValueUTRA ::=					INTEGER (0..16383)


BandclassCDMA2000 ::=					ENUMERATED {
											bc0, bc1, bc2, bc3, bc4, bc5, bc6, bc7, bc8,
											bc9, bc10, bc11, bc12, bc13, bc14, bc15, bc16,
											bc17, bc18-v9a0, bc19-v9a0, bc20-v9a0, bc21-v9a0,
											spare10, spare9, spare8, spare7, spare6, spare5, spare4,
											spare3, spare2, spare1, ...}


BandIndicatorGERAN ::=			ENUMERATED {dcs1800, pcs1900}


CarrierFreqCDMA2000 ::=			SEQUENCE {
	bandClass							BandclassCDMA2000,
	arfcn							ARFCN-ValueCDMA2000
}


CarrierFreqGERAN ::=			SEQUENCE {
	arfcn							ARFCN-ValueGERAN,
	bandIndicator					BandIndicatorGERAN
}


CarrierFreqsGERAN ::=			SEQUENCE {
	startingARFCN						ARFCN-ValueGERAN,
	bandIndicator						BandIndicatorGERAN,
	followingARFCNs						CHOICE {
		explicitListOfARFCNs				ExplicitListOfARFCNs,
		equallySpacedARFCNs					SEQUENCE {
			arfcn-Spacing						INTEGER (1..8),
			numberOfFollowingARFCNs				INTEGER (0..31)
		},
		variableBitMapOfARFCNs				OCTET STRING (SIZE (1..16))
	}
}

ExplicitListOfARFCNs ::=			SEQUENCE (SIZE (0..31)) OF ARFCN-ValueGERAN


CDMA2000-Type ::=					ENUMERATED {type1XRTT, typeHRPD}


CellIdentity ::=					BIT STRING (SIZE (28))


CellIndexList ::=						SEQUENCE (SIZE (1..maxCellMeas)) OF CellIndex

CellIndex ::=							INTEGER (1..maxCellMeas)


CellReselectionPriority ::=				INTEGER (0..7)


CSFB-RegistrationParam1XRTT ::=		SEQUENCE {
	sid									BIT STRING (SIZE (15)),
	nid									BIT STRING (SIZE (16)),
	multipleSID							BOOLEAN,
	multipleNID							BOOLEAN,
	homeReg								BOOLEAN,
	foreignSIDReg						BOOLEAN,
	foreignNIDReg						BOOLEAN,
	parameterReg						BOOLEAN,
	powerUpReg							BOOLEAN,
	registrationPeriod					BIT STRING (SIZE (7)),
	registrationZone					BIT STRING (SIZE (12)),
	totalZone							BIT STRING (SIZE (3)),
	zoneTimer							BIT STRING (SIZE (3))
}

CSFB-RegistrationParam1XRTT-v920 ::=	SEQUENCE {
	powerDownReg-r9						ENUMERATED {true}
}


CellGlobalIdEUTRA ::=					SEQUENCE {
	plmn-Identity							PLMN-Identity,
	cellIdentity							CellIdentity
}


CellGlobalIdUTRA ::=					SEQUENCE {
	plmn-Identity							PLMN-Identity,
	cellIdentity							BIT STRING (SIZE (28))
}


CellGlobalIdGERAN ::=					SEQUENCE {
	plmn-Identity							PLMN-Identity,
	locationAreaCode						BIT STRING (SIZE (16)),
	cellIdentity						BIT STRING (SIZE (16))
}


CellGlobalIdCDMA2000 ::=				CHOICE {
	cellGlobalId1XRTT						BIT STRING (SIZE (47)),
	cellGlobalIdHRPD						BIT STRING (SIZE (128))
}


CSG-Identity ::=					BIT STRING (SIZE (27))


FreqBandIndicator ::=					INTEGER (1..maxFBI)

FreqBandIndicator-v9e0 ::=				INTEGER (maxFBI-Plus1..maxFBI2)


MobilityControlInfo ::=		SEQUENCE {
	targetPhysCellId					PhysCellId,
	carrierFreq							CarrierFreqEUTRA					OPTIONAL,	-- Cond HO-toEUTRA2
	carrierBandwidth					CarrierBandwidthEUTRA				OPTIONAL,	-- Cond HO-toEUTRA
	additionalSpectrumEmission			AdditionalSpectrumEmission			OPTIONAL,	-- Cond HO-toEUTRA
	t304								ENUMERATED {
											ms50, ms100, ms150, ms200, ms500, ms1000,
											ms2000, spare1},
	newUE-Identity						C-RNTI,
	radioResourceConfigCommon			RadioResourceConfigCommon,
	rach-ConfigDedicated				RACH-ConfigDedicated				OPTIONAL,	-- Need OP
	...,
	[[	carrierFreq-v9e0				CarrierFreqEUTRA-v9e0				OPTIONAL	-- Need ON
	]]
}

CarrierBandwidthEUTRA ::=			SEQUENCE {
	dl-Bandwidth						ENUMERATED {
												n6, n15, n25, n50, n75, n100, spare10,
												spare9, spare8, spare7, spare6, spare5,
												spare4, spare3, spare2, spare1},
	ul-Bandwidth						ENUMERATED {
												n6, n15, n25, n50, n75, n100, spare10,
												spare9, spare8, spare7, spare6, spare5,
												spare4, spare3, spare2, spare1}	OPTIONAL -- Need OP
}

CarrierFreqEUTRA ::=				SEQUENCE {
	dl-CarrierFreq						ARFCN-ValueEUTRA,
	ul-CarrierFreq						ARFCN-ValueEUTRA				OPTIONAL	-- Cond FDD
}

CarrierFreqEUTRA-v9e0 ::=			SEQUENCE {
	dl-CarrierFreq-v9e0					ARFCN-ValueEUTRA-r9,
	ul-CarrierFreq-v9e0					ARFCN-ValueEUTRA-r9			OPTIONAL	-- Cond FDD
}


MobilityParametersCDMA2000 ::=			OCTET STRING


MobilityStateParameters ::=			SEQUENCE {
	t-Evaluation						ENUMERATED {
											s30, s60, s120, s180, s240, spare3, spare2, spare1},
	t-HystNormal						ENUMERATED {
											s30, s60, s120, s180, s240, spare3, spare2, spare1},
	n-CellChangeMedium					INTEGER (1..16),
	n-CellChangeHigh					INTEGER (1..16)
}


MultiBandInfoList ::=	SEQUENCE (SIZE (1..maxMultiBands)) OF FreqBandIndicator

MultiBandInfoList-v9e0 ::=	SEQUENCE (SIZE (1..maxMultiBands)) OF MultiBandInfo-v9e0

MultiBandInfo-v9e0 ::=		SEQUENCE {
	freqBandIndicator-v9e0				FreqBandIndicator-v9e0		OPTIONAL	-- Need OP
}


PhysCellId ::=						INTEGER (0..503)


PhysCellIdRange ::=				SEQUENCE {
	start							PhysCellId,
	range							ENUMERATED {
										n4, n8, n12, n16, n24, n32, n48, n64, n84,
										n96, n128, n168, n252, n504, spare2,
										spare1} 					OPTIONAL	-- Need OP
}


PhysCellIdRangeUTRA-FDDList-r9::=		SEQUENCE (SIZE (1.. maxPhysCellIdRange-r9)) OF PhysCellIdRangeUTRA-FDD-r9

PhysCellIdRangeUTRA-FDD-r9 ::=			SEQUENCE {
		start-r9							PhysCellIdUTRA-FDD,
		range-r9							INTEGER (2..512)				OPTIONAL	-- Need OP
}


PhysCellIdCDMA2000 ::=			INTEGER (0..maxPNOffset)


PhysCellIdGERAN ::=				SEQUENCE {
	networkColourCode					BIT STRING (SIZE (3)),
	baseStationColourCode				BIT STRING (SIZE (3))
}


PhysCellIdUTRA-FDD ::=				INTEGER (0..511)


PhysCellIdUTRA-TDD ::=				INTEGER (0..127)


PLMN-Identity ::=					SEQUENCE {
	mcc									MCC					OPTIONAL,					-- Cond MCC
	mnc									MNC
}

MCC ::=								SEQUENCE (SIZE (3)) OF
											MCC-MNC-Digit

MNC ::=								SEQUENCE (SIZE (2..3)) OF
											MCC-MNC-Digit

MCC-MNC-Digit ::=					INTEGER (0..9)



PreRegistrationInfoHRPD ::=			SEQUENCE {
	preRegistrationAllowed				BOOLEAN,
	preRegistrationZoneId				PreRegistrationZoneIdHRPD	OPTIONAL, -- cond PreRegAllowed
	secondaryPreRegistrationZoneIdList	SecondaryPreRegistrationZoneIdListHRPD	OPTIONAL -- Need OR
}

SecondaryPreRegistrationZoneIdListHRPD ::=	SEQUENCE (SIZE (1..2)) OF PreRegistrationZoneIdHRPD

PreRegistrationZoneIdHRPD ::=			INTEGER (0..255)


Q-QualMin-r9 ::=					INTEGER (-34..-3)


Q-RxLevMin ::=						INTEGER (-70..-22)


Q-OffsetRange ::=						ENUMERATED {
												dB-24, dB-22, dB-20, dB-18, dB-16, dB-14,
												dB-12, dB-10, dB-8, dB-6, dB-5, dB-4, dB-3,
												dB-2, dB-1, dB0, dB1, dB2, dB3, dB4, dB5,
												dB6, dB8, dB10, dB12, dB14, dB16, dB18,
												dB20, dB22, dB24}


Q-OffsetRangeInterRAT ::=					INTEGER (-15..15)


ReselectionThreshold ::=				INTEGER (0..31)


ReselectionThresholdQ-r9 ::=			INTEGER (0..31)


SpeedStateScaleFactors ::=			SEQUENCE {
	sf-Medium							ENUMERATED {oDot25, oDot5, oDot75, lDot0},
	sf-High								ENUMERATED {oDot25, oDot5, oDot75, lDot0}
}

SystemInfoListGERAN ::=				SEQUENCE (SIZE (1..maxGERAN-SI)) OF
										OCTET STRING (SIZE (1..23))


SystemTimeInfoCDMA2000 ::=			SEQUENCE {
	cdma-EUTRA-Synchronisation			BOOLEAN,
	cdma-SystemTime						CHOICE {
		synchronousSystemTime				BIT STRING (SIZE (39)),
		asynchronousSystemTime				BIT STRING (SIZE (49))
	}
}


TrackingAreaCode ::=				BIT STRING (SIZE (16))


T-Reselection ::=					INTEGER (0..7)


AllowedMeasBandwidth ::=				ENUMERATED {mbw6, mbw15, mbw25, mbw50, mbw75, mbw100}


Hysteresis ::=							INTEGER (0..30)


MeasConfig ::=						SEQUENCE {
	-- Measurement objects
	measObjectToRemoveList				MeasObjectToRemoveList				OPTIONAL,	-- Need ON
	measObjectToAddModList				MeasObjectToAddModList				OPTIONAL,	-- Need ON
	-- Reporting configurations
	reportConfigToRemoveList			ReportConfigToRemoveList			OPTIONAL,	-- Need ON
	reportConfigToAddModList			ReportConfigToAddModList			OPTIONAL,	-- Need ON
	-- Measurement identities
	measIdToRemoveList					MeasIdToRemoveList					OPTIONAL,	-- Need ON
	measIdToAddModList					MeasIdToAddModList					OPTIONAL,	-- Need ON
	-- Other parameters
	quantityConfig						QuantityConfig						OPTIONAL,	-- Need ON
	measGapConfig						MeasGapConfig						OPTIONAL,	-- Need ON
	s-Measure							RSRP-Range							OPTIONAL,	-- Need ON
	preRegistrationInfoHRPD				PreRegistrationInfoHRPD				OPTIONAL, 	-- Need OP
	speedStatePars			CHOICE {
		release								NULL,
		setup								SEQUENCE {
			mobilityStateParameters				MobilityStateParameters,
			timeToTrigger-SF					SpeedStateScaleFactors
		}
	}																		OPTIONAL,	-- Need ON
	...,
	[[	measObjectToAddModList-v9e0			MeasObjectToAddModList-v9e0		OPTIONAL	-- Need ON
	]]
}

MeasIdToRemoveList ::=				SEQUENCE (SIZE (1..maxMeasId)) OF MeasId

MeasObjectToRemoveList ::=			SEQUENCE (SIZE (1..maxObjectId)) OF MeasObjectId

ReportConfigToRemoveList ::=		SEQUENCE (SIZE (1..maxReportConfigId)) OF ReportConfigId


MeasGapConfig ::=					CHOICE {
	release								NULL,
	setup								SEQUENCE {
		gapOffset							CHOICE {
				gp0									INTEGER (0..39),
				gp1									INTEGER (0..79),
				...
		}
	}
}


MeasId ::=							INTEGER (1..maxMeasId)


MeasIdToAddModList ::=				SEQUENCE (SIZE (1..maxMeasId)) OF MeasIdToAddMod

MeasIdToAddMod ::=	SEQUENCE {
	measId								MeasId,
	measObjectId						MeasObjectId,
	reportConfigId						ReportConfigId
}


MeasObjectCDMA2000 ::=				SEQUENCE {
	cdma2000-Type						CDMA2000-Type,
	carrierFreq							CarrierFreqCDMA2000,
	searchWindowSize					INTEGER (0..15)						OPTIONAL,	-- Need ON
	offsetFreq							Q-OffsetRangeInterRAT				DEFAULT 0,
	cellsToRemoveList					CellIndexList						OPTIONAL,	-- Need ON
	cellsToAddModList					CellsToAddModListCDMA2000			OPTIONAL,	-- Need ON
	cellForWhichToReportCGI				PhysCellIdCDMA2000					OPTIONAL,	-- Need ON
	...
}

CellsToAddModListCDMA2000 ::=		SEQUENCE (SIZE (1..maxCellMeas)) OF CellsToAddModCDMA2000

CellsToAddModCDMA2000 ::=	SEQUENCE {
	cellIndex							INTEGER (1..maxCellMeas),
	physCellId							PhysCellIdCDMA2000
}


MeasObjectEUTRA ::=					SEQUENCE {
	carrierFreq							ARFCN-ValueEUTRA,
	allowedMeasBandwidth				AllowedMeasBandwidth,
	presenceAntennaPort1				PresenceAntennaPort1,
	neighCellConfig						NeighCellConfig,
	offsetFreq							Q-OffsetRange				DEFAULT dB0,
	-- Cell list
	cellsToRemoveList					CellIndexList				OPTIONAL,		-- Need ON
	cellsToAddModList					CellsToAddModList			OPTIONAL,		-- Need ON
	-- Black list
	blackCellsToRemoveList				CellIndexList				OPTIONAL,		-- Need ON
	blackCellsToAddModList				BlackCellsToAddModList		OPTIONAL,		-- Need ON
	cellForWhichToReportCGI				PhysCellId					OPTIONAL, 		-- Need ON
	...
}

MeasObjectEUTRA-v9e0 ::=			SEQUENCE {
	carrierFreq-v9e0					ARFCN-ValueEUTRA-v9e0
}

CellsToAddModList ::=				SEQUENCE (SIZE (1..maxCellMeas)) OF CellsToAddMod

CellsToAddMod ::=	SEQUENCE {
	cellIndex							INTEGER (1..maxCellMeas),
	physCellId							PhysCellId,
	cellIndividualOffset				Q-OffsetRange
}

BlackCellsToAddModList ::=			SEQUENCE (SIZE (1..maxCellMeas)) OF BlackCellsToAddMod

BlackCellsToAddMod ::=	SEQUENCE {
	cellIndex							INTEGER (1..maxCellMeas),
	physCellIdRange						PhysCellIdRange
}


MeasObjectGERAN ::=					SEQUENCE {
	carrierFreqs						CarrierFreqsGERAN,
	offsetFreq							Q-OffsetRangeInterRAT		DEFAULT 0,
	ncc-Permitted						BIT STRING(SIZE (8))		DEFAULT '11111111'B,
	cellForWhichToReportCGI				PhysCellIdGERAN				OPTIONAL, 	-- Need ON
	...
}


MeasObjectId ::=					INTEGER (1..maxObjectId)


MeasObjectToAddModList ::=			SEQUENCE (SIZE (1..maxObjectId)) OF MeasObjectToAddMod

MeasObjectToAddModList-v9e0 ::=		SEQUENCE (SIZE (1..maxObjectId)) OF MeasObjectToAddMod-v9e0

MeasObjectToAddMod ::=	SEQUENCE {
	measObjectId						MeasObjectId,
	measObject							CHOICE {
		measObjectEUTRA						MeasObjectEUTRA,
		measObjectUTRA						MeasObjectUTRA,
		measObjectGERAN						MeasObjectGERAN,
		measObjectCDMA2000					MeasObjectCDMA2000,
		...
	}
}

MeasObjectToAddMod-v9e0 ::=	SEQUENCE {
	measObjectEUTRA-v9e0				MeasObjectEUTRA-v9e0		OPTIONAL	-- Cond eutra
}


MeasObjectUTRA ::=					SEQUENCE {
	carrierFreq							ARFCN-ValueUTRA,
	offsetFreq							Q-OffsetRangeInterRAT		DEFAULT 0,
	cellsToRemoveList					CellIndexList				OPTIONAL,			-- Need ON
	cellsToAddModList					CHOICE {
		cellsToAddModListUTRA-FDD			CellsToAddModListUTRA-FDD,
		cellsToAddModListUTRA-TDD			CellsToAddModListUTRA-TDD
	}																OPTIONAL,			-- Need ON
	cellForWhichToReportCGI				CHOICE {
		utra-FDD							PhysCellIdUTRA-FDD,
		utra-TDD							PhysCellIdUTRA-TDD
	}																OPTIONAL, 	-- Need ON
	...,
	[[	csg-allowedReportingCells-v930			CSG-AllowedReportingCells-r9	OPTIONAL		-- Need ON
	]]
}

CellsToAddModListUTRA-FDD ::=		SEQUENCE (SIZE (1..maxCellMeas)) OF CellsToAddModUTRA-FDD

CellsToAddModUTRA-FDD ::=	SEQUENCE {
	cellIndex							INTEGER (1..maxCellMeas),
	physCellId							PhysCellIdUTRA-FDD
}

CellsToAddModListUTRA-TDD ::=		SEQUENCE (SIZE (1..maxCellMeas)) OF CellsToAddModUTRA-TDD

CellsToAddModUTRA-TDD ::=	SEQUENCE {
	cellIndex							INTEGER (1..maxCellMeas),
	physCellId							PhysCellIdUTRA-TDD
}

CSG-AllowedReportingCells-r9 ::=		SEQUENCE {
	physCellIdRangeUTRA-FDDList-r9			PhysCellIdRangeUTRA-FDDList-r9	OPTIONAL	-- Need OR
}

MeasResults ::=						SEQUENCE {
	measId								MeasId,
	measResultServCell					SEQUENCE {
		rsrpResult							RSRP-Range,
		rsrqResult							RSRQ-Range
	},
	measResultNeighCells				CHOICE {
		measResultListEUTRA					MeasResultListEUTRA,
		measResultListUTRA					MeasResultListUTRA,
		measResultListGERAN					MeasResultListGERAN,
		measResultsCDMA2000					MeasResultsCDMA2000,
		...
	}																		OPTIONAL,
	...,
	[[	measResultForECID-r9				MeasResultForECID-r9			OPTIONAL
	]]
}

MeasResultListEUTRA ::=				SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultEUTRA

MeasResultEUTRA ::=	SEQUENCE {
	physCellId							PhysCellId,
	cgi-Info							SEQUENCE {
		cellGlobalId						CellGlobalIdEUTRA,
		trackingAreaCode					TrackingAreaCode,
		plmn-IdentityList					PLMN-IdentityList2 				OPTIONAL
	}			 												OPTIONAL,
	measResult							SEQUENCE {
		rsrpResult							RSRP-Range						OPTIONAL,
		rsrqResult							RSRQ-Range						OPTIONAL,
		...,
		[[	additionalSI-Info-r9				AdditionalSI-Info-r9				OPTIONAL
		]]
	}
}

MeasResultListUTRA ::=				SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultUTRA

MeasResultUTRA ::=	SEQUENCE {
	physCellId							CHOICE {
		fdd									PhysCellIdUTRA-FDD,
		tdd									PhysCellIdUTRA-TDD
	},
	cgi-Info							SEQUENCE {
		cellGlobalId						CellGlobalIdUTRA,
		locationAreaCode					BIT STRING (SIZE (16))			OPTIONAL,
		routingAreaCode						BIT STRING (SIZE (8))			OPTIONAL,
		plmn-IdentityList					PLMN-IdentityList2 				OPTIONAL
	}			 												OPTIONAL,
	measResult							SEQUENCE {
		utra-RSCP							INTEGER (-5..91)				OPTIONAL,
		utra-EcN0							INTEGER (0..49)					OPTIONAL,
		...,
		[[	additionalSI-Info-r9				AdditionalSI-Info-r9				OPTIONAL
		]]
	}
}

MeasResultListGERAN ::=				SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultGERAN

MeasResultGERAN ::=	SEQUENCE {
	carrierFreq							CarrierFreqGERAN,
	physCellId							PhysCellIdGERAN,
	cgi-Info							SEQUENCE {
		cellGlobalId						CellGlobalIdGERAN,
		routingAreaCode						BIT STRING (SIZE (8))			OPTIONAL
	}			 															OPTIONAL,
	measResult							SEQUENCE {
		rssi								INTEGER (0..63),
		...
	}
}

MeasResultsCDMA2000 ::=				SEQUENCE {
	preRegistrationStatusHRPD			BOOLEAN,
	measResultListCDMA2000				MeasResultListCDMA2000
}

MeasResultListCDMA2000 ::=			SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultCDMA2000

MeasResultCDMA2000 ::=	SEQUENCE {
	physCellId							PhysCellIdCDMA2000,
	cgi-Info							CellGlobalIdCDMA2000		 		OPTIONAL,
	measResult							SEQUENCE {
		pilotPnPhase						INTEGER	(0..32767)				OPTIONAL,
		pilotStrength						INTEGER (0..63),
		...
	}
}

MeasResultForECID-r9 ::=		SEQUENCE {
	ue-RxTxTimeDiffResult-r9				INTEGER (0..4095),
	currentSFN-r9							BIT STRING (SIZE (10))
}

PLMN-IdentityList2 ::=				SEQUENCE (SIZE (1..5)) OF PLMN-Identity

AdditionalSI-Info-r9 ::=			SEQUENCE {
	csg-MemberStatus-r9				ENUMERATED {member}				OPTIONAL,
	csg-Identity-r9						CSG-Identity						OPTIONAL
}


QuantityConfig ::=					SEQUENCE {
	quantityConfigEUTRA					QuantityConfigEUTRA					OPTIONAL,	-- Need ON
	quantityConfigUTRA					QuantityConfigUTRA					OPTIONAL,	-- Need ON
	quantityConfigGERAN					QuantityConfigGERAN					OPTIONAL,	-- Need ON
	quantityConfigCDMA2000				QuantityConfigCDMA2000				OPTIONAL,	-- Need ON
	...
}

QuantityConfigEUTRA ::=				SEQUENCE {
	filterCoefficientRSRP				FilterCoefficient					DEFAULT fc4,
	filterCoefficientRSRQ				FilterCoefficient					DEFAULT fc4
}

QuantityConfigUTRA ::=				SEQUENCE {
	measQuantityUTRA-FDD				ENUMERATED {cpich-RSCP, cpich-EcN0},
	measQuantityUTRA-TDD				ENUMERATED {pccpch-RSCP},
	filterCoefficient					FilterCoefficient					DEFAULT fc4
}

QuantityConfigGERAN ::=				SEQUENCE {
	measQuantityGERAN					ENUMERATED {rssi},
	filterCoefficient					FilterCoefficient					DEFAULT fc2
}

QuantityConfigCDMA2000 ::=			SEQUENCE {
	measQuantityCDMA2000				ENUMERATED {pilotStrength, pilotPnPhaseAndPilotStrength}
}


ReportConfigEUTRA ::=				SEQUENCE {
	triggerType							CHOICE {
		event								SEQUENCE {
			eventId								CHOICE {
				eventA1								SEQUENCE {
					a1-Threshold						ThresholdEUTRA
				},
				eventA2								SEQUENCE {
					a2-Threshold						ThresholdEUTRA
				},
				eventA3								SEQUENCE {
					a3-Offset							INTEGER (-30..30),
					reportOnLeave						BOOLEAN
				},
				eventA4								SEQUENCE {
					a4-Threshold						ThresholdEUTRA
				},
				eventA5								SEQUENCE {
					a5-Threshold1						ThresholdEUTRA,
					a5-Threshold2						ThresholdEUTRA
				},
				...
			},
			hysteresis							Hysteresis,
			timeToTrigger						TimeToTrigger
		},
		periodical								SEQUENCE {
			purpose									ENUMERATED {
														reportStrongestCells, reportCGI}
		}
	},
	triggerQuantity						ENUMERATED {rsrp, rsrq},
	reportQuantity						ENUMERATED {sameAsTriggerQuantity, both},
	maxReportCells						INTEGER (1..maxCellReport),
	reportInterval						ReportInterval,
	reportAmount						ENUMERATED {r1, r2, r4, r8, r16, r32, r64, infinity},
	...,
	[[	si-RequestForHO-r9					ENUMERATED {setup}		OPTIONAL,	-- Cond reportCGI
		ue-RxTxTimeDiffPeriodical-r9		ENUMERATED {setup}		OPTIONAL	-- Need OR
	]]
}

ThresholdEUTRA ::=					CHOICE{
	threshold-RSRP						RSRP-Range,
	threshold-RSRQ						RSRQ-Range
}


ReportConfigId ::=					INTEGER (1..maxReportConfigId)


ReportConfigInterRAT ::=			SEQUENCE {
	triggerType							CHOICE {
		event								SEQUENCE {
			eventId								CHOICE {
				eventB1								SEQUENCE {
					b1-Threshold						CHOICE {
						b1-ThresholdUTRA					ThresholdUTRA,
						b1-ThresholdGERAN					ThresholdGERAN,
						b1-ThresholdCDMA2000				ThresholdCDMA2000
					}
				},
				eventB2								SEQUENCE {
					b2-Threshold1						ThresholdEUTRA,
					b2-Threshold2						CHOICE {
						b2-Threshold2UTRA					ThresholdUTRA,
						b2-Threshold2GERAN					ThresholdGERAN,
						b2-Threshold2CDMA2000				ThresholdCDMA2000
					}
				},
				...
			},
			hysteresis						Hysteresis,
			timeToTrigger					TimeToTrigger
		},
		periodical								SEQUENCE {
			purpose									ENUMERATED {
														reportStrongestCells,
														reportStrongestCellsForSON,
														reportCGI}
		}
	},
	maxReportCells						INTEGER (1..maxCellReport),
	reportInterval						ReportInterval,
	reportAmount						ENUMERATED {r1, r2, r4, r8, r16, r32, r64, infinity},
	...,
	[[	si-RequestForHO-r9					ENUMERATED {setup}		OPTIONAL	-- Cond reportCGI
	]]
}

ThresholdUTRA ::=					CHOICE{
	utra-RSCP							INTEGER (-5..91),
	utra-EcN0							INTEGER (0..49)
}

ThresholdGERAN ::= 				INTEGER (0..63)

ThresholdCDMA2000 ::= 			INTEGER (0..63)


ReportConfigToAddModList ::=		SEQUENCE (SIZE (1..maxReportConfigId)) OF ReportConfigToAddMod

ReportConfigToAddMod ::=	SEQUENCE {
	reportConfigId						ReportConfigId,
	reportConfig						CHOICE {
		reportConfigEUTRA					ReportConfigEUTRA,
		reportConfigInterRAT				ReportConfigInterRAT
	}
}



ReportInterval ::=					ENUMERATED {
										ms120, ms240, ms480, ms640, ms1024, ms2048, ms5120, ms10240,
										min1, min6, min12, min30, min60, spare3, spare2, spare1}


RSRP-Range ::=						INTEGER(0..97)


RSRQ-Range ::=						INTEGER(0..34)


TimeToTrigger ::=					ENUMERATED {
										ms0, ms40, ms64, ms80, ms100, ms128, ms160, ms256,
										ms320, ms480, ms512, ms640, ms1024, ms1280, ms2560,
										ms5120}


C-RNTI ::=							BIT STRING (SIZE (16))


DedicatedInfoCDMA2000 ::=				OCTET STRING


DedicatedInfoNAS ::=		OCTET STRING


FilterCoefficient ::=					ENUMERATED {
											fc0, fc1, fc2, fc3, fc4, fc5,
											fc6, fc7, fc8, fc9, fc11, fc13,
											fc15, fc17, fc19, spare1, ...}


MMEC ::=							BIT STRING (SIZE (8))


NeighCellConfig ::=			BIT STRING (SIZE (2))


OtherConfig-r9 ::= SEQUENCE	{
	reportProximityConfig-r9			ReportProximityConfig-r9		OPTIONAL,	-- Need ON
	...
}

ReportProximityConfig-r9 ::= SEQUENCE {
	proximityIndicationEUTRA-r9		ENUMERATED {enabled}			OPTIONAL, 		-- Need OR
	proximityIndicationUTRA-r9		ENUMERATED {enabled}			OPTIONAL		-- Need OR
}


RAND-CDMA2000 ::=						BIT STRING (SIZE (32))


RAT-Type ::=						ENUMERATED {
										eutra, utra, geran-cs, geran-ps, cdma2000-1XRTT,
										spare3, spare2, spare1, ...}


RRC-TransactionIdentifier ::=		INTEGER (0..3)


S-TMSI ::=							SEQUENCE {
	mmec								MMEC,
	m-TMSI								BIT STRING (SIZE (32))
}


UE-CapabilityRAT-ContainerList ::=SEQUENCE (SIZE (0..maxRAT-Capabilities)) OF UE-CapabilityRAT-Container

UE-CapabilityRAT-Container ::= SEQUENCE {
	rat-Type							RAT-Type,
	ueCapabilityRAT-Container			OCTET STRING
}


UE-EUTRA-Capability ::=			SEQUENCE {
	accessStratumRelease				AccessStratumRelease,
	ue-Category							INTEGER (1..5),
	pdcp-Parameters						PDCP-Parameters,
	phyLayerParameters					PhyLayerParameters,
	rf-Parameters						RF-Parameters,
	measParameters						MeasParameters,
	featureGroupIndicators				BIT STRING (SIZE (32))				OPTIONAL,
	interRAT-Parameters				SEQUENCE {
		utraFDD								IRAT-ParametersUTRA-FDD				OPTIONAL,
		utraTDD128							IRAT-ParametersUTRA-TDD128				OPTIONAL,
		utraTDD384							IRAT-ParametersUTRA-TDD384				OPTIONAL,
		utraTDD768							IRAT-ParametersUTRA-TDD768				OPTIONAL,
		geran								IRAT-ParametersGERAN					OPTIONAL,
		cdma2000-HRPD						IRAT-ParametersCDMA2000-HRPD			OPTIONAL,
		cdma2000-1xRTT						IRAT-ParametersCDMA2000-1XRTT			OPTIONAL
	},
	nonCriticalExtension				UE-EUTRA-Capability-v920-IEs		OPTIONAL
}

UE-EUTRA-Capability-v920-IEs ::=		SEQUENCE {
	phyLayerParameters-v920				PhyLayerParameters-v920,
	interRAT-ParametersGERAN-v920			IRAT-ParametersGERAN-v920,
	interRAT-ParametersUTRA-v920			IRAT-ParametersUTRA-v920			OPTIONAL,
	interRAT-ParametersCDMA2000-v920		IRAT-ParametersCDMA2000-1XRTT-v920	OPTIONAL,
	deviceType-r9							ENUMERATED {noBenFromBatConsumpOpt}	OPTIONAL,
	csg-ProximityIndicationParameters-r9	CSG-ProximityIndicationParameters-r9,
	neighCellSI-AcquisitionParameters-r9	NeighCellSI-AcquisitionParameters-r9,
	son-Parameters-r9						SON-Parameters-r9,
	nonCriticalExtension					UE-EUTRA-Capability-v940-IEs		OPTIONAL
}

UE-EUTRA-Capability-v940-IEs ::=	SEQUENCE {
	lateNonCriticalExtension			OCTET STRING (CONTAINING UE-EUTRA-Capability-v9a0-IEs)
																			OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

UE-EUTRA-Capability-v9a0-IEs ::=	SEQUENCE {
	featureGroupIndRel9Add-r9			BIT STRING (SIZE (32))				OPTIONAL,
	fdd-Add-UE-EUTRA-Capabilities-r9	UE-EUTRA-CapabilityAddXDD-Mode-r9	OPTIONAL,
	tdd-Add-UE-EUTRA-Capabilities-r9	UE-EUTRA-CapabilityAddXDD-Mode-r9	OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v9c0-IEs		OPTIONAL
}

UE-EUTRA-Capability-v9c0-IEs ::=		SEQUENCE {
	interRAT-ParametersUTRA-v9c0		IRAT-ParametersUTRA-v9c0		OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v9d0-IEs	OPTIONAL
}

UE-EUTRA-Capability-v9d0-IEs ::=		SEQUENCE {
	phyLayerParameters-v9d0				PhyLayerParameters-v9d0			OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v9e0-IEs	OPTIONAL
}

UE-EUTRA-Capability-v9e0-IEs ::=	SEQUENCE {
	rf-Parameters-v9e0					RF-Parameters-v9e0					OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v9h0-IEs		OPTIONAL
}

UE-EUTRA-Capability-v9h0-IEs ::=	SEQUENCE {
	interRAT-ParametersUTRA-v9h0		IRAT-ParametersUTRA-v9h0			OPTIONAL,
	-- Following field is only to be used for late REL-9 extensions
	lateNonCriticalExtension			OCTET STRING							OPTIONAL,
	-- Following field is only to be used for late extensions from REL-10
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

UE-EUTRA-CapabilityAddXDD-Mode-r9 ::=	SEQUENCE {
	phyLayerParameters-r9				PhyLayerParameters					OPTIONAL,
	featureGroupIndicators-r9			BIT STRING (SIZE (32))				OPTIONAL,
	featureGroupIndRel9Add-r9			BIT STRING (SIZE (32))				OPTIONAL,
	interRAT-ParametersGERAN-r9			IRAT-ParametersGERAN				OPTIONAL,
	interRAT-ParametersUTRA-r9			IRAT-ParametersUTRA-v920			OPTIONAL,
	interRAT-ParametersCDMA2000-r9		IRAT-ParametersCDMA2000-1XRTT-v920	OPTIONAL,
	neighCellSI-AcquisitionParameters-r9	NeighCellSI-AcquisitionParameters-r9	OPTIONAL,
	...
}

AccessStratumRelease ::=			ENUMERATED {
										rel8, rel9, spare6, spare5, spare4, spare3,
										spare2, spare1, ...}

PDCP-Parameters ::=				SEQUENCE {
	supportedROHC-Profiles				SEQUENCE {
		profile0x0001						BOOLEAN,
		profile0x0002						BOOLEAN,
		profile0x0003						BOOLEAN,
		profile0x0004						BOOLEAN,
		profile0x0006						BOOLEAN,
		profile0x0101						BOOLEAN,
		profile0x0102						BOOLEAN,
		profile0x0103						BOOLEAN,
		profile0x0104						BOOLEAN
	},
	maxNumberROHC-ContextSessions		ENUMERATED {
											cs2, cs4, cs8, cs12, cs16, cs24, cs32,
											cs48, cs64, cs128, cs256, cs512, cs1024,
											cs16384, spare2, spare1}				DEFAULT cs16,
	...
}

PhyLayerParameters ::=				SEQUENCE {
	ue-TxAntennaSelectionSupported		BOOLEAN,
	ue-SpecificRefSigsSupported		BOOLEAN
}

PhyLayerParameters-v920 ::=		SEQUENCE {
	enhancedDualLayerFDD-r9			ENUMERATED {supported}			OPTIONAL,
	enhancedDualLayerTDD-r9			ENUMERATED {supported}			OPTIONAL
}

PhyLayerParameters-v9d0 ::=			SEQUENCE {
	tm5-FDD-r9						ENUMERATED {supported}			OPTIONAL,
	tm5-TDD-r9						ENUMERATED {supported}			OPTIONAL
}

RF-Parameters ::=					SEQUENCE {
	supportedBandListEUTRA				SupportedBandListEUTRA
}

RF-Parameters-v9e0 ::=					SEQUENCE {
	supportedBandListEUTRA-v9e0				SupportedBandListEUTRA-v9e0				OPTIONAL
}

SupportedBandListEUTRA ::=			SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA

SupportedBandListEUTRA-v9e0::=			SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v9e0

SupportedBandEUTRA ::=				SEQUENCE {
	bandEUTRA							INTEGER (1..64),
	halfDuplex							BOOLEAN
}

SupportedBandEUTRA-v9e0 ::=		SEQUENCE {
	bandEUTRA-v9e0						FreqBandIndicator-v9e0		OPTIONAL
}

MeasParameters ::=					SEQUENCE {
	bandListEUTRA						BandListEUTRA
}

BandListEUTRA ::=					SEQUENCE (SIZE (1..maxBands)) OF BandInfoEUTRA

BandInfoEUTRA ::=					SEQUENCE {
	interFreqBandList					InterFreqBandList,
	interRAT-BandList					InterRAT-BandList		OPTIONAL
}

InterFreqBandList ::=				SEQUENCE (SIZE (1..maxBands)) OF InterFreqBandInfo

InterFreqBandInfo ::=				SEQUENCE {
	interFreqNeedForGaps				BOOLEAN
}

InterRAT-BandList ::=				SEQUENCE (SIZE (1..maxBands)) OF InterRAT-BandInfo

InterRAT-BandInfo ::=				SEQUENCE {
	interRAT-NeedForGaps				BOOLEAN
}

IRAT-ParametersUTRA-FDD ::=		SEQUENCE {
	supportedBandListUTRA-FDD			SupportedBandListUTRA-FDD
}

IRAT-ParametersUTRA-v920 ::=		SEQUENCE {
	e-RedirectionUTRA-r9				ENUMERATED {supported}
}

IRAT-ParametersUTRA-v9c0 ::=		SEQUENCE {
	voiceOverPS-HS-UTRA-FDD-r9						ENUMERATED {supported}		OPTIONAL,
	voiceOverPS-HS-UTRA-TDD128-r9					ENUMERATED {supported}		OPTIONAL,
	srvcc-FromUTRA-FDD-ToUTRA-FDD-r9				ENUMERATED {supported}		OPTIONAL,
	srvcc-FromUTRA-FDD-ToGERAN-r9					ENUMERATED {supported}		OPTIONAL,
	srvcc-FromUTRA-TDD128-ToUTRA-TDD128-r9			ENUMERATED {supported}		OPTIONAL,
	srvcc-FromUTRA-TDD128-ToGERAN-r9				ENUMERATED {supported}		OPTIONAL
}

IRAT-ParametersUTRA-v9h0 ::=		SEQUENCE {
	mfbi-UTRA-r9						ENUMERATED {supported}
}

SupportedBandListUTRA-FDD ::=		SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-FDD

SupportedBandUTRA-FDD ::=			ENUMERATED {
										bandI, bandII, bandIII, bandIV, bandV, bandVI,
										bandVII, bandVIII, bandIX, bandX, bandXI,
										bandXII, bandXIII, bandXIV, bandXV, bandXVI, ...,
										bandXVII-8a0, bandXVIII-8a0, bandXIX-8a0, bandXX-8a0,
										bandXXI-8a0, bandXXII-8a0, bandXXIII-8a0, bandXXIV-8a0,
										bandXXV-8a0, bandXXVI-8a0, bandXXVII-8a0, bandXXVIII-8a0,
										bandXXIX-8a0, bandXXX-8a0, bandXXXI-8a0, bandXXXII-8a0}

IRAT-ParametersUTRA-TDD128 ::=		SEQUENCE {
	supportedBandListUTRA-TDD128		SupportedBandListUTRA-TDD128
}

SupportedBandListUTRA-TDD128 ::=	SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-TDD128

SupportedBandUTRA-TDD128 ::=		ENUMERATED {
										a, b, c, d, e, f, g, h, i, j, k, l, m, n,
										o, p, ...}

IRAT-ParametersUTRA-TDD384 ::=		SEQUENCE {
	supportedBandListUTRA-TDD384		SupportedBandListUTRA-TDD384
}

SupportedBandListUTRA-TDD384 ::=	SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-TDD384

SupportedBandUTRA-TDD384 ::=		ENUMERATED {
											a, b, c, d, e, f, g, h, i, j, k, l, m, n,
											o, p, ...}

IRAT-ParametersUTRA-TDD768 ::=		SEQUENCE {
	supportedBandListUTRA-TDD768		SupportedBandListUTRA-TDD768
}

SupportedBandListUTRA-TDD768 ::=	SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-TDD768

SupportedBandUTRA-TDD768 ::=		ENUMERATED {
										a, b, c, d, e, f, g, h, i, j, k, l, m, n,
										o, p, ...}

IRAT-ParametersGERAN ::=			SEQUENCE {
	supportedBandListGERAN				SupportedBandListGERAN,
	interRAT-PS-HO-ToGERAN				BOOLEAN
}

IRAT-ParametersGERAN-v920 ::=		SEQUENCE {
	dtm-r9								ENUMERATED {supported}			OPTIONAL,
	e-RedirectionGERAN-r9				ENUMERATED {supported}			OPTIONAL
}

SupportedBandListGERAN ::=			SEQUENCE (SIZE (1..maxBands)) OF SupportedBandGERAN

SupportedBandGERAN ::=				ENUMERATED {
										gsm450, gsm480, gsm710, gsm750, gsm810, gsm850,
										gsm900P, gsm900E, gsm900R, gsm1800, gsm1900,
										spare5, spare4, spare3, spare2, spare1, ...}

IRAT-ParametersCDMA2000-HRPD ::=	SEQUENCE {
	supportedBandListHRPD				SupportedBandListHRPD,
	tx-ConfigHRPD						ENUMERATED {single, dual},
	rx-ConfigHRPD						ENUMERATED {single, dual}
}

SupportedBandListHRPD ::=			SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandclassCDMA2000

IRAT-ParametersCDMA2000-1XRTT ::=	SEQUENCE {
	supportedBandList1XRTT				SupportedBandList1XRTT,
	tx-Config1XRTT						ENUMERATED {single, dual},
	rx-Config1XRTT						ENUMERATED {single, dual}
}

IRAT-ParametersCDMA2000-1XRTT-v920 ::=	SEQUENCE {
	e-CSFB-1XRTT-r9						ENUMERATED {supported},
	e-CSFB-ConcPS-Mob1XRTT-r9			ENUMERATED {supported}			OPTIONAL
}

SupportedBandList1XRTT ::=			SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandclassCDMA2000

CSG-ProximityIndicationParameters-r9 ::=	SEQUENCE {
	intraFreqProximityIndication-r9	ENUMERATED {supported}			OPTIONAL,
	interFreqProximityIndication-r9	ENUMERATED {supported}			OPTIONAL,
	utran-ProximityIndication-r9		ENUMERATED {supported}			OPTIONAL
}

NeighCellSI-AcquisitionParameters-r9 ::=	SEQUENCE {
	intraFreqSI-AcquisitionForHO-r9	ENUMERATED {supported}			OPTIONAL,
	interFreqSI-AcquisitionForHO-r9	ENUMERATED {supported}			OPTIONAL,
	utran-SI-AcquisitionForHO-r9		ENUMERATED {supported}			OPTIONAL
}

SON-Parameters-r9 ::=				SEQUENCE {
	rach-Report-r9						ENUMERATED {supported}			OPTIONAL
}


UE-TimersAndConstants ::=			SEQUENCE {
	t300								ENUMERATED {
											ms100, ms200, ms300, ms400, ms600, ms1000, ms1500,
											ms2000},
	t301								ENUMERATED {
											ms100, ms200, ms300, ms400, ms600, ms1000, ms1500,
											ms2000},
	t310								ENUMERATED {
											ms0, ms50, ms100, ms200, ms500, ms1000, ms2000},
	n310								ENUMERATED {
											n1, n2, n3, n4, n6, n8, n10, n20},
	t311								ENUMERATED {
											ms1000, ms3000, ms5000, ms10000, ms15000,
											ms20000, ms30000},
	n311								ENUMERATED {
											n1, n2, n3, n4, n5, n6, n8, n10},
	...
}


MBMS-NotificationConfig-r9 ::=				SEQUENCE {
	notificationRepetitionCoeff-r9		ENUMERATED {n2, n4},
	notificationOffset-r9				INTEGER (0..10),
	notificationSF-Index-r9				INTEGER (1..6)
}


MBSFN-AreaInfoList-r9 ::=			SEQUENCE (SIZE(1..maxMBSFN-Area)) OF MBSFN-AreaInfo-r9

MBSFN-AreaInfo-r9 ::=				SEQUENCE {
	mbsfn-AreaId-r9						INTEGER (0..255),
	non-MBSFNregionLength				ENUMERATED {s1, s2},
	notificationIndicator-r9				INTEGER (0..7),
	mcch-Config-r9						SEQUENCE {
		mcch-RepetitionPeriod-r9			ENUMERATED {rf32, rf64, rf128, rf256},
		mcch-Offset-r9						INTEGER (0..10),
		mcch-ModificationPeriod-r9			ENUMERATED {rf512, rf1024},
		sf-AllocInfo-r9						BIT STRING (SIZE(6)),
		signallingMCS-r9					ENUMERATED {n2, n7, n13, n19}
	},
	...
}


MBSFN-SubframeConfig ::=			SEQUENCE {
	radioframeAllocationPeriod			ENUMERATED {n1, n2, n4, n8, n16, n32},
	radioframeAllocationOffset			INTEGER (0..7),
	subframeAllocation					CHOICE {
		oneFrame							BIT STRING (SIZE(6)),
		fourFrames							BIT STRING (SIZE(24))
	}
}

PMCH-InfoList-r9 ::=				SEQUENCE (SIZE (0..maxPMCH-PerMBSFN)) OF PMCH-Info-r9

PMCH-Info-r9 ::=					SEQUENCE {
	pmch-Config-r9						PMCH-Config-r9,
	mbms-SessionInfoList-r9			MBMS-SessionInfoList-r9,
	...
}

MBMS-SessionInfoList-r9 ::=		SEQUENCE (SIZE (0..maxSessionPerPMCH)) OF MBMS-SessionInfo-r9

MBMS-SessionInfo-r9 ::=			SEQUENCE {
	tmgi-r9								TMGI-r9,
	sessionId-r9						OCTET STRING (SIZE (1)) 		OPTIONAL, 	-- Need OR
	logicalChannelIdentity-r9			INTEGER (0..maxSessionPerPMCH-1),
	...
}

PMCH-Config-r9 ::=					SEQUENCE {
	sf-AllocEnd-r9						INTEGER (0..1535),
	dataMCS-r9							INTEGER (0..28),
	mch-SchedulingPeriod-r9			ENUMERATED {
										rf8, rf16, rf32, rf64, rf128, rf256, rf512, rf1024},
	...
}

TMGI-r9 ::=						SEQUENCE {
	plmn-Id-r9							CHOICE {
		plmn-Index-r9						INTEGER (1..6),
		explicitValue-r9					PLMN-Identity
	},
	serviceId-r9						OCTET STRING (SIZE (3))
}


maxBands					INTEGER ::= 64	-- Maximum number of bands listed in EUTRA UE caps
maxCDMA-BandClass			INTEGER ::= 32	-- Maximum value of the CDMA band classes
maxCellBlack				INTEGER ::= 16	-- Maximum number of blacklisted cells
											--	listed in SIB type 4 and 5
maxCellInfoGERAN-r9 		INTEGER ::=	32	-- Maximum number of GERAN cells for which system in-
											-- formation can be provided as redirection assistance
maxCellInfoUTRA-r9			INTEGER ::=	16	-- Maximum number of UTRA cells for which system
											-- information can be provided as redirection
											-- assistance
maxCellInter				INTEGER ::= 16	-- Maximum number of neighbouring inter-frequency
											-- cells listed in SIB type 5
maxCellIntra				INTEGER ::= 16	-- Maximum number of neighbouring intra-frequency
											-- cells listed in SIB type 4
maxCellMeas					INTEGER ::= 32	-- Maximum number of entries in each of the
											-- cell lists in a measurement object
maxCellReport				INTEGER ::= 8	-- Maximum number of reported cells
maxDRB						INTEGER ::= 11	-- Maximum number of Data Radio Bearers
maxEARFCN					INTEGER ::= 65535	-- Maximum value of EUTRA carrier frequency
maxEARFCN-Plus1				INTEGER ::= 65536	-- Lowest value extended EARFCN range
maxEARFCN2					INTEGER ::= 262143	-- Highest value extended EARFCN range
maxFBI						INTEGER ::= 64	-- Maximum value of fequency band indicator
maxFBI-Plus1				INTEGER ::= 65	-- Lowest value extended FBI range
maxFBI2						INTEGER ::= 256	-- Highest value extended FBI range
maxFreq						INTEGER ::= 8	-- Maximum number of EUTRA carrier frequencies
maxGERAN-SI					INTEGER ::= 10	-- Maximum number of GERAN SI blocks that can be
											-- provided as part of NACC information
maxGNFG						INTEGER ::= 16	-- Maximum number of GERAN neighbour freq groups
maxMBSFN-Allocations		INTEGER ::= 8	-- Maximum number of MBSFN frame allocations with
											-- different offset
maxMBSFN-Area				INTEGER ::= 8
maxMeasId					INTEGER ::= 32
maxMultiBands				INTEGER ::= 8	-- Maximum number of additional frequency bands
											-- that a cell belongs to
maxObjectId					INTEGER ::= 32
maxPageRec					INTEGER ::= 16	--
maxPhysCellIdRange-r9 		INTEGER ::= 4	-- Maximum number of physical cell identity ranges
maxPNOffset					INTEGER ::=	511	-- Maximum number of CDMA2000 PNOffsets
maxPMCH-PerMBSFN			INTEGER ::= 15
maxRAT-Capabilities			INTEGER ::= 8	-- Maximum number of interworking RATs (incl EUTRA)
maxReportConfigId			INTEGER ::= 32
maxSessionPerPMCH			INTEGER ::= 29
maxSessionPerPMCH-1			INTEGER ::= 28
maxSIB						INTEGER ::= 32	-- Maximum number of SIBs
maxSIB-1					INTEGER ::= 31
maxSI-Message				INTEGER ::= 32	-- Maximum number of SI messages
maxUTRA-FDD-Carrier			INTEGER ::= 16	-- Maximum number of UTRA FDD carrier frequencies
maxUTRA-TDD-Carrier			INTEGER ::= 16	-- Maximum number of UTRA TDD carrier frequencies


END


EUTRA-UE-Variables DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS
	CarrierFreqGERAN,
	CellIdentity,
	SpeedStateScaleFactors,
	C-RNTI,
	MeasId,
	MeasIdToAddModList,
	MeasObjectToAddModList,
	MeasObjectToAddModList-v9e0,
	MobilityStateParameters,
	NeighCellConfig,
	PhysCellId,
	PhysCellIdCDMA2000,
	PhysCellIdGERAN,
	PhysCellIdUTRA-FDD,
	PhysCellIdUTRA-TDD,
	QuantityConfig,
	ReportConfigToAddModList,
	RSRP-Range,
	maxCellMeas,
	maxMeasId
FROM EUTRA-RRC-Definitions;


VarMeasConfig ::=					SEQUENCE {
	-- Measurement identities
	measIdList							MeasIdToAddModList					OPTIONAL,
	-- Measurement objects
	measObjectList						MeasObjectToAddModList				OPTIONAL,
	measObjectList-v9i0					MeasObjectToAddModList-v9e0			OPTIONAL,
	-- Reporting configurations
	reportConfigList					ReportConfigToAddModList			OPTIONAL,
	-- Other parameters
	quantityConfig						QuantityConfig						OPTIONAL,
	s-Measure							RSRP-Range							OPTIONAL,
	speedStatePars						CHOICE {
		release								NULL,
		setup								SEQUENCE {
			mobilityStateParameters				MobilityStateParameters,
			timeToTrigger-SF					SpeedStateScaleFactors
		}
	}																		OPTIONAL
}


VarMeasReportList ::=				SEQUENCE (SIZE (1..maxMeasId)) OF VarMeasReport

VarMeasReport ::=					SEQUENCE {
	-- List of measurement that have been triggered
	measId								MeasId,
	cellsTriggeredList					CellsTriggeredList				OPTIONAL,
	numberOfReportsSent					INTEGER
}

CellsTriggeredList ::=				SEQUENCE (SIZE (1..maxCellMeas)) OF CHOICE {
	physCellIdEUTRA							PhysCellId,
	physCellIdUTRA							CHOICE {
		fdd										PhysCellIdUTRA-FDD,
		tdd										PhysCellIdUTRA-TDD
	},
	physCellIdGERAN							SEQUENCE {
		carrierFreq								CarrierFreqGERAN,
		physCellId								PhysCellIdGERAN
	},
	physCellIdCDMA2000						PhysCellIdCDMA2000
}

VarShortMAC-Input ::=					SEQUENCE {
	cellIdentity							CellIdentity,
	physCellId								PhysCellId,
	c-RNTI									C-RNTI
}



END


EUTRA-InterNodeDefinitions DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS
	AntennaInfoCommon,
	CellIdentity,
	C-RNTI,
	DL-DCCH-Message,
	ARFCN-ValueEUTRA,
	ARFCN-ValueEUTRA-v9e0,
	MasterInformationBlock,
	MeasConfig,
	OtherConfig-r9,
	PhysCellId,
	RadioResourceConfigDedicated,
	SecurityAlgorithmConfig,
	ShortMAC-I,
	SystemInformationBlockType1,
	SystemInformationBlockType1-v890-IEs,
	SystemInformationBlockType2,
	UECapabilityInformation,
	UE-CapabilityRAT-ContainerList
FROM EUTRA-RRC-Definitions;


HandoverCommand ::=					SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			handoverCommand-r8					HandoverCommand-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

HandoverCommand-r8-IEs ::=			SEQUENCE {
	handoverCommandMessage				OCTET STRING (CONTAINING DL-DCCH-Message),
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


HandoverPreparationInformation ::=	SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			handoverPreparationInformation-r8	HandoverPreparationInformation-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

HandoverPreparationInformation-r8-IEs ::= SEQUENCE {
	ue-RadioAccessCapabilityInfo		UE-CapabilityRAT-ContainerList,
	as-Config							AS-Config					OPTIONAL, 		-- Cond HO
	rrm-Config							RRM-Config					OPTIONAL,
	as-Context							AS-Context				OPTIONAL, 		-- Cond HO
	nonCriticalExtension				HandoverPreparationInformation-v920-IEs		OPTIONAL
}

HandoverPreparationInformation-v920-IEs	::= SEQUENCE {
	ue-ConfigRelease-r9					ENUMERATED {
										rel9, spare7, spare6, spare5, spare4, spare3,
										spare2, spare1, ...} 			OPTIONAL, 	-- Cond HO2
	nonCriticalExtension				HandoverPreparationInformation-v9d0-IEs		OPTIONAL
}

HandoverPreparationInformation-v9d0-IEs	::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING								OPTIONAL,
	nonCriticalExtension				HandoverPreparationInformation-v9e0-IEs		OPTIONAL
}

HandoverPreparationInformation-v9e0-IEs	::= SEQUENCE {
	as-Config-v9e0						AS-Config-v9e0					OPTIONAL,	-- Cond HO2
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}


UERadioAccessCapabilityInformation ::= SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			ueRadioAccessCapabilityInformation-r8
												UERadioAccessCapabilityInformation-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UERadioAccessCapabilityInformation-r8-IEs ::= SEQUENCE {
	ue-RadioAccessCapabilityInfo		OCTET STRING (CONTAINING UECapabilityInformation),
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


AS-Config ::=				SEQUENCE {
	sourceMeasConfig					MeasConfig,
	sourceRadioResourceConfig			RadioResourceConfigDedicated,
	sourceSecurityAlgorithmConfig		SecurityAlgorithmConfig,
	sourceUE-Identity					C-RNTI,
	sourceMasterInformationBlock		MasterInformationBlock,
	sourceSystemInformationBlockType1	SystemInformationBlockType1(WITH COMPONENTS
											{..., nonCriticalExtension ABSENT}),
	sourceSystemInformationBlockType2	SystemInformationBlockType2,
	antennaInfoCommon					AntennaInfoCommon,
	sourceDl-CarrierFreq				ARFCN-ValueEUTRA,
	...,
	[[	sourceSystemInformationBlockType1Ext	OCTET STRING (CONTAINING
												SystemInformationBlockType1-v890-IEs)	OPTIONAL,
		sourceOtherConfig-r9				OtherConfig-r9
	]]
}

AS-Config-v9e0 ::=				SEQUENCE {
	sourceDl-CarrierFreq-v9e0		ARFCN-ValueEUTRA-v9e0
}


AS-Context ::=							SEQUENCE {
	reestablishmentInfo						ReestablishmentInfo			OPTIONAL	-- Cond HO
}


ReestablishmentInfo ::=				SEQUENCE {
	sourcePhysCellId					PhysCellId,
	targetCellShortMAC-I				ShortMAC-I,
	additionalReestabInfoList			AdditionalReestabInfoList				OPTIONAL,
	...
}

AdditionalReestabInfoList ::=		SEQUENCE ( SIZE (1..maxReestabInfo) ) OF AdditionalReestabInfo

AdditionalReestabInfo ::=	SEQUENCE{
	cellIdentity						CellIdentity,
	key-eNodeB-Star					Key-eNodeB-Star,
	shortMAC-I							ShortMAC-I
}

Key-eNodeB-Star ::=					BIT STRING (SIZE (256))


RRM-Config ::=				SEQUENCE {
	ue-InactiveTime				ENUMERATED {
									s1, s2, s3, s5, s7, s10, s15, s20,
									s25, s30, s40, s50, min1, min1s20c, min1s40,
									min2, min2s30, min3, min3s30, min4, min5, min6,
									min7, min8, min9, min10, min12, min14, min17, min20,
									min24, min28, min33, min38, min44, min50, hr1,
									hr1min30, hr2, hr2min30, hr3, hr3min30, hr4, hr5, hr6,
									hr8, hr10, hr13, hr16, hr20, day1, day1hr12, day2,
									day2hr12, day3, day4, day5, day7, day10, day14, day19,
									day24, day30, dayMoreThan30}		OPTIONAL,
	...
}


maxReestabInfo				INTEGER ::= 32	-- Maximum number of KeNB* and shortMAC-I forwarded
											-- at handover for re-establishment preparation


END


