<table style="border-collapse: collapse; border: none;">
  <tr style="border-collapse: collapse; border: none;">
    <td style="border-collapse: collapse; border: none;">
      <a href="http://www.openairinterface.org/">
         <img src="./images/oai_final_logo.png" alt="" border=3 height=50 width=150>
         </img>
      </a>
    </td>
    <td style="border-collapse: collapse; border: none; vertical-align: center;">
      <b><font size = "5">OAI 5G NR SA tutorial: setting up OAI CN5G</font></b>
    </td>
  </tr>
</table>

**Table of Contents**

[[_TOC_]]

#  1. Scenario
In this tutorial we describe how to configure and run a 5G end-to-end setup with OAI CN5G, OAI gNB and COTS UE.

Minimum hardware requirements:
- Laptop/Desktop/Server for OAI CN5G and OAI gNB
    - Operating System: [Ubuntu 22.04 LTS](https://releases.ubuntu.com/22.04/ubuntu-22.04.2-desktop-amd64.iso)
    - CPU: 8 cores x86_64 @ 3.5 GHz
    - RAM: 32 GB

# 2. OAI CN5G

## 2.1 OAI CN5G pre-requisites

```bash
sudo apt install -y git net-tools putty

sudo apt install -y apt-transport-https ca-certificates curl software-properties-common
curl -fsSL https://download.docker.com/linux/ubuntu/gpg | sudo apt-key add -
sudo add-apt-repository "deb [arch=amd64] https://download.docker.com/linux/ubuntu  $(lsb_release -cs)  stable"
sudo apt update
sudo apt install -y docker docker-ce

# Add your username to the docker group, otherwise you will have to run in sudo mode.
sudo usermod -a -G docker $(whoami)
reboot
```

## 2.2 OAI CN5G configuration files
Download and copy configuration files:
```bash
wget -O ~/oai-cn5g.zip https://gitlab.eurecom.fr/oai/openairinterface5g/-/archive/develop/openairinterface5g-develop.zip?path=doc/tutorial_resources/oai-cn5g
unzip ~/oai-cn5g.zip
mv ~/openairinterface5g-develop-doc-tutorial_resources-oai-cn5g/doc/tutorial_resources/oai-cn5g ~/oai-cn5g
rm -r ~/openairinterface5g-develop-doc-tutorial_resources-oai-cn5g ~/oai-cn5g.zip
```

## 2.3 Pull OAI CN5G docker images

```bash
docker pull mysql:8.0
docker pull oaisoftwarealliance/oai-amf:develop
docker pull oaisoftwarealliance/oai-nrf:develop
docker pull oaisoftwarealliance/oai-smf:develop
docker pull oaisoftwarealliance/oai-udr:develop
docker pull oaisoftwarealliance/oai-udm:develop
docker pull oaisoftwarealliance/oai-ausf:develop
docker pull oaisoftwarealliance/oai-spgwu-tiny:develop
docker pull oaisoftwarealliance/trf-gen-cn5g:latest
docker build --target ims --tag asterisk-ims:latest --file ~/oai-cn5g/Dockerfile .
```

# 3. Run OAI CN5G
## 3.1 Start OAI CN5G
```bash
cd ~/oai-cn5g
docker compose up -d
```

## 3.2 Stop OAI CN5G
```bash
cd ~/oai-cn5g
docker compose down
```

# 4. Run 5G NR SA end-to-end setup with OAI gNB
## 4.1 Testing with COTS UE
Please check this link:
[Testing with OAI gNB and COTS UE](NR_SA_Tutorial_COTS_UE.md)

## 4.2 Testing with OAI nrUE
Please check this link:
[Testing with OAI gNB and OAI nrUE](NR_SA_Tutorial_OAI_nrUE.md)